Plug-in Reference — Messages — EE_SERIAL_TO_LOGICAL

# EE_SERIAL_TO_LOGICAL

Converts the serial position to the logical coordinates. The serial position is the zero-based index of the character from the beginning of the entire text. You can send this message explicitly or use the Editor_SerialToLogical inline function.

    EE_SERIAL_TO_LOGICAL
    wParam = (WPARAM) (UINT) nSerial;
    lParam = (LPARAM) (POINT_PTR*) pptLogical;

## Parameters

nSerial

Specifies a serial position to be converted.

pptLogical

Pointer to a POINT_PTR structure that will receive the converted logical coordinates.

## Return Values

The return value is not used.