Plug-in Reference — Messages — EE_ENUM_CONFIG

# EE_ENUM_CONFIG

Enumerates available configurations. You can send this message explicitly or use the Editor_EnumConfig inline function.

    EE_ENUM_CONFIG
    wParam = (WPARAM) (size_t) cchBuf;
    lParam = (LPARAM) (LPWSTR) pBuf;

## Parameters

cchBuf

Specifies the size of the buffer in characters. Note that two null characters will be added at the end of the list of configurations. If 0 is specified, this message returns the size necessary to retrieve the list of configurations.

pBuf

Specifies the pointer to the buffer to retrieve the list of configurations. In this buffer, the list of available configurations each separated by a null character will be retrieved. Two null characters will be added at the end of the list of configurations. If 0 is specified, pBuf can be NULL.

## Return Values

The return value is the size necessary to retrieve the list of configurations.

## Version

Supported on Version 6.00 or later.