Plug-in Reference — Structures — ACTIVE_STRING_INFO

# ACTIVE_STRING_INFO

Used by EE_GET_ACTIVE_STRING message.

    typedef struct _ACTIVE_STRING_INFO {
    	UINT cbSize;
    	LPWSTR pBuf;
    	UINT cchBuf;
    	UINT nFlags;
    } ACTIVE_STRING_INFO;

## Members

cbSize

Size of this data structure, in bytes. Set this member to sizeof( ACTIVE_STRING_INFO ) before sending the EE_GET_ACTIVE_STRING message.

pBuf

Specifies the buffer to receive the active string.

cchBuf

Specifies the size of the buffer in characters.

nFlags

Currently not used.

## Version

Supported on Version 16.9 or later.