---
name: Bug report
about: Create a report to help us improve
title: ''
labels: ''
assignees: ''

---

**IMPORTANT: Check the wiki**
Before submitting new issue, please check the [Wiki](https://github.com/jgromes/RadioLib/wiki) and the [API documentation](https://jgromes.github.io/RadioLib/). You might find a solution to your issue there. 

**Describe the bug**
A clear and concise description of what the bug is. When applicable, please include [debug mode output](https://github.com/jgromes/RadioLib/wiki/Debug-mode).

**To Reproduce**
Minimal Arduino sketch to reproduce the behavior. Please user Markdown to style the code to make it readable (see [Markdown Cheatsheet](https://github.com/adam-p/markdown-here/wiki/Markdown-Cheatsheet#code)).

**Expected behavior**
A clear and concise description of what you expected to happen.

**Screenshots**
If applicable, add screenshots to help explain your problem.

**Additional info (please complete):**
 - MCU: [e.g. Arduino Uno, ESP8266 etc.]
 - Link to Arduino core: [e.g. https://github.com/stm32duino/Arduino_Core_STM32 when using official STM32 core. See readme for links to all supported cores]
 - Wireless module type [e.g. CC1101, SX1268, etc.]
 - Arduino IDE version  [e.g. 1.8.5]
 - Library version [e.g. 3.0.0]
