#### First plug your wristband to USB, then you can connect.
Please select port with name NUCLEO.

##### Device is new, has never been configured yet

##### Data sent successfully to your wristband. Device will reboot now.
You can safely unplug the device.

Your callsign with SSID
We prefer -7 SSID for now for your wristband.
Path
Comment
Select predefined icon
Overlay
Symbol
Packet interval
From 60 to 900 seconds
Vibrate during packet sending
Append battery voltage after comment