Storage API
***********

.. toctree::
   :maxdepth: 1

   SPI Flash and Partition APIs <spi_flash>
   SD/SDIO/MMC Driver <sdmmc>
   Non-Volatile Storage <nvs_flash>
   NVS Partition Generation Utility <nvs_partition_gen.rst>
   Virtual Filesystem <vfs>
   FAT Filesystem <fatfs>
   Wear Levelling <wear-levelling>
   SPIFFS Filesystem <spiffs>
   Mass Manufacturing Utility <mass_mfg.rst>


Example code for this API section is provided in :example:`storage` directory of ESP-IDF examples.
