#Diagram of CAN Controller Acceptance Filter (Dual) Configuration

packetdiag can_acceptance_filter_dual {
    node_width = 30
    node_height = 35
    default_fontsize = 15
    colwidth = 32

    0-3: "F1 DB1[0:3]" [color = lightyellow];
    4: "F2\nRTR" [color = lightyellow];
    5-15: "F2 11-bit ID" [color = lightyellow];
    16-19: "F1 DB1[4:7]" [color = lightyellow];
    20: "F1\nRTR" [color = lightyellow];
    21-31: "F1 11-bit ID" [color = lightyellow];

    32-47: "F2 29-bit ID [13:28]" [color = lightblue];
    48-63: "F1 29-bit ID [13:28]" [color = lightblue];

}