# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F378RCTx
GenF3.menu.pnum.GENERIC_F378RCTX=Generic F378RCTx
GenF3.menu.pnum.GENERIC_F378RCTX.upload.maximum_size=262144
GenF3.menu.pnum.GENERIC_F378RCTX.upload.maximum_data_size=32768
GenF3.menu.pnum.GENERIC_F378RCTX.build.board=GENERIC_F378RCTX
GenF3.menu.pnum.GENERIC_F378RCTX.build.product_line=STM32F378xx
GenF3.menu.pnum.GENERIC_F378RCTX.build.variant=STM32F3xx/F378RC(T-Y)
GenF3.menu.pnum.GENERIC_F378RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F3x8.svd

# Generic F378RCYx
GenF3.menu.pnum.GENERIC_F378RCYX=Generic F378RCYx
GenF3.menu.pnum.GENERIC_F378RCYX.upload.maximum_size=262144
GenF3.menu.pnum.GENERIC_F378RCYX.upload.maximum_data_size=32768
GenF3.menu.pnum.GENERIC_F378RCYX.build.board=GENERIC_F378RCYX
GenF3.menu.pnum.GENERIC_F378RCYX.build.product_line=STM32F378xx
GenF3.menu.pnum.GENERIC_F378RCYX.build.variant=STM32F3xx/F378RC(T-Y)
GenF3.menu.pnum.GENERIC_F378RCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F3x8.svd

