# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F078CBTx
GenF0.menu.pnum.GENERIC_F078CBTX=Generic F078CBTx
GenF0.menu.pnum.GENERIC_F078CBTX.upload.maximum_size=131072
GenF0.menu.pnum.GENERIC_F078CBTX.upload.maximum_data_size=16384
GenF0.menu.pnum.GENERIC_F078CBTX.build.board=GENERIC_F078CBTX
GenF0.menu.pnum.GENERIC_F078CBTX.build.product_line=STM32F078xx
GenF0.menu.pnum.GENERIC_F078CBTX.build.variant=STM32F0xx/F078CB(T-U-Y)
GenF0.menu.pnum.GENERIC_F078CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x8.svd

# Generic F078CBUx
GenF0.menu.pnum.GENERIC_F078CBUX=Generic F078CBUx
GenF0.menu.pnum.GENERIC_F078CBUX.upload.maximum_size=131072
GenF0.menu.pnum.GENERIC_F078CBUX.upload.maximum_data_size=16384
GenF0.menu.pnum.GENERIC_F078CBUX.build.board=GENERIC_F078CBUX
GenF0.menu.pnum.GENERIC_F078CBUX.build.product_line=STM32F078xx
GenF0.menu.pnum.GENERIC_F078CBUX.build.variant=STM32F0xx/F078CB(T-U-Y)
GenF0.menu.pnum.GENERIC_F078CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x8.svd

# Generic F078CBYx
GenF0.menu.pnum.GENERIC_F078CBYX=Generic F078CBYx
GenF0.menu.pnum.GENERIC_F078CBYX.upload.maximum_size=131072
GenF0.menu.pnum.GENERIC_F078CBYX.upload.maximum_data_size=16384
GenF0.menu.pnum.GENERIC_F078CBYX.build.board=GENERIC_F078CBYX
GenF0.menu.pnum.GENERIC_F078CBYX.build.product_line=STM32F078xx
GenF0.menu.pnum.GENERIC_F078CBYX.build.variant=STM32F0xx/F078CB(T-U-Y)
GenF0.menu.pnum.GENERIC_F078CBYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x8.svd

