# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L433CBYx
GenL4.menu.pnum.GENERIC_L433CBYX=Generic L433CBYx
GenL4.menu.pnum.GENERIC_L433CBYX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L433CBYX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L433CBYX.build.board=GENERIC_L433CBYX
GenL4.menu.pnum.GENERIC_L433CBYX.build.product_line=STM32L433xx
GenL4.menu.pnum.GENERIC_L433CBYX.build.variant=STM32L4xx/L433C(B-C)Y_L443CC(F-Y)
GenL4.menu.pnum.GENERIC_L433CBYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L433.svd

# Generic L433CCYx
GenL4.menu.pnum.GENERIC_L433CCYX=Generic L433CCYx
GenL4.menu.pnum.GENERIC_L433CCYX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L433CCYX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L433CCYX.build.board=GENERIC_L433CCYX
GenL4.menu.pnum.GENERIC_L433CCYX.build.product_line=STM32L433xx
GenL4.menu.pnum.GENERIC_L433CCYX.build.variant=STM32L4xx/L433C(B-C)Y_L443CC(F-Y)
GenL4.menu.pnum.GENERIC_L433CCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L433.svd

# Generic L443CCFx
GenL4.menu.pnum.GENERIC_L443CCFX=Generic L443CCFx
GenL4.menu.pnum.GENERIC_L443CCFX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L443CCFX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L443CCFX.build.board=GENERIC_L443CCFX
GenL4.menu.pnum.GENERIC_L443CCFX.build.product_line=STM32L443xx
GenL4.menu.pnum.GENERIC_L443CCFX.build.variant=STM32L4xx/L433C(B-C)Y_L443CC(F-Y)
GenL4.menu.pnum.GENERIC_L443CCFX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L443.svd

# Generic L443CCYx
GenL4.menu.pnum.GENERIC_L443CCYX=Generic L443CCYx
GenL4.menu.pnum.GENERIC_L443CCYX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L443CCYX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L443CCYX.build.board=GENERIC_L443CCYX
GenL4.menu.pnum.GENERIC_L443CCYX.build.product_line=STM32L443xx
GenL4.menu.pnum.GENERIC_L443CCYX.build.variant=STM32L4xx/L433C(B-C)Y_L443CC(F-Y)
GenL4.menu.pnum.GENERIC_L443CCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L443.svd

