# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L072KBTx
GenL0.menu.pnum.GENERIC_L072KBTX=Generic L072KBTx
GenL0.menu.pnum.GENERIC_L072KBTX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L072KBTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072KBTX.build.board=GENERIC_L072KBTX
GenL0.menu.pnum.GENERIC_L072KBTX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072KBTX.build.variant=STM32L0xx/L072K(B-Z)T_L082K(B-Z)T
GenL0.menu.pnum.GENERIC_L072KBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072KZTx
GenL0.menu.pnum.GENERIC_L072KZTX=Generic L072KZTx
GenL0.menu.pnum.GENERIC_L072KZTX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L072KZTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072KZTX.build.board=GENERIC_L072KZTX
GenL0.menu.pnum.GENERIC_L072KZTX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072KZTX.build.variant=STM32L0xx/L072K(B-Z)T_L082K(B-Z)T
GenL0.menu.pnum.GENERIC_L072KZTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L082KBTx
GenL0.menu.pnum.GENERIC_L082KBTX=Generic L082KBTx
GenL0.menu.pnum.GENERIC_L082KBTX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L082KBTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L082KBTX.build.board=GENERIC_L082KBTX
GenL0.menu.pnum.GENERIC_L082KBTX.build.product_line=STM32L082xx
GenL0.menu.pnum.GENERIC_L082KBTX.build.variant=STM32L0xx/L072K(B-Z)T_L082K(B-Z)T
GenL0.menu.pnum.GENERIC_L082KBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L082KZTx
GenL0.menu.pnum.GENERIC_L082KZTX=Generic L082KZTx
GenL0.menu.pnum.GENERIC_L082KZTX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L082KZTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L082KZTX.build.board=GENERIC_L082KZTX
GenL0.menu.pnum.GENERIC_L082KZTX.build.product_line=STM32L082xx
GenL0.menu.pnum.GENERIC_L082KZTX.build.variant=STM32L0xx/L072K(B-Z)T_L082K(B-Z)T
GenL0.menu.pnum.GENERIC_L082KZTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

