# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F205VBTx
GenF2.menu.pnum.GENERIC_F205VBTX=Generic F205VBTx
GenF2.menu.pnum.GENERIC_F205VBTX.upload.maximum_size=131072
GenF2.menu.pnum.GENERIC_F205VBTX.upload.maximum_data_size=65536
GenF2.menu.pnum.GENERIC_F205VBTX.build.board=GENERIC_F205VBTX
GenF2.menu.pnum.GENERIC_F205VBTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205VBTX.build.variant=STM32F2xx/F205V(B-C-E-F-G)T_F215V(E-G)T
GenF2.menu.pnum.GENERIC_F205VBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205VCTx
GenF2.menu.pnum.GENERIC_F205VCTX=Generic F205VCTx
GenF2.menu.pnum.GENERIC_F205VCTX.upload.maximum_size=262144
GenF2.menu.pnum.GENERIC_F205VCTX.upload.maximum_data_size=98304
GenF2.menu.pnum.GENERIC_F205VCTX.build.board=GENERIC_F205VCTX
GenF2.menu.pnum.GENERIC_F205VCTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205VCTX.build.variant=STM32F2xx/F205V(B-C-E-F-G)T_F215V(E-G)T
GenF2.menu.pnum.GENERIC_F205VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205VETx
GenF2.menu.pnum.GENERIC_F205VETX=Generic F205VETx
GenF2.menu.pnum.GENERIC_F205VETX.upload.maximum_size=524288
GenF2.menu.pnum.GENERIC_F205VETX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205VETX.build.board=GENERIC_F205VETX
GenF2.menu.pnum.GENERIC_F205VETX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205VETX.build.variant=STM32F2xx/F205V(B-C-E-F-G)T_F215V(E-G)T
GenF2.menu.pnum.GENERIC_F205VETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205VFTx
GenF2.menu.pnum.GENERIC_F205VFTX=Generic F205VFTx
GenF2.menu.pnum.GENERIC_F205VFTX.upload.maximum_size=786432
GenF2.menu.pnum.GENERIC_F205VFTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205VFTX.build.board=GENERIC_F205VFTX
GenF2.menu.pnum.GENERIC_F205VFTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205VFTX.build.variant=STM32F2xx/F205V(B-C-E-F-G)T_F215V(E-G)T
GenF2.menu.pnum.GENERIC_F205VFTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205VGTx
GenF2.menu.pnum.GENERIC_F205VGTX=Generic F205VGTx
GenF2.menu.pnum.GENERIC_F205VGTX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F205VGTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205VGTX.build.board=GENERIC_F205VGTX
GenF2.menu.pnum.GENERIC_F205VGTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205VGTX.build.variant=STM32F2xx/F205V(B-C-E-F-G)T_F215V(E-G)T
GenF2.menu.pnum.GENERIC_F205VGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F215VETx
GenF2.menu.pnum.GENERIC_F215VETX=Generic F215VETx
GenF2.menu.pnum.GENERIC_F215VETX.upload.maximum_size=524288
GenF2.menu.pnum.GENERIC_F215VETX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F215VETX.build.board=GENERIC_F215VETX
GenF2.menu.pnum.GENERIC_F215VETX.build.product_line=STM32F215xx
GenF2.menu.pnum.GENERIC_F215VETX.build.variant=STM32F2xx/F205V(B-C-E-F-G)T_F215V(E-G)T
GenF2.menu.pnum.GENERIC_F215VETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F215.svd

# Generic F215VGTx
GenF2.menu.pnum.GENERIC_F215VGTX=Generic F215VGTx
GenF2.menu.pnum.GENERIC_F215VGTX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F215VGTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F215VGTX.build.board=GENERIC_F215VGTX
GenF2.menu.pnum.GENERIC_F215VGTX.build.product_line=STM32F215xx
GenF2.menu.pnum.GENERIC_F215VGTX.build.variant=STM32F2xx/F205V(B-C-E-F-G)T_F215V(E-G)T
GenF2.menu.pnum.GENERIC_F215VGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F215.svd

