# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F091VBTx
GenF0.menu.pnum.GENERIC_F091VBTX=Generic F091VBTx
GenF0.menu.pnum.GENERIC_F091VBTX.upload.maximum_size=131072
GenF0.menu.pnum.GENERIC_F091VBTX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F091VBTX.build.board=GENERIC_F091VBTX
GenF0.menu.pnum.GENERIC_F091VBTX.build.product_line=STM32F091xC
GenF0.menu.pnum.GENERIC_F091VBTX.build.variant=STM32F0xx/F091VBT_F091VC(H-T)
GenF0.menu.pnum.GENERIC_F091VBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

# Generic F091VCTx
GenF0.menu.pnum.GENERIC_F091VCTX=Generic F091VCTx
GenF0.menu.pnum.GENERIC_F091VCTX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F091VCTX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F091VCTX.build.board=GENERIC_F091VCTX
GenF0.menu.pnum.GENERIC_F091VCTX.build.product_line=STM32F091xC
GenF0.menu.pnum.GENERIC_F091VCTX.build.variant=STM32F0xx/F091VBT_F091VC(H-T)
GenF0.menu.pnum.GENERIC_F091VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

# Generic F091VCHx
GenF0.menu.pnum.GENERIC_F091VCHX=Generic F091VCHx
GenF0.menu.pnum.GENERIC_F091VCHX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F091VCHX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F091VCHX.build.board=GENERIC_F091VCHX
GenF0.menu.pnum.GENERIC_F091VCHX.build.product_line=STM32F091xC
GenF0.menu.pnum.GENERIC_F091VCHX.build.variant=STM32F0xx/F091VBT_F091VC(H-T)
GenF0.menu.pnum.GENERIC_F091VCHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

