# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L011K3Ux
GenL0.menu.pnum.GENERIC_L011K3UX=Generic L011K3Ux
GenL0.menu.pnum.GENERIC_L011K3UX.upload.maximum_size=8192
GenL0.menu.pnum.GENERIC_L011K3UX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L011K3UX.build.board=GENERIC_L011K3UX
GenL0.menu.pnum.GENERIC_L011K3UX.build.product_line=STM32L011xx
GenL0.menu.pnum.GENERIC_L011K3UX.build.variant=STM32L0xx/L011K(3-4)U_L021K4U
GenL0.menu.pnum.GENERIC_L011K3UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L011K4Ux
GenL0.menu.pnum.GENERIC_L011K4UX=Generic L011K4Ux
GenL0.menu.pnum.GENERIC_L011K4UX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L011K4UX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L011K4UX.build.board=GENERIC_L011K4UX
GenL0.menu.pnum.GENERIC_L011K4UX.build.product_line=STM32L011xx
GenL0.menu.pnum.GENERIC_L011K4UX.build.variant=STM32L0xx/L011K(3-4)U_L021K4U
GenL0.menu.pnum.GENERIC_L011K4UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L021K4Ux
GenL0.menu.pnum.GENERIC_L021K4UX=Generic L021K4Ux
GenL0.menu.pnum.GENERIC_L021K4UX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L021K4UX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L021K4UX.build.board=GENERIC_L021K4UX
GenL0.menu.pnum.GENERIC_L021K4UX.build.product_line=STM32L021xx
GenL0.menu.pnum.GENERIC_L021K4UX.build.variant=STM32L0xx/L011K(3-4)U_L021K4U
GenL0.menu.pnum.GENERIC_L021K4UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

