# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L496QGIxP
GenL4.menu.pnum.GENERIC_L496QGIXP=Generic L496QGIxP
GenL4.menu.pnum.GENERIC_L496QGIXP.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L496QGIXP.upload.maximum_data_size=327680
GenL4.menu.pnum.GENERIC_L496QGIXP.build.board=GENERIC_L496QGIXP
GenL4.menu.pnum.GENERIC_L496QGIXP.build.product_line=STM32L496xx
GenL4.menu.pnum.GENERIC_L496QGIXP.build.variant=STM32L4xx/L496QGIxP_L4A6QGIxP
GenL4.menu.pnum.GENERIC_L496QGIXP.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L496.svd

# Generic L4A6QGIxP
GenL4.menu.pnum.GENERIC_L4A6QGIXP=Generic L4A6QGIxP
GenL4.menu.pnum.GENERIC_L4A6QGIXP.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L4A6QGIXP.upload.maximum_data_size=327680
GenL4.menu.pnum.GENERIC_L4A6QGIXP.build.board=GENERIC_L4A6QGIXP
GenL4.menu.pnum.GENERIC_L4A6QGIXP.build.product_line=STM32L4A6xx
GenL4.menu.pnum.GENERIC_L4A6QGIXP.build.variant=STM32L4xx/L496QGIxP_L4A6QGIxP
GenL4.menu.pnum.GENERIC_L4A6QGIXP.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4A6.svd

