# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic C092RBTx
GenC0.menu.pnum.GENERIC_C092RBTX=Generic C092RBTx
GenC0.menu.pnum.GENERIC_C092RBTX.upload.maximum_size=131072
GenC0.menu.pnum.GENERIC_C092RBTX.upload.maximum_data_size=30720
GenC0.menu.pnum.GENERIC_C092RBTX.build.board=GENERIC_C092RBTX
GenC0.menu.pnum.GENERIC_C092RBTX.build.product_line=STM32C092xx
GenC0.menu.pnum.GENERIC_C092RBTX.build.variant=STM32C0xx/C092RBT_C092RC(I-T)
GenC0.menu.pnum.GENERIC_C092RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C092.svd

# Generic C092RCIx
GenC0.menu.pnum.GENERIC_C092RCIX=Generic C092RCIx
GenC0.menu.pnum.GENERIC_C092RCIX.upload.maximum_size=262144
GenC0.menu.pnum.GENERIC_C092RCIX.upload.maximum_data_size=30720
GenC0.menu.pnum.GENERIC_C092RCIX.build.board=GENERIC_C092RCIX
GenC0.menu.pnum.GENERIC_C092RCIX.build.product_line=STM32C092xx
GenC0.menu.pnum.GENERIC_C092RCIX.build.variant=STM32C0xx/C092RBT_C092RC(I-T)
GenC0.menu.pnum.GENERIC_C092RCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C092.svd

# Generic C092RCTx
GenC0.menu.pnum.GENERIC_C092RCTX=Generic C092RCTx
GenC0.menu.pnum.GENERIC_C092RCTX.upload.maximum_size=262144
GenC0.menu.pnum.GENERIC_C092RCTX.upload.maximum_data_size=30720
GenC0.menu.pnum.GENERIC_C092RCTX.build.board=GENERIC_C092RCTX
GenC0.menu.pnum.GENERIC_C092RCTX.build.product_line=STM32C092xx
GenC0.menu.pnum.GENERIC_C092RCTX.build.variant=STM32C0xx/C092RBT_C092RC(I-T)
GenC0.menu.pnum.GENERIC_C092RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C092.svd

