# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F098RCHx
GenF0.menu.pnum.GENERIC_F098RCHX=Generic F098RCHx
GenF0.menu.pnum.GENERIC_F098RCHX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F098RCHX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F098RCHX.build.board=GENERIC_F098RCHX
GenF0.menu.pnum.GENERIC_F098RCHX.build.product_line=STM32F098xx
GenF0.menu.pnum.GENERIC_F098RCHX.build.variant=STM32F0xx/F098RC(H-T-Y)
GenF0.menu.pnum.GENERIC_F098RCHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x8.svd

# Generic F098RCTx
GenF0.menu.pnum.GENERIC_F098RCTX=Generic F098RCTx
GenF0.menu.pnum.GENERIC_F098RCTX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F098RCTX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F098RCTX.build.board=GENERIC_F098RCTX
GenF0.menu.pnum.GENERIC_F098RCTX.build.product_line=STM32F098xx
GenF0.menu.pnum.GENERIC_F098RCTX.build.variant=STM32F0xx/F098RC(H-T-Y)
GenF0.menu.pnum.GENERIC_F098RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x8.svd

# Generic F098RCYx
GenF0.menu.pnum.GENERIC_F098RCYX=Generic F098RCYx
GenF0.menu.pnum.GENERIC_F098RCYX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F098RCYX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F098RCYX.build.board=GENERIC_F098RCYX
GenF0.menu.pnum.GENERIC_F098RCYX.build.product_line=STM32F098xx
GenF0.menu.pnum.GENERIC_F098RCYX.build.variant=STM32F0xx/F098RC(H-T-Y)
GenF0.menu.pnum.GENERIC_F098RCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x8.svd

