# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L412C8Tx
GenL4.menu.pnum.GENERIC_L412C8TX=Generic L412C8Tx
GenL4.menu.pnum.GENERIC_L412C8TX.upload.maximum_size=65536
GenL4.menu.pnum.GENERIC_L412C8TX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412C8TX.build.board=GENERIC_L412C8TX
GenL4.menu.pnum.GENERIC_L412C8TX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412C8TX.build.variant=STM32L4xx/L412C(8-B)(T-U)_L422CB(T-U)
GenL4.menu.pnum.GENERIC_L412C8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L412C8Ux
GenL4.menu.pnum.GENERIC_L412C8UX=Generic L412C8Ux
GenL4.menu.pnum.GENERIC_L412C8UX.upload.maximum_size=65536
GenL4.menu.pnum.GENERIC_L412C8UX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412C8UX.build.board=GENERIC_L412C8UX
GenL4.menu.pnum.GENERIC_L412C8UX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412C8UX.build.variant=STM32L4xx/L412C(8-B)(T-U)_L422CB(T-U)
GenL4.menu.pnum.GENERIC_L412C8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L412CBTx
GenL4.menu.pnum.GENERIC_L412CBTX=Generic L412CBTx
GenL4.menu.pnum.GENERIC_L412CBTX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L412CBTX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412CBTX.build.board=GENERIC_L412CBTX
GenL4.menu.pnum.GENERIC_L412CBTX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412CBTX.build.variant=STM32L4xx/L412C(8-B)(T-U)_L422CB(T-U)
GenL4.menu.pnum.GENERIC_L412CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L412CBUx
GenL4.menu.pnum.GENERIC_L412CBUX=Generic L412CBUx
GenL4.menu.pnum.GENERIC_L412CBUX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L412CBUX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412CBUX.build.board=GENERIC_L412CBUX
GenL4.menu.pnum.GENERIC_L412CBUX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412CBUX.build.variant=STM32L4xx/L412C(8-B)(T-U)_L422CB(T-U)
GenL4.menu.pnum.GENERIC_L412CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L422CBTx
GenL4.menu.pnum.GENERIC_L422CBTX=Generic L422CBTx
GenL4.menu.pnum.GENERIC_L422CBTX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L422CBTX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L422CBTX.build.board=GENERIC_L422CBTX
GenL4.menu.pnum.GENERIC_L422CBTX.build.product_line=STM32L422xx
GenL4.menu.pnum.GENERIC_L422CBTX.build.variant=STM32L4xx/L412C(8-B)(T-U)_L422CB(T-U)
GenL4.menu.pnum.GENERIC_L422CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L422.svd

# Generic L422CBUx
GenL4.menu.pnum.GENERIC_L422CBUX=Generic L422CBUx
GenL4.menu.pnum.GENERIC_L422CBUX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L422CBUX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L422CBUX.build.board=GENERIC_L422CBUX
GenL4.menu.pnum.GENERIC_L422CBUX.build.product_line=STM32L422xx
GenL4.menu.pnum.GENERIC_L422CBUX.build.variant=STM32L4xx/L412C(8-B)(T-U)_L422CB(T-U)
GenL4.menu.pnum.GENERIC_L422CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L422.svd

