# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L412K8Tx
GenL4.menu.pnum.GENERIC_L412K8TX=Generic L412K8Tx
GenL4.menu.pnum.GENERIC_L412K8TX.upload.maximum_size=65536
GenL4.menu.pnum.GENERIC_L412K8TX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412K8TX.build.board=GENERIC_L412K8TX
GenL4.menu.pnum.GENERIC_L412K8TX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412K8TX.build.variant=STM32L4xx/L412K(8-B)(T-U)_L422KB(T-U)
GenL4.menu.pnum.GENERIC_L412K8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L412K8Ux
GenL4.menu.pnum.GENERIC_L412K8UX=Generic L412K8Ux
GenL4.menu.pnum.GENERIC_L412K8UX.upload.maximum_size=65536
GenL4.menu.pnum.GENERIC_L412K8UX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412K8UX.build.board=GENERIC_L412K8UX
GenL4.menu.pnum.GENERIC_L412K8UX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412K8UX.build.variant=STM32L4xx/L412K(8-B)(T-U)_L422KB(T-U)
GenL4.menu.pnum.GENERIC_L412K8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L412KBTx
GenL4.menu.pnum.GENERIC_L412KBTX=Generic L412KBTx
GenL4.menu.pnum.GENERIC_L412KBTX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L412KBTX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412KBTX.build.board=GENERIC_L412KBTX
GenL4.menu.pnum.GENERIC_L412KBTX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412KBTX.build.variant=STM32L4xx/L412K(8-B)(T-U)_L422KB(T-U)
GenL4.menu.pnum.GENERIC_L412KBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L412KBUx
GenL4.menu.pnum.GENERIC_L412KBUX=Generic L412KBUx
GenL4.menu.pnum.GENERIC_L412KBUX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L412KBUX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L412KBUX.build.board=GENERIC_L412KBUX
GenL4.menu.pnum.GENERIC_L412KBUX.build.product_line=STM32L412xx
GenL4.menu.pnum.GENERIC_L412KBUX.build.variant=STM32L4xx/L412K(8-B)(T-U)_L422KB(T-U)
GenL4.menu.pnum.GENERIC_L412KBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L412.svd

# Generic L422KBTx
GenL4.menu.pnum.GENERIC_L422KBTX=Generic L422KBTx
GenL4.menu.pnum.GENERIC_L422KBTX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L422KBTX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L422KBTX.build.board=GENERIC_L422KBTX
GenL4.menu.pnum.GENERIC_L422KBTX.build.product_line=STM32L422xx
GenL4.menu.pnum.GENERIC_L422KBTX.build.variant=STM32L4xx/L412K(8-B)(T-U)_L422KB(T-U)
GenL4.menu.pnum.GENERIC_L422KBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L422.svd

# Generic L422KBUx
GenL4.menu.pnum.GENERIC_L422KBUX=Generic L422KBUx
GenL4.menu.pnum.GENERIC_L422KBUX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L422KBUX.upload.maximum_data_size=40960
GenL4.menu.pnum.GENERIC_L422KBUX.build.board=GENERIC_L422KBUX
GenL4.menu.pnum.GENERIC_L422KBUX.build.product_line=STM32L422xx
GenL4.menu.pnum.GENERIC_L422KBUX.build.variant=STM32L4xx/L412K(8-B)(T-U)_L422KB(T-U)
GenL4.menu.pnum.GENERIC_L422KBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L422.svd

