# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L031K4Ux
GenL0.menu.pnum.GENERIC_L031K4UX=Generic L031K4Ux
GenL0.menu.pnum.GENERIC_L031K4UX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L031K4UX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L031K4UX.build.board=GENERIC_L031K4UX
GenL0.menu.pnum.GENERIC_L031K4UX.build.product_line=STM32L031xx
GenL0.menu.pnum.GENERIC_L031K4UX.build.variant=STM32L0xx/L031K(4-6)U_L041K6U
GenL0.menu.pnum.GENERIC_L031K4UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L031K6Ux
GenL0.menu.pnum.GENERIC_L031K6UX=Generic L031K6Ux
GenL0.menu.pnum.GENERIC_L031K6UX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L031K6UX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L031K6UX.build.board=GENERIC_L031K6UX
GenL0.menu.pnum.GENERIC_L031K6UX.build.product_line=STM32L031xx
GenL0.menu.pnum.GENERIC_L031K6UX.build.variant=STM32L0xx/L031K(4-6)U_L041K6U
GenL0.menu.pnum.GENERIC_L031K6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L041K6Ux
GenL0.menu.pnum.GENERIC_L041K6UX=Generic L041K6Ux
GenL0.menu.pnum.GENERIC_L041K6UX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L041K6UX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L041K6UX.build.board=GENERIC_L041K6UX
GenL0.menu.pnum.GENERIC_L041K6UX.build.product_line=STM32L041xx
GenL0.menu.pnum.GENERIC_L041K6UX.build.variant=STM32L0xx/L031K(4-6)U_L041K6U
GenL0.menu.pnum.GENERIC_L041K6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

