# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F745IEKx
GenF7.menu.pnum.GENERIC_F745IEKX=Generic F745IEKx
GenF7.menu.pnum.GENERIC_F745IEKX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F745IEKX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F745IEKX.build.board=GENERIC_F745IEKX
GenF7.menu.pnum.GENERIC_F745IEKX.build.product_line=STM32F745xx
GenF7.menu.pnum.GENERIC_F745IEKX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F745IEKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F745.svd

# Generic F745IGKx
GenF7.menu.pnum.GENERIC_F745IGKX=Generic F745IGKx
GenF7.menu.pnum.GENERIC_F745IGKX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F745IGKX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F745IGKX.build.board=GENERIC_F745IGKX
GenF7.menu.pnum.GENERIC_F745IGKX.build.product_line=STM32F745xx
GenF7.menu.pnum.GENERIC_F745IGKX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F745IGKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F745.svd

# Generic F745IETx
GenF7.menu.pnum.GENERIC_F745IETX=Generic F745IETx
GenF7.menu.pnum.GENERIC_F745IETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F745IETX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F745IETX.build.board=GENERIC_F745IETX
GenF7.menu.pnum.GENERIC_F745IETX.build.product_line=STM32F745xx
GenF7.menu.pnum.GENERIC_F745IETX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F745IETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F745.svd

# Generic F745IGTx
GenF7.menu.pnum.GENERIC_F745IGTX=Generic F745IGTx
GenF7.menu.pnum.GENERIC_F745IGTX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F745IGTX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F745IGTX.build.board=GENERIC_F745IGTX
GenF7.menu.pnum.GENERIC_F745IGTX.build.product_line=STM32F745xx
GenF7.menu.pnum.GENERIC_F745IGTX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F745IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F745.svd

# Generic F746IEKx
GenF7.menu.pnum.GENERIC_F746IEKX=Generic F746IEKx
GenF7.menu.pnum.GENERIC_F746IEKX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F746IEKX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F746IEKX.build.board=GENERIC_F746IEKX
GenF7.menu.pnum.GENERIC_F746IEKX.build.product_line=STM32F746xx
GenF7.menu.pnum.GENERIC_F746IEKX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F746IEKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F746.svd

# Generic F746IGKx
GenF7.menu.pnum.GENERIC_F746IGKX=Generic F746IGKx
GenF7.menu.pnum.GENERIC_F746IGKX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F746IGKX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F746IGKX.build.board=GENERIC_F746IGKX
GenF7.menu.pnum.GENERIC_F746IGKX.build.product_line=STM32F746xx
GenF7.menu.pnum.GENERIC_F746IGKX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F746IGKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F746.svd

# Generic F746IETx
GenF7.menu.pnum.GENERIC_F746IETX=Generic F746IETx
GenF7.menu.pnum.GENERIC_F746IETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F746IETX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F746IETX.build.board=GENERIC_F746IETX
GenF7.menu.pnum.GENERIC_F746IETX.build.product_line=STM32F746xx
GenF7.menu.pnum.GENERIC_F746IETX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F746IETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F746.svd

# Generic F746IGTx
GenF7.menu.pnum.GENERIC_F746IGTX=Generic F746IGTx
GenF7.menu.pnum.GENERIC_F746IGTX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F746IGTX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F746IGTX.build.board=GENERIC_F746IGTX
GenF7.menu.pnum.GENERIC_F746IGTX.build.product_line=STM32F746xx
GenF7.menu.pnum.GENERIC_F746IGTX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F746IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F746.svd

# Generic F756IGKx
GenF7.menu.pnum.GENERIC_F756IGKX=Generic F756IGKx
GenF7.menu.pnum.GENERIC_F756IGKX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F756IGKX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F756IGKX.build.board=GENERIC_F756IGKX
GenF7.menu.pnum.GENERIC_F756IGKX.build.product_line=STM32F756xx
GenF7.menu.pnum.GENERIC_F756IGKX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F756IGKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F756.svd

# Generic F756IGTx
GenF7.menu.pnum.GENERIC_F756IGTX=Generic F756IGTx
GenF7.menu.pnum.GENERIC_F756IGTX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F756IGTX.upload.maximum_data_size=327680
GenF7.menu.pnum.GENERIC_F756IGTX.build.board=GENERIC_F756IGTX
GenF7.menu.pnum.GENERIC_F756IGTX.build.product_line=STM32F756xx
GenF7.menu.pnum.GENERIC_F756IGTX.build.variant=STM32F7xx/F745I(E-G)(K-T)_F746I(E-G)(K-T)_F756IG(K-T)
GenF7.menu.pnum.GENERIC_F756IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F756.svd

