# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F303K6Tx
GenF3.menu.pnum.GENERIC_F303K6TX=Generic F303K6Tx
GenF3.menu.pnum.GENERIC_F303K6TX.upload.maximum_size=32768
GenF3.menu.pnum.GENERIC_F303K6TX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F303K6TX.build.board=GENERIC_F303K6TX
GenF3.menu.pnum.GENERIC_F303K6TX.build.product_line=STM32F303x8
GenF3.menu.pnum.GENERIC_F303K6TX.build.variant=STM32F3xx/F303K(6-8)T_F334K(4-6-8)T
GenF3.menu.pnum.GENERIC_F303K6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

# Generic F303K8Tx
GenF3.menu.pnum.GENERIC_F303K8TX=Generic F303K8Tx
GenF3.menu.pnum.GENERIC_F303K8TX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F303K8TX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F303K8TX.build.board=GENERIC_F303K8TX
GenF3.menu.pnum.GENERIC_F303K8TX.build.product_line=STM32F303x8
GenF3.menu.pnum.GENERIC_F303K8TX.build.variant=STM32F3xx/F303K(6-8)T_F334K(4-6-8)T
GenF3.menu.pnum.GENERIC_F303K8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

# Generic F334K4Tx
GenF3.menu.pnum.GENERIC_F334K4TX=Generic F334K4Tx
GenF3.menu.pnum.GENERIC_F334K4TX.upload.maximum_size=16384
GenF3.menu.pnum.GENERIC_F334K4TX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F334K4TX.build.board=GENERIC_F334K4TX
GenF3.menu.pnum.GENERIC_F334K4TX.build.product_line=STM32F334x8
GenF3.menu.pnum.GENERIC_F334K4TX.build.variant=STM32F3xx/F303K(6-8)T_F334K(4-6-8)T
GenF3.menu.pnum.GENERIC_F334K4TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F3x4.svd

# Generic F334K6Tx
GenF3.menu.pnum.GENERIC_F334K6TX=Generic F334K6Tx
GenF3.menu.pnum.GENERIC_F334K6TX.upload.maximum_size=32768
GenF3.menu.pnum.GENERIC_F334K6TX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F334K6TX.build.board=GENERIC_F334K6TX
GenF3.menu.pnum.GENERIC_F334K6TX.build.product_line=STM32F334x8
GenF3.menu.pnum.GENERIC_F334K6TX.build.variant=STM32F3xx/F303K(6-8)T_F334K(4-6-8)T
GenF3.menu.pnum.GENERIC_F334K6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F3x4.svd

# Generic F334K8Tx
GenF3.menu.pnum.GENERIC_F334K8TX=Generic F334K8Tx
GenF3.menu.pnum.GENERIC_F334K8TX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F334K8TX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F334K8TX.build.board=GENERIC_F334K8TX
GenF3.menu.pnum.GENERIC_F334K8TX.build.product_line=STM32F334x8
GenF3.menu.pnum.GENERIC_F334K8TX.build.variant=STM32F3xx/F303K(6-8)T_F334K(4-6-8)T
GenF3.menu.pnum.GENERIC_F334K8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F3x4.svd

