# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F205RBTx
GenF2.menu.pnum.GENERIC_F205RBTX=Generic F205RBTx
GenF2.menu.pnum.GENERIC_F205RBTX.upload.maximum_size=131072
GenF2.menu.pnum.GENERIC_F205RBTX.upload.maximum_data_size=65536
GenF2.menu.pnum.GENERIC_F205RBTX.build.board=GENERIC_F205RBTX
GenF2.menu.pnum.GENERIC_F205RBTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205RBTX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F205RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205RCTx
GenF2.menu.pnum.GENERIC_F205RCTX=Generic F205RCTx
GenF2.menu.pnum.GENERIC_F205RCTX.upload.maximum_size=262144
GenF2.menu.pnum.GENERIC_F205RCTX.upload.maximum_data_size=98304
GenF2.menu.pnum.GENERIC_F205RCTX.build.board=GENERIC_F205RCTX
GenF2.menu.pnum.GENERIC_F205RCTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205RCTX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F205RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205RETx
GenF2.menu.pnum.GENERIC_F205RETX=Generic F205RETx
GenF2.menu.pnum.GENERIC_F205RETX.upload.maximum_size=524288
GenF2.menu.pnum.GENERIC_F205RETX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205RETX.build.board=GENERIC_F205RETX
GenF2.menu.pnum.GENERIC_F205RETX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205RETX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F205RETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205RFTx
GenF2.menu.pnum.GENERIC_F205RFTX=Generic F205RFTx
GenF2.menu.pnum.GENERIC_F205RFTX.upload.maximum_size=786432
GenF2.menu.pnum.GENERIC_F205RFTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205RFTX.build.board=GENERIC_F205RFTX
GenF2.menu.pnum.GENERIC_F205RFTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205RFTX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F205RFTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205RGTx
GenF2.menu.pnum.GENERIC_F205RGTX=Generic F205RGTx
GenF2.menu.pnum.GENERIC_F205RGTX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F205RGTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205RGTX.build.board=GENERIC_F205RGTX
GenF2.menu.pnum.GENERIC_F205RGTX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205RGTX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F205RGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205REYx
GenF2.menu.pnum.GENERIC_F205REYX=Generic F205REYx
GenF2.menu.pnum.GENERIC_F205REYX.upload.maximum_size=524288
GenF2.menu.pnum.GENERIC_F205REYX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205REYX.build.board=GENERIC_F205REYX
GenF2.menu.pnum.GENERIC_F205REYX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205REYX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F205REYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205RGYx
GenF2.menu.pnum.GENERIC_F205RGYX=Generic F205RGYx
GenF2.menu.pnum.GENERIC_F205RGYX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F205RGYX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205RGYX.build.board=GENERIC_F205RGYX
GenF2.menu.pnum.GENERIC_F205RGYX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205RGYX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F205RGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F205RGEx
GenF2.menu.pnum.GENERIC_F205RGEX=Generic F205RGEx
GenF2.menu.pnum.GENERIC_F205RGEX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F205RGEX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F205RGEX.build.board=GENERIC_F205RGEX
GenF2.menu.pnum.GENERIC_F205RGEX.build.product_line=STM32F205xx
GenF2.menu.pnum.GENERIC_F205RGEX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F205RGEX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F205.svd

# Generic F215RETx
GenF2.menu.pnum.GENERIC_F215RETX=Generic F215RETx
GenF2.menu.pnum.GENERIC_F215RETX.upload.maximum_size=524288
GenF2.menu.pnum.GENERIC_F215RETX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F215RETX.build.board=GENERIC_F215RETX
GenF2.menu.pnum.GENERIC_F215RETX.build.product_line=STM32F215xx
GenF2.menu.pnum.GENERIC_F215RETX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F215RETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F215.svd

# Generic F215RGTx
GenF2.menu.pnum.GENERIC_F215RGTX=Generic F215RGTx
GenF2.menu.pnum.GENERIC_F215RGTX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F215RGTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F215RGTX.build.board=GENERIC_F215RGTX
GenF2.menu.pnum.GENERIC_F215RGTX.build.product_line=STM32F215xx
GenF2.menu.pnum.GENERIC_F215RGTX.build.variant=STM32F2xx/F205RE(T-Y)_F205R(B-C-F)T_F205RG(E-T-Y)_F215R(E-G)T
GenF2.menu.pnum.GENERIC_F215RGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F215.svd

