# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U535CBTxQ
GenU5.menu.pnum.GENERIC_U535CBTXQ=Generic U535CBTxQ
GenU5.menu.pnum.GENERIC_U535CBTXQ.upload.maximum_size=131072
GenU5.menu.pnum.GENERIC_U535CBTXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CBTXQ.build.board=GENERIC_U535CBTXQ
GenU5.menu.pnum.GENERIC_U535CBTXQ.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CBTXQ.build.variant=STM32U5xx/U535C(B-C-E)(T-U)xQ_U545CE(T-U)xQ
GenU5.menu.pnum.GENERIC_U535CBTXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CBUxQ
GenU5.menu.pnum.GENERIC_U535CBUXQ=Generic U535CBUxQ
GenU5.menu.pnum.GENERIC_U535CBUXQ.upload.maximum_size=131072
GenU5.menu.pnum.GENERIC_U535CBUXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CBUXQ.build.board=GENERIC_U535CBUXQ
GenU5.menu.pnum.GENERIC_U535CBUXQ.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CBUXQ.build.variant=STM32U5xx/U535C(B-C-E)(T-U)xQ_U545CE(T-U)xQ
GenU5.menu.pnum.GENERIC_U535CBUXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CCTxQ
GenU5.menu.pnum.GENERIC_U535CCTXQ=Generic U535CCTxQ
GenU5.menu.pnum.GENERIC_U535CCTXQ.upload.maximum_size=262144
GenU5.menu.pnum.GENERIC_U535CCTXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CCTXQ.build.board=GENERIC_U535CCTXQ
GenU5.menu.pnum.GENERIC_U535CCTXQ.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CCTXQ.build.variant=STM32U5xx/U535C(B-C-E)(T-U)xQ_U545CE(T-U)xQ
GenU5.menu.pnum.GENERIC_U535CCTXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CCUxQ
GenU5.menu.pnum.GENERIC_U535CCUXQ=Generic U535CCUxQ
GenU5.menu.pnum.GENERIC_U535CCUXQ.upload.maximum_size=262144
GenU5.menu.pnum.GENERIC_U535CCUXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CCUXQ.build.board=GENERIC_U535CCUXQ
GenU5.menu.pnum.GENERIC_U535CCUXQ.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CCUXQ.build.variant=STM32U5xx/U535C(B-C-E)(T-U)xQ_U545CE(T-U)xQ
GenU5.menu.pnum.GENERIC_U535CCUXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CETxQ
GenU5.menu.pnum.GENERIC_U535CETXQ=Generic U535CETxQ
GenU5.menu.pnum.GENERIC_U535CETXQ.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U535CETXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CETXQ.build.board=GENERIC_U535CETXQ
GenU5.menu.pnum.GENERIC_U535CETXQ.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CETXQ.build.variant=STM32U5xx/U535C(B-C-E)(T-U)xQ_U545CE(T-U)xQ
GenU5.menu.pnum.GENERIC_U535CETXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CEUxQ
GenU5.menu.pnum.GENERIC_U535CEUXQ=Generic U535CEUxQ
GenU5.menu.pnum.GENERIC_U535CEUXQ.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U535CEUXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CEUXQ.build.board=GENERIC_U535CEUXQ
GenU5.menu.pnum.GENERIC_U535CEUXQ.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CEUXQ.build.variant=STM32U5xx/U535C(B-C-E)(T-U)xQ_U545CE(T-U)xQ
GenU5.menu.pnum.GENERIC_U535CEUXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U545CETxQ
GenU5.menu.pnum.GENERIC_U545CETXQ=Generic U545CETxQ
GenU5.menu.pnum.GENERIC_U545CETXQ.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U545CETXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U545CETXQ.build.board=GENERIC_U545CETXQ
GenU5.menu.pnum.GENERIC_U545CETXQ.build.product_line=STM32U545xx
GenU5.menu.pnum.GENERIC_U545CETXQ.build.variant=STM32U5xx/U535C(B-C-E)(T-U)xQ_U545CE(T-U)xQ
GenU5.menu.pnum.GENERIC_U545CETXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U545.svd

# Generic U545CEUxQ
GenU5.menu.pnum.GENERIC_U545CEUXQ=Generic U545CEUxQ
GenU5.menu.pnum.GENERIC_U545CEUXQ.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U545CEUXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U545CEUXQ.build.board=GENERIC_U545CEUXQ
GenU5.menu.pnum.GENERIC_U545CEUXQ.build.product_line=STM32U545xx
GenU5.menu.pnum.GENERIC_U545CEUXQ.build.variant=STM32U5xx/U535C(B-C-E)(T-U)xQ_U545CE(T-U)xQ
GenU5.menu.pnum.GENERIC_U545CEUXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U545.svd

