# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F303K6Ux
GenF3.menu.pnum.GENERIC_F303K6UX=Generic F303K6Ux
GenF3.menu.pnum.GENERIC_F303K6UX.upload.maximum_size=32768
GenF3.menu.pnum.GENERIC_F303K6UX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F303K6UX.build.board=GENERIC_F303K6UX
GenF3.menu.pnum.GENERIC_F303K6UX.build.product_line=STM32F303x8
GenF3.menu.pnum.GENERIC_F303K6UX.build.variant=STM32F3xx/F303K(6-8)U_F334K(4-6-8)U
GenF3.menu.pnum.GENERIC_F303K6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

# Generic F303K8Ux
GenF3.menu.pnum.GENERIC_F303K8UX=Generic F303K8Ux
GenF3.menu.pnum.GENERIC_F303K8UX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F303K8UX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F303K8UX.build.board=GENERIC_F303K8UX
GenF3.menu.pnum.GENERIC_F303K8UX.build.product_line=STM32F303x8
GenF3.menu.pnum.GENERIC_F303K8UX.build.variant=STM32F3xx/F303K(6-8)U_F334K(4-6-8)U
GenF3.menu.pnum.GENERIC_F303K8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

# Generic F334K4Ux
GenF3.menu.pnum.GENERIC_F334K4UX=Generic F334K4Ux
GenF3.menu.pnum.GENERIC_F334K4UX.upload.maximum_size=16384
GenF3.menu.pnum.GENERIC_F334K4UX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F334K4UX.build.board=GENERIC_F334K4UX
GenF3.menu.pnum.GENERIC_F334K4UX.build.product_line=STM32F334x8
GenF3.menu.pnum.GENERIC_F334K4UX.build.variant=STM32F3xx/F303K(6-8)U_F334K(4-6-8)U
GenF3.menu.pnum.GENERIC_F334K4UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F3x4.svd

# Generic F334K6Ux
GenF3.menu.pnum.GENERIC_F334K6UX=Generic F334K6Ux
GenF3.menu.pnum.GENERIC_F334K6UX.upload.maximum_size=32768
GenF3.menu.pnum.GENERIC_F334K6UX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F334K6UX.build.board=GENERIC_F334K6UX
GenF3.menu.pnum.GENERIC_F334K6UX.build.product_line=STM32F334x8
GenF3.menu.pnum.GENERIC_F334K6UX.build.variant=STM32F3xx/F303K(6-8)U_F334K(4-6-8)U
GenF3.menu.pnum.GENERIC_F334K6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F3x4.svd

# Generic F334K8Ux
GenF3.menu.pnum.GENERIC_F334K8UX=Generic F334K8Ux
GenF3.menu.pnum.GENERIC_F334K8UX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F334K8UX.upload.maximum_data_size=12288
GenF3.menu.pnum.GENERIC_F334K8UX.build.board=GENERIC_F334K8UX
GenF3.menu.pnum.GENERIC_F334K8UX.build.product_line=STM32F334x8
GenF3.menu.pnum.GENERIC_F334K8UX.build.variant=STM32F3xx/F303K(6-8)U_F334K(4-6-8)U
GenF3.menu.pnum.GENERIC_F334K8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F3x4.svd

