# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L451CCUx
GenL4.menu.pnum.GENERIC_L451CCUX=Generic L451CCUx
GenL4.menu.pnum.GENERIC_L451CCUX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L451CCUX.upload.maximum_data_size=163840
GenL4.menu.pnum.GENERIC_L451CCUX.build.board=GENERIC_L451CCUX
GenL4.menu.pnum.GENERIC_L451CCUX.build.product_line=STM32L451xx
GenL4.menu.pnum.GENERIC_L451CCUX.build.variant=STM32L4xx/L451CCU_L451CE(T-U)
GenL4.menu.pnum.GENERIC_L451CCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L451.svd

# Generic L451CEUx
GenL4.menu.pnum.GENERIC_L451CEUX=Generic L451CEUx
GenL4.menu.pnum.GENERIC_L451CEUX.upload.maximum_size=524288
GenL4.menu.pnum.GENERIC_L451CEUX.upload.maximum_data_size=163840
GenL4.menu.pnum.GENERIC_L451CEUX.build.board=GENERIC_L451CEUX
GenL4.menu.pnum.GENERIC_L451CEUX.build.product_line=STM32L451xx
GenL4.menu.pnum.GENERIC_L451CEUX.build.variant=STM32L4xx/L451CCU_L451CE(T-U)
GenL4.menu.pnum.GENERIC_L451CEUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L451.svd

# Generic L451CETx
GenL4.menu.pnum.GENERIC_L451CETX=Generic L451CETx
GenL4.menu.pnum.GENERIC_L451CETX.upload.maximum_size=524288
GenL4.menu.pnum.GENERIC_L451CETX.upload.maximum_data_size=163840
GenL4.menu.pnum.GENERIC_L451CETX.build.board=GENERIC_L451CETX
GenL4.menu.pnum.GENERIC_L451CETX.build.product_line=STM32L451xx
GenL4.menu.pnum.GENERIC_L451CETX.build.variant=STM32L4xx/L451CCU_L451CE(T-U)
GenL4.menu.pnum.GENERIC_L451CETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L451.svd

