# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U575CGTxQ
GenU5.menu.pnum.GENERIC_U575CGTXQ=Generic U575CGTxQ
GenU5.menu.pnum.GENERIC_U575CGTXQ.upload.maximum_size=1048576
GenU5.menu.pnum.GENERIC_U575CGTXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575CGTXQ.build.board=GENERIC_U575CGTXQ
GenU5.menu.pnum.GENERIC_U575CGTXQ.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575CGTXQ.build.variant=STM32U5xx/U575C(G-I)(T-U)xQ_U585CI(T-U)xQ
GenU5.menu.pnum.GENERIC_U575CGTXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575CGUxQ
GenU5.menu.pnum.GENERIC_U575CGUXQ=Generic U575CGUxQ
GenU5.menu.pnum.GENERIC_U575CGUXQ.upload.maximum_size=1048576
GenU5.menu.pnum.GENERIC_U575CGUXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575CGUXQ.build.board=GENERIC_U575CGUXQ
GenU5.menu.pnum.GENERIC_U575CGUXQ.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575CGUXQ.build.variant=STM32U5xx/U575C(G-I)(T-U)xQ_U585CI(T-U)xQ
GenU5.menu.pnum.GENERIC_U575CGUXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575CITxQ
GenU5.menu.pnum.GENERIC_U575CITXQ=Generic U575CITxQ
GenU5.menu.pnum.GENERIC_U575CITXQ.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U575CITXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575CITXQ.build.board=GENERIC_U575CITXQ
GenU5.menu.pnum.GENERIC_U575CITXQ.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575CITXQ.build.variant=STM32U5xx/U575C(G-I)(T-U)xQ_U585CI(T-U)xQ
GenU5.menu.pnum.GENERIC_U575CITXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575CIUxQ
GenU5.menu.pnum.GENERIC_U575CIUXQ=Generic U575CIUxQ
GenU5.menu.pnum.GENERIC_U575CIUXQ.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U575CIUXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575CIUXQ.build.board=GENERIC_U575CIUXQ
GenU5.menu.pnum.GENERIC_U575CIUXQ.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575CIUXQ.build.variant=STM32U5xx/U575C(G-I)(T-U)xQ_U585CI(T-U)xQ
GenU5.menu.pnum.GENERIC_U575CIUXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U585CITxQ
GenU5.menu.pnum.GENERIC_U585CITXQ=Generic U585CITxQ
GenU5.menu.pnum.GENERIC_U585CITXQ.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U585CITXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U585CITXQ.build.board=GENERIC_U585CITXQ
GenU5.menu.pnum.GENERIC_U585CITXQ.build.product_line=STM32U585xx
GenU5.menu.pnum.GENERIC_U585CITXQ.build.variant=STM32U5xx/U575C(G-I)(T-U)xQ_U585CI(T-U)xQ
GenU5.menu.pnum.GENERIC_U585CITXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U585.svd

# Generic U585CIUxQ
GenU5.menu.pnum.GENERIC_U585CIUXQ=Generic U585CIUxQ
GenU5.menu.pnum.GENERIC_U585CIUXQ.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U585CIUXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U585CIUXQ.build.board=GENERIC_U585CIUXQ
GenU5.menu.pnum.GENERIC_U585CIUXQ.build.product_line=STM32U585xx
GenU5.menu.pnum.GENERIC_U585CIUXQ.build.variant=STM32U5xx/U575C(G-I)(T-U)xQ_U585CI(T-U)xQ
GenU5.menu.pnum.GENERIC_U585CIUXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U585.svd

