# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U575CGTx
GenU5.menu.pnum.GENERIC_U575CGTX=Generic U575CGTx
GenU5.menu.pnum.GENERIC_U575CGTX.upload.maximum_size=1048576
GenU5.menu.pnum.GENERIC_U575CGTX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575CGTX.build.board=GENERIC_U575CGTX
GenU5.menu.pnum.GENERIC_U575CGTX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575CGTX.build.variant=STM32U5xx/U575C(G-I)(T-U)_U585CI(T-U)
GenU5.menu.pnum.GENERIC_U575CGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575CGUx
GenU5.menu.pnum.GENERIC_U575CGUX=Generic U575CGUx
GenU5.menu.pnum.GENERIC_U575CGUX.upload.maximum_size=1048576
GenU5.menu.pnum.GENERIC_U575CGUX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575CGUX.build.board=GENERIC_U575CGUX
GenU5.menu.pnum.GENERIC_U575CGUX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575CGUX.build.variant=STM32U5xx/U575C(G-I)(T-U)_U585CI(T-U)
GenU5.menu.pnum.GENERIC_U575CGUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575CITx
GenU5.menu.pnum.GENERIC_U575CITX=Generic U575CITx
GenU5.menu.pnum.GENERIC_U575CITX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U575CITX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575CITX.build.board=GENERIC_U575CITX
GenU5.menu.pnum.GENERIC_U575CITX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575CITX.build.variant=STM32U5xx/U575C(G-I)(T-U)_U585CI(T-U)
GenU5.menu.pnum.GENERIC_U575CITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575CIUx
GenU5.menu.pnum.GENERIC_U575CIUX=Generic U575CIUx
GenU5.menu.pnum.GENERIC_U575CIUX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U575CIUX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575CIUX.build.board=GENERIC_U575CIUX
GenU5.menu.pnum.GENERIC_U575CIUX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575CIUX.build.variant=STM32U5xx/U575C(G-I)(T-U)_U585CI(T-U)
GenU5.menu.pnum.GENERIC_U575CIUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U585CITx
GenU5.menu.pnum.GENERIC_U585CITX=Generic U585CITx
GenU5.menu.pnum.GENERIC_U585CITX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U585CITX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U585CITX.build.board=GENERIC_U585CITX
GenU5.menu.pnum.GENERIC_U585CITX.build.product_line=STM32U585xx
GenU5.menu.pnum.GENERIC_U585CITX.build.variant=STM32U5xx/U575C(G-I)(T-U)_U585CI(T-U)
GenU5.menu.pnum.GENERIC_U585CITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U585.svd

# Generic U585CIUx
GenU5.menu.pnum.GENERIC_U585CIUX=Generic U585CIUx
GenU5.menu.pnum.GENERIC_U585CIUX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U585CIUX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U585CIUX.build.board=GENERIC_U585CIUX
GenU5.menu.pnum.GENERIC_U585CIUX.build.product_line=STM32U585xx
GenU5.menu.pnum.GENERIC_U585CIUX.build.variant=STM32U5xx/U575C(G-I)(T-U)_U585CI(T-U)
GenU5.menu.pnum.GENERIC_U585CIUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U585.svd

