# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F098VCHx
GenF0.menu.pnum.GENERIC_F098VCHX=Generic F098VCHx
GenF0.menu.pnum.GENERIC_F098VCHX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F098VCHX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F098VCHX.build.board=GENERIC_F098VCHX
GenF0.menu.pnum.GENERIC_F098VCHX.build.product_line=STM32F098xx
GenF0.menu.pnum.GENERIC_F098VCHX.build.variant=STM32F0xx/F098VC(H-T)
GenF0.menu.pnum.GENERIC_F098VCHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x8.svd

# Generic F098VCTx
GenF0.menu.pnum.GENERIC_F098VCTX=Generic F098VCTx
GenF0.menu.pnum.GENERIC_F098VCTX.upload.maximum_size=262144
GenF0.menu.pnum.GENERIC_F098VCTX.upload.maximum_data_size=32768
GenF0.menu.pnum.GENERIC_F098VCTX.build.board=GENERIC_F098VCTX
GenF0.menu.pnum.GENERIC_F098VCTX.build.product_line=STM32F098xx
GenF0.menu.pnum.GENERIC_F098VCTX.build.variant=STM32F0xx/F098VC(H-T)
GenF0.menu.pnum.GENERIC_F098VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x8.svd

