# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G050K6Tx
GenG0.menu.pnum.GENERIC_G050K6TX=Generic G050K6Tx
GenG0.menu.pnum.GENERIC_G050K6TX.upload.maximum_size=32768
GenG0.menu.pnum.GENERIC_G050K6TX.upload.maximum_data_size=18432
GenG0.menu.pnum.GENERIC_G050K6TX.build.board=GENERIC_G050K6TX
GenG0.menu.pnum.GENERIC_G050K6TX.build.product_line=STM32G050xx
GenG0.menu.pnum.GENERIC_G050K6TX.build.variant=STM32G0xx/G050K(6-8)T
GenG0.menu.pnum.GENERIC_G050K6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G050.svd

# Generic G050K8Tx
GenG0.menu.pnum.GENERIC_G050K8TX=Generic G050K8Tx
GenG0.menu.pnum.GENERIC_G050K8TX.upload.maximum_size=65536
GenG0.menu.pnum.GENERIC_G050K8TX.upload.maximum_data_size=18432
GenG0.menu.pnum.GENERIC_G050K8TX.build.board=GENERIC_G050K8TX
GenG0.menu.pnum.GENERIC_G050K8TX.build.product_line=STM32G050xx
GenG0.menu.pnum.GENERIC_G050K8TX.build.variant=STM32G0xx/G050K(6-8)T
GenG0.menu.pnum.GENERIC_G050K8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G050.svd

