# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L432KBUx
GenL4.menu.pnum.GENERIC_L432KBUX=Generic L432KBUx
GenL4.menu.pnum.GENERIC_L432KBUX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L432KBUX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L432KBUX.build.board=GENERIC_L432KBUX
GenL4.menu.pnum.GENERIC_L432KBUX.build.product_line=STM32L432xx
GenL4.menu.pnum.GENERIC_L432KBUX.build.variant=STM32L4xx/L432K(B-C)U_L442KCU
GenL4.menu.pnum.GENERIC_L432KBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L432.svd

# Generic L432KCUx
GenL4.menu.pnum.GENERIC_L432KCUX=Generic L432KCUx
GenL4.menu.pnum.GENERIC_L432KCUX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L432KCUX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L432KCUX.build.board=GENERIC_L432KCUX
GenL4.menu.pnum.GENERIC_L432KCUX.build.product_line=STM32L432xx
GenL4.menu.pnum.GENERIC_L432KCUX.build.variant=STM32L4xx/L432K(B-C)U_L442KCU
GenL4.menu.pnum.GENERIC_L432KCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L432.svd

# Generic L442KCUx
GenL4.menu.pnum.GENERIC_L442KCUX=Generic L442KCUx
GenL4.menu.pnum.GENERIC_L442KCUX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L442KCUX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L442KCUX.build.board=GENERIC_L442KCUX
GenL4.menu.pnum.GENERIC_L442KCUX.build.product_line=STM32L442xx
GenL4.menu.pnum.GENERIC_L442KCUX.build.variant=STM32L4xx/L432K(B-C)U_L442KCU
GenL4.menu.pnum.GENERIC_L442KCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L442.svd

