# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F405OEYx
GenF4.menu.pnum.GENERIC_F405OEYX=Generic F405OEYx
GenF4.menu.pnum.GENERIC_F405OEYX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F405OEYX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F405OEYX.build.board=GENERIC_F405OEYX
GenF4.menu.pnum.GENERIC_F405OEYX.build.product_line=STM32F405xx
GenF4.menu.pnum.GENERIC_F405OEYX.build.variant=STM32F4xx/F405O(E-G)Y_F415OGY
GenF4.menu.pnum.GENERIC_F405OEYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F405.svd

# Generic F405OGYx
GenF4.menu.pnum.GENERIC_F405OGYX=Generic F405OGYx
GenF4.menu.pnum.GENERIC_F405OGYX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F405OGYX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F405OGYX.build.board=GENERIC_F405OGYX
GenF4.menu.pnum.GENERIC_F405OGYX.build.product_line=STM32F405xx
GenF4.menu.pnum.GENERIC_F405OGYX.build.variant=STM32F4xx/F405O(E-G)Y_F415OGY
GenF4.menu.pnum.GENERIC_F405OGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F405.svd

# Generic F415OGYx
GenF4.menu.pnum.GENERIC_F415OGYX=Generic F415OGYx
GenF4.menu.pnum.GENERIC_F415OGYX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F415OGYX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F415OGYX.build.board=GENERIC_F415OGYX
GenF4.menu.pnum.GENERIC_F415OGYX.build.product_line=STM32F415xx
GenF4.menu.pnum.GENERIC_F415OGYX.build.variant=STM32F4xx/F405O(E-G)Y_F415OGY
GenF4.menu.pnum.GENERIC_F415OGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F415.svd

