# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U535CBTx
GenU5.menu.pnum.GENERIC_U535CBTX=Generic U535CBTx
GenU5.menu.pnum.GENERIC_U535CBTX.upload.maximum_size=131072
GenU5.menu.pnum.GENERIC_U535CBTX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CBTX.build.board=GENERIC_U535CBTX
GenU5.menu.pnum.GENERIC_U535CBTX.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CBTX.build.variant=STM32U5xx/U535C(B-C-E)(T-U)_U545CE(T-U)
GenU5.menu.pnum.GENERIC_U535CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CBUx
GenU5.menu.pnum.GENERIC_U535CBUX=Generic U535CBUx
GenU5.menu.pnum.GENERIC_U535CBUX.upload.maximum_size=131072
GenU5.menu.pnum.GENERIC_U535CBUX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CBUX.build.board=GENERIC_U535CBUX
GenU5.menu.pnum.GENERIC_U535CBUX.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CBUX.build.variant=STM32U5xx/U535C(B-C-E)(T-U)_U545CE(T-U)
GenU5.menu.pnum.GENERIC_U535CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CCTx
GenU5.menu.pnum.GENERIC_U535CCTX=Generic U535CCTx
GenU5.menu.pnum.GENERIC_U535CCTX.upload.maximum_size=262144
GenU5.menu.pnum.GENERIC_U535CCTX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CCTX.build.board=GENERIC_U535CCTX
GenU5.menu.pnum.GENERIC_U535CCTX.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CCTX.build.variant=STM32U5xx/U535C(B-C-E)(T-U)_U545CE(T-U)
GenU5.menu.pnum.GENERIC_U535CCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CCUx
GenU5.menu.pnum.GENERIC_U535CCUX=Generic U535CCUx
GenU5.menu.pnum.GENERIC_U535CCUX.upload.maximum_size=262144
GenU5.menu.pnum.GENERIC_U535CCUX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CCUX.build.board=GENERIC_U535CCUX
GenU5.menu.pnum.GENERIC_U535CCUX.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CCUX.build.variant=STM32U5xx/U535C(B-C-E)(T-U)_U545CE(T-U)
GenU5.menu.pnum.GENERIC_U535CCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CETx
GenU5.menu.pnum.GENERIC_U535CETX=Generic U535CETx
GenU5.menu.pnum.GENERIC_U535CETX.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U535CETX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CETX.build.board=GENERIC_U535CETX
GenU5.menu.pnum.GENERIC_U535CETX.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CETX.build.variant=STM32U5xx/U535C(B-C-E)(T-U)_U545CE(T-U)
GenU5.menu.pnum.GENERIC_U535CETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535CEUx
GenU5.menu.pnum.GENERIC_U535CEUX=Generic U535CEUx
GenU5.menu.pnum.GENERIC_U535CEUX.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U535CEUX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535CEUX.build.board=GENERIC_U535CEUX
GenU5.menu.pnum.GENERIC_U535CEUX.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535CEUX.build.variant=STM32U5xx/U535C(B-C-E)(T-U)_U545CE(T-U)
GenU5.menu.pnum.GENERIC_U535CEUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U545CETx
GenU5.menu.pnum.GENERIC_U545CETX=Generic U545CETx
GenU5.menu.pnum.GENERIC_U545CETX.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U545CETX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U545CETX.build.board=GENERIC_U545CETX
GenU5.menu.pnum.GENERIC_U545CETX.build.product_line=STM32U545xx
GenU5.menu.pnum.GENERIC_U545CETX.build.variant=STM32U5xx/U535C(B-C-E)(T-U)_U545CE(T-U)
GenU5.menu.pnum.GENERIC_U545CETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U545.svd

# Generic U545CEUx
GenU5.menu.pnum.GENERIC_U545CEUX=Generic U545CEUx
GenU5.menu.pnum.GENERIC_U545CEUX.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U545CEUX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U545CEUX.build.board=GENERIC_U545CEUX
GenU5.menu.pnum.GENERIC_U545CEUX.build.product_line=STM32U545xx
GenU5.menu.pnum.GENERIC_U545CEUX.build.variant=STM32U5xx/U535C(B-C-E)(T-U)_U545CE(T-U)
GenU5.menu.pnum.GENERIC_U545CEUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U545.svd

