# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G491MCSx
GenG4.menu.pnum.GENERIC_G491MCSX=Generic G491MCSx
GenG4.menu.pnum.GENERIC_G491MCSX.upload.maximum_size=262144
GenG4.menu.pnum.GENERIC_G491MCSX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G491MCSX.build.board=GENERIC_G491MCSX
GenG4.menu.pnum.GENERIC_G491MCSX.build.product_line=STM32G491xx
GenG4.menu.pnum.GENERIC_G491MCSX.build.variant=STM32G4xx/G491M(C-E)(S-T)_G4A1ME(S-T)
GenG4.menu.pnum.GENERIC_G491MCSX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G491.svd

# Generic G491MESx
GenG4.menu.pnum.GENERIC_G491MESX=Generic G491MESx
GenG4.menu.pnum.GENERIC_G491MESX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G491MESX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G491MESX.build.board=GENERIC_G491MESX
GenG4.menu.pnum.GENERIC_G491MESX.build.product_line=STM32G491xx
GenG4.menu.pnum.GENERIC_G491MESX.build.variant=STM32G4xx/G491M(C-E)(S-T)_G4A1ME(S-T)
GenG4.menu.pnum.GENERIC_G491MESX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G491.svd

# Generic G491MCTx
GenG4.menu.pnum.GENERIC_G491MCTX=Generic G491MCTx
GenG4.menu.pnum.GENERIC_G491MCTX.upload.maximum_size=262144
GenG4.menu.pnum.GENERIC_G491MCTX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G491MCTX.build.board=GENERIC_G491MCTX
GenG4.menu.pnum.GENERIC_G491MCTX.build.product_line=STM32G491xx
GenG4.menu.pnum.GENERIC_G491MCTX.build.variant=STM32G4xx/G491M(C-E)(S-T)_G4A1ME(S-T)
GenG4.menu.pnum.GENERIC_G491MCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G491.svd

# Generic G491METx
GenG4.menu.pnum.GENERIC_G491METX=Generic G491METx
GenG4.menu.pnum.GENERIC_G491METX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G491METX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G491METX.build.board=GENERIC_G491METX
GenG4.menu.pnum.GENERIC_G491METX.build.product_line=STM32G491xx
GenG4.menu.pnum.GENERIC_G491METX.build.variant=STM32G4xx/G491M(C-E)(S-T)_G4A1ME(S-T)
GenG4.menu.pnum.GENERIC_G491METX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G491.svd

# Generic G4A1MESx
GenG4.menu.pnum.GENERIC_G4A1MESX=Generic G4A1MESx
GenG4.menu.pnum.GENERIC_G4A1MESX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G4A1MESX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G4A1MESX.build.board=GENERIC_G4A1MESX
GenG4.menu.pnum.GENERIC_G4A1MESX.build.product_line=STM32G4A1xx
GenG4.menu.pnum.GENERIC_G4A1MESX.build.variant=STM32G4xx/G491M(C-E)(S-T)_G4A1ME(S-T)
GenG4.menu.pnum.GENERIC_G4A1MESX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G4A1.svd

# Generic G4A1METx
GenG4.menu.pnum.GENERIC_G4A1METX=Generic G4A1METx
GenG4.menu.pnum.GENERIC_G4A1METX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G4A1METX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G4A1METX.build.board=GENERIC_G4A1METX
GenG4.menu.pnum.GENERIC_G4A1METX.build.product_line=STM32G4A1xx
GenG4.menu.pnum.GENERIC_G4A1METX.build.variant=STM32G4xx/G491M(C-E)(S-T)_G4A1ME(S-T)
GenG4.menu.pnum.GENERIC_G4A1METX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G4A1.svd

