# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U535RBIx
GenU5.menu.pnum.GENERIC_U535RBIX=Generic U535RBIx
GenU5.menu.pnum.GENERIC_U535RBIX.upload.maximum_size=131072
GenU5.menu.pnum.GENERIC_U535RBIX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535RBIX.build.board=GENERIC_U535RBIX
GenU5.menu.pnum.GENERIC_U535RBIX.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535RBIX.build.variant=STM32U5xx/U535R(B-C-E)I_U545REI
GenU5.menu.pnum.GENERIC_U535RBIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535RCIx
GenU5.menu.pnum.GENERIC_U535RCIX=Generic U535RCIx
GenU5.menu.pnum.GENERIC_U535RCIX.upload.maximum_size=262144
GenU5.menu.pnum.GENERIC_U535RCIX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535RCIX.build.board=GENERIC_U535RCIX
GenU5.menu.pnum.GENERIC_U535RCIX.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535RCIX.build.variant=STM32U5xx/U535R(B-C-E)I_U545REI
GenU5.menu.pnum.GENERIC_U535RCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535REIx
GenU5.menu.pnum.GENERIC_U535REIX=Generic U535REIx
GenU5.menu.pnum.GENERIC_U535REIX.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U535REIX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535REIX.build.board=GENERIC_U535REIX
GenU5.menu.pnum.GENERIC_U535REIX.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535REIX.build.variant=STM32U5xx/U535R(B-C-E)I_U545REI
GenU5.menu.pnum.GENERIC_U535REIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U545REIx
GenU5.menu.pnum.GENERIC_U545REIX=Generic U545REIx
GenU5.menu.pnum.GENERIC_U545REIX.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U545REIX.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U545REIX.build.board=GENERIC_U545REIX
GenU5.menu.pnum.GENERIC_U545REIX.build.product_line=STM32U545xx
GenU5.menu.pnum.GENERIC_U545REIX.build.variant=STM32U5xx/U535R(B-C-E)I_U545REI
GenU5.menu.pnum.GENERIC_U545REIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U545.svd

