# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L031C4Tx
GenL0.menu.pnum.GENERIC_L031C4TX=Generic L031C4Tx
GenL0.menu.pnum.GENERIC_L031C4TX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L031C4TX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L031C4TX.build.board=GENERIC_L031C4TX
GenL0.menu.pnum.GENERIC_L031C4TX.build.product_line=STM32L031xx
GenL0.menu.pnum.GENERIC_L031C4TX.build.variant=STM32L0xx/L031C(4-6)(T-U)_L041C4T_L041C6(T-U)
GenL0.menu.pnum.GENERIC_L031C4TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L031C6Tx
GenL0.menu.pnum.GENERIC_L031C6TX=Generic L031C6Tx
GenL0.menu.pnum.GENERIC_L031C6TX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L031C6TX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L031C6TX.build.board=GENERIC_L031C6TX
GenL0.menu.pnum.GENERIC_L031C6TX.build.product_line=STM32L031xx
GenL0.menu.pnum.GENERIC_L031C6TX.build.variant=STM32L0xx/L031C(4-6)(T-U)_L041C4T_L041C6(T-U)
GenL0.menu.pnum.GENERIC_L031C6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L031C4Ux
GenL0.menu.pnum.GENERIC_L031C4UX=Generic L031C4Ux
GenL0.menu.pnum.GENERIC_L031C4UX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L031C4UX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L031C4UX.build.board=GENERIC_L031C4UX
GenL0.menu.pnum.GENERIC_L031C4UX.build.product_line=STM32L031xx
GenL0.menu.pnum.GENERIC_L031C4UX.build.variant=STM32L0xx/L031C(4-6)(T-U)_L041C4T_L041C6(T-U)
GenL0.menu.pnum.GENERIC_L031C4UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L031C6Ux
GenL0.menu.pnum.GENERIC_L031C6UX=Generic L031C6Ux
GenL0.menu.pnum.GENERIC_L031C6UX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L031C6UX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L031C6UX.build.board=GENERIC_L031C6UX
GenL0.menu.pnum.GENERIC_L031C6UX.build.product_line=STM32L031xx
GenL0.menu.pnum.GENERIC_L031C6UX.build.variant=STM32L0xx/L031C(4-6)(T-U)_L041C4T_L041C6(T-U)
GenL0.menu.pnum.GENERIC_L031C6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L041C4Tx
GenL0.menu.pnum.GENERIC_L041C4TX=Generic L041C4Tx
GenL0.menu.pnum.GENERIC_L041C4TX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L041C4TX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L041C4TX.build.board=GENERIC_L041C4TX
GenL0.menu.pnum.GENERIC_L041C4TX.build.product_line=STM32L041xx
GenL0.menu.pnum.GENERIC_L041C4TX.build.variant=STM32L0xx/L031C(4-6)(T-U)_L041C4T_L041C6(T-U)
GenL0.menu.pnum.GENERIC_L041C4TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L041C6Tx
GenL0.menu.pnum.GENERIC_L041C6TX=Generic L041C6Tx
GenL0.menu.pnum.GENERIC_L041C6TX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L041C6TX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L041C6TX.build.board=GENERIC_L041C6TX
GenL0.menu.pnum.GENERIC_L041C6TX.build.product_line=STM32L041xx
GenL0.menu.pnum.GENERIC_L041C6TX.build.variant=STM32L0xx/L031C(4-6)(T-U)_L041C4T_L041C6(T-U)
GenL0.menu.pnum.GENERIC_L041C6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L041C6Ux
GenL0.menu.pnum.GENERIC_L041C6UX=Generic L041C6Ux
GenL0.menu.pnum.GENERIC_L041C6UX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L041C6UX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L041C6UX.build.board=GENERIC_L041C6UX
GenL0.menu.pnum.GENERIC_L041C6UX.build.product_line=STM32L041xx
GenL0.menu.pnum.GENERIC_L041C6UX.build.variant=STM32L0xx/L031C(4-6)(T-U)_L041C4T_L041C6(T-U)
GenL0.menu.pnum.GENERIC_L041C6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

