# Release Notes for

# STM32L4xx HAL Drivers

Copyright © 2017 STMicroelectronics

# Purpose

The STM32Cube HAL and LL, an STM32 abstraction layer embedded software, ensure maximized portability across STM32 portfolio.

The portable APIs layer provides a generic, multi instanced and simple set of APIs to interact with the upper layer (application, libraries and stacks). It is composed of native and extended APIs set. It is directly built around a generic architecture and allows the build-upon layers, like the middleware layer, to implement its functions without knowing in-depth the used STM32 device. This improves the library code reusability and guarantees an easy portability on other devices and STM32 families.

The Low Layer (LL) drivers are part of the STM32Cube firmware HAL that provides a basic set of optimized and one shot services. The Low layer drivers, contrary to the HAL ones are not fully portable across the STM32 families; the availability of some functions depends on the physical availability of the relative features on the product. The Low Layer (LL) drivers are designed to offer the following features:

- New set of inline functions for direct and atomic register access
- One-shot operations that can be used by the HAL drivers or from application level
- Full independence from HAL and standalone usage (without HAL drivers)
- Full features coverage of all the supported peripherals

# Update History

V1.13.6 / 14-November-2025

## Main Changes

- General updates to fix known defects and implementation enhancements.
- HAL code quality enhancement for MISRA-C Rule-8.13 by adding const qualifiers.
- HAL code quality enhancement for MISRA-C2012 Rule-12.1.

## Contents

- HAL code quality enhancement for MISRA-C 2012 Rule-8.13 by adding ‘const’ qualifier.
- HAL code quality enhancement for MISRA-C 2012 Rule-12.2 by adding ‘UL’ qualifier on defined const.
- Upgrated HAL drivers to be compliant with Synopsys Coverity static analysis tool.
- HAL ADC update
  - Add busy-state check in before aborting DMA.
  - Fix length param definition in HAL_ADCEx_MultiModeStart_DMA() API.
- HAL DAC update
  - Update the check for software trigger enablement by adding a verification of the Trigger selection.
- HAL I2C update
  - Improvement and simplification IsDeviceReady() function.
  - Move variable tmp declaration at the beginning in I2C_TransferCofig() function.
  - Update HAL_I2C_IsDeviceReady() API to take into account the number of trials.
  - Add support for memory transfer mode to the HAL_I2C_Master_Abort_IT() API.
- HAL FMC update
  - Change “deviceaddress” variable as volatile in HAL_NAND_Read_Page_8b(), HAL_NAND_Read_SpareArea_8b(), HAL_NAND_Read_Page_16b() and HAL_NAND_Read_SpareArea_16b() APIs to avoid compiler optimizations and ensure correct data reads.
- HAL OSPI update
  - Add HAL_OSPI_IsMemoryMapped() API.
  - change ChipSelectHighTime max limits to 64 to feat with specification.
- HAL QSPI update
  - Race condition with QSPI data transfer (DMA).
- HAL SPI update
  - Check data size before changing state in reception API.
  - Replace SD defines by MMC defines in HAL_MMC_IRQHandler() API.
  - Add note to clarify HAL_SPI_Receive() API behavior in master mode.
  - Add units to physical measurements.
  - Avoid buffer overflow in SPI_WaitFifoStateUntilTimeout().
- HAL TIM update
  - Fix update flag (UIF) clearing in TIM_Base_SetConfig.
  - Update HAL_TIMEx_ConfigBreakInput() API to fix MISRAC 2012 Rule-16.1 violation.
  - Update TIM_CCER_CCxE_MASK to support internal TIM Channel5 and TIM Channel6.
  - Fix complementary channel systematically disabled by TIM_OCx_SetConfig().
- HAL UART update
  - Correct DMA Rx abort procedure impact on ongoing Tx transfer in polling mode.
  - Correct references to HAL_UARTEx_WakeupCallback and to HAL_UART_WAKEUP_CB_ID define, according to serie capabilities.
  - Provide accurate position in RxEventCallback when ReceptionToIdle mode is used with DMA, when UART and DMA interrupts process is delayed.
  - Fix transfer count underflow when using polling mode.
- HAL SDMMC update
  - Add a check condition before aborting DMA in HAL_MMC_IRQHandler() API.
- HAL DMA update
  - Fix DMA channel mask calculation bug for DMA2.
  - Update HAL DMA request defines to reference LL DMAMUX define.
- HAL RTC update
  - Add missing enumerator ‘HAL_RTC_SSRU_EVENT_CB_ID’ to the enumerated type ‘HAL_RTC_CallbackIDTypeDef’.
  - Avoid entering initialization mode when calling HAL_RTC_Init() API if the RTC is already configured in binary mode to prevent unwanted reset of the SSR register.
- HAL USB update
  - Fix the condition on EONUM flag of DOEPCTLx register in HAL_PCD_IRQHandler() to correctly check on the frame number parity.
- LL RNG update
  - Update the LL RNG driver to support access to the HTCR register.
  - Alignment of LL RNG API naming across the STM32 series.
    - LL_RNG_SetConditioningResetBit() -> LL_RNG_EnableCondReset()
    - LL_RNG_ResetConditioningResetBit() -> LL_RNG_DisableCondReset()
    - LL_RNG_IsResetConditioningBitSet() -> LL_RNG_IsEnabledCondReset()
    - LL_RNG_IsNistComplianceEnabled() -> LL_RNG_IsEnabledNistCompliance()
    - LL_RNG_SetHealthconfiguration() -> LL_RNG_SetHealthConfig()
    - LL_RNG_GetHealthconfiguration() -> LL_RNG_GetHealthConfig()

V1.13.5 / 28-June-2024

## Main Changes

- General updates to fix known defects and implementation enhancements.
- HAL code quality enhancement for MISRA-C Rule-8.13 by adding const qualifiers.

## Contents

- LL GENERIC update
  - Update LL_SYSCFG_SetEXTISource() and LL_SYSCFG_GetEXTISource() APIs to fix CodeSonar Type-Overrun violation.
- LL ADC update
  - Remove useless action of conversion trigger change in LL_ADC_DeInit() API. Moreover, this action was not compliant with ADC enable state (cf reference manual).
- HAL GPIO update
  - Replace GPIO_Pin_x with GPIO_PIN_x to be compliant with macros definition.
- HAL/LL CORTEX update
  - Add missing parenthesis() in LL_MPU_ConfigRegion() API.
  - Updated HAL_MPU_ConfigRegion() to allow the configuration of the MPU registers independently of the value of Enable/Disable field.
  - Add new HAL_MPU_EnableRegion() / HAL_MPU_DisableRegion() APIs.
- LL DMA update
  - Fix LL_DMA_SetPeriphRequest() and LL_DMA_GetPeriphRequest() to fix MISRAC2012-Rule-12.2 violation.
- HAL DMA2D update
  - Fix incorrect word ‘surcharged’ in functions headers.
- HAL RTC update
  - Complete the check on the tamper trigger configuration in HAL_RTCEx_SetTamper_IT() API to be the same as in HAL_RTCEx_SetTamper().
- HAL HASH update
  - Code quality enhancement : Fix MISRAC Rules 12.1, 10.7, 10.6, 10.4
  - Read the last remaining bytes (3 or 2 or 1) of the data in a temporary variable (taking into account swap mode) and enter this variable into the HASH->DIN when the data is not a multiple of 4 bytes.
- HAL IWDG update
  - Calculate the maximum IWDG Timeout period “HAL_IWDG_DEFAULT_TIMEOUT”, based on a Prescaler=128 at LSI frequency=32kHz (refer to the datasheet).
- HAL PKA update
  - Remove multiple volatile reads or writes in interrupt handler for better performance.
- HAL PSSI driver
  - Replace hdmatx by hdmarx in HAL_PSSI_Receive_DMA() API.
  - Use MODIFY_REG in HAL_PSSI_Transmit() and HAL_PSSI_Receive() APIs.
- HAL/LL TIM update
  - Assert check for the right channels.
  - Fix typo in PWM symmetric mode related constants names
  - Update interrupt flag is cleared when the update event is generated by software.
  - Remove unnecessary change of MOE bitfield in LL_TIM_BDTR_Init().
  - Remove useless check on IS_TIM_ADVANCED_INSTANCE() within LL_TIM_BDTR_Init() API to fix Break Filter configuration problem with specific TIM instances.
  - Improve HAL TIM driver’s operational behavior.
  - Improve period configuration parameter check.
- LL LPTIM update
  - Remove redundant macro IS_LPTIM_AUTORELOAD().
- HAL/LL RNG update
  - Update the flag in the check if data register contains valid random data in HAL_RNG_Init() API.
  - Update the flag in new check to avoid false timeout detection in HAL_RNG_Init() API.
- HAL OSPI update
  - Fix issue related to second XSPI instance management inside XSPIM. Second instance is wrongly deactivated in case of DQS not use.
- HAL QSPI update
  - Clear AR register after CCR to avoid new transfer when address is not needed.
- HAL CAN update
  - Clarify pin configuration in driver header by removing open-drain info.
- HAL SAI update
  - Improve audio quality (avoid potential glitch).
  - Fix incorrect word ‘surcharged’ in functions headers.
- HAL UART update
  - Fix incorrect gState check in HAL_UART_RegisterRxEventCallback()/HAL_UART_UnRegisterRxEventCallback() APIs to allow user Rx Event Callback registration when a transmit is ongoing.
  - Avoid RTOF flag to be cleared by a transmit process in polling mode.
  - Add HAL_UART_RXEVENT_IDLE event notification to user in case of HAL_UARTEx_ReceiveToIdle_DMA() API use with Circular DMA, even if occurring just after TC event.
  - Align prescaler value used by default in UART_GET_DIV_FACTOR macro with RM.
  - Correct wrong comment in HAL_UARTEx_DisableFifoMode() API.
  - Ensure UART Rx buffer is not written beyond boundaries in case of RX FIFO reception in Interrupt mode.
- LL LPUART update
  - Add LL LPUART API allowing TX FIFO flush request.
- HAL USART driver
  - Align prescaler value used by default in macro USART_GET_DIV_FACTOR with Reference manual.
  - Correct wrong comment in HAL_USARTEx_DisableFifoMode() API.
  - Improve the visibility of the SPI mode support in HAL USART description.
- HAL DSI update
  - Align DSI Initialization sequence to the recommended ‘Programing procedure overview’ part to avoid DSI read LCD controller register 0x0A error.
- HAL/LL I2C update
  - Update I2C_Slave_ISR_IT(), I2C_Slave_ISR_DMA() and I2C_ITSlaveCplt() APIs to prevent the call of HAL_I2C_ListenCpltCallback() API twice.
  - Update I2C_WaitOnRXNEFlagUntilTimeout() to check I2C_FLAG_AF independently from I2C_FLAG_RXNE.
  - Remove the unusable code in function HAL_I2C_IsDeviceReady() APIs.
  - Update I2C_WaitOnFlagUntilTimeout() to handle error case.
  - Update the HAL I2C driver to implement the errata workaround “Last-received byte loss in reload mode”.
  - Update HAL_I2C_Slave_Transmit() API to check if the received NACK is the good one.
  - Update LL_I2C_HandleTranfer() API to prevent undefined behavior of volatile usage before updating the CR2 register.
  - Add a temporary variable to get the value to check before comparison.
  - Add abort memory management to HAL_I2C_Master_Abort_IT() API.
  - Move the prefetch process in HAL_I2C_Slave_Transmit() API.
- HAL SMBUS update
  - Update SMBUS IT processes to flush TXDR just in case of error.
- HAL SDMMC update
  - Fix issue related to the SD Card initialization with 4-bit bus width.
- HAL SPI update
  - Update HAL SPI driver to remove “got to” instruction and avoid misplaced __HAL_LOCK() API issue.
- HAL/LL USB update
  - pcd.c/ll_usb.c: fix device connection in case battery charging used with HS instance linked to internal FS PHY.
  - ll_usb.c: increase timeout value to allow core reset to complete
  - ll_usb.c: improve delay management to set core mode.
- LL UTILS update
  - Fix a note about Ticks parameter.

V1.13.4 / 07-June-2023

## Main Changes

- General updates to fix known defects and implementation enhancements.
- HAL code quality enhancement for MISRA-C Rule-8.13 by adding const qualifiers.

## Contents

- HAL Generic update
  - Allow redefinition of macro UNUSED(x).
  - Update of HAL_GetTickFreq() brief.
  - Add definition of UNUSED() macro to avoid the generation of a warning related to the unused argument ‘DACx’ and ‘RNGx’.
- HAL GPIO update
  - Add missing GPIO_AF14_TIM2 definition for STM32L4P5xx and STM32L4Q5xx.
- HAL EXTI update
  - Fix computation of pExtiConfig->GPIOSel in HAL_EXTI_GetConfigLine().
  - Add UNUSED() macro to avoid the generation of a warning related to the unused argument ‘Edge’.
- HAL CRC update
  - Add filter in HAL_CRCEx_Polynomial_Set() to exclude even polynomials.
- HAL CRYP update
  - Put __CRYP_HandleTypeDef definition under a compilation condition to avoid MISRAC2012-Rule-2.4 violation.
- LL ADC update
  - Correct the comment describing parameter VREFINT_CAL_VREF.
- LL COMP update
  - Remove a constant integer operand from IS_LL_COMP_OUTPUT_BLANKING_SOURCE definition to avoid MISRAC2012-Rule-10.1_R2 and MISRAC2012-Rule-10.4_b violation.
- HAL/LL DAC update
  - Fix incorrect word ‘surcharged’ in functions headers.
  - Add UNUSED() macro to avoid the generation of a warning related to the unused argument ‘DACx’.
  - Fix HAL_GetTick() timeout vulnerability.
- HAL/LL RTC update
  - Check if the RTC calendar has been previously initialized before entering Initialization mode.
  - Clear RSF flag using a single ‘write’ operation instead of a ‘read-modify-write’ sequence to avoid clearing other ISR flags if set in the meantime.
  - Avoid waiting for the RSF bit to be cleared in the LL_RTC_WaitForSynchro() API to prevent getting stuck in an infinite loop.
- HAL RCC update
  - Add a note in HAL_RCC_OscConfig() to inform the users of the steps to take if HSE failed to start.
  - Add uint32_t cast to shift left operands constants defined with ‘U’ suffix in case MISRAC2012-Rule-12.2 violated.
- HAL/LL HASH update
  - Remove initialization of local variable ‘status’ in HASH_DMAXferCplt() to avoid MISRA-C2012 Rule-2.2.c-related warning ‘Value assigned to variable is never used’.
- HAL/LL TIM update
  - Remove useless check on IS_TIM_ADVANCED_INSTANCE() within LL_TIM_BDTR_Init() to fix Break Filter configuration problem with specific TIM instances.
  - Remove Lock management from callback management functions.
- LL LPTIM update
  - Apply same naming rules to clear FLAG related functions.
  - Remove Lock management from callback management functions.
- HAL/LL RNG update
  - Add UNUSED() macro to avoid the generation of a warning related to the unused argument ‘RNGx’.
  - Update timeout mechanism to avoid false timeout detection in case of preemption.
  - Add ERROR status use case to API LL_RNG_DeInit().
- HAL TSC update
  - Add parameter assertion depends on Duration time restriction link to product.
- HAL OPAMP update
  - Fix incorrect word ‘surcharged’ in functions headers.
- HAL CAN update
  - Improve protection against bad inputs.
  - Put __CAN_HandleTypeDef definition under a compilation condition to avoid MISRAC2012-Rule-2.4 violation.
- HAL SAI update
  - Avoid using magic numbers.
- HAL UART update
  - Rework of UART_WaitOnFlagUntilTimeout() API to avoid being stuck forever when UART overrun error occurs and to enhance behavior.
  - Add new API HAL_UARTEx_GetRxEventType() to retrieve the type of event that has led the RxEventCallback execution.
  - Remove HAL_LOCK/HAL_UNLOCK calls in HAL UART Tx and Rx APIs.
  - Remove __HAL_LOCK() from HAL_xxx_RegisterCallback()/HAL_xxx_UnRegisterCallback().
  - Disable the Receiver Timeout Interrupt when data reception is completed.
  - Update initialisation sequence for TXINV, RXINV and TXRXSWAP settings.
- HAL USART update
  - Remove __HAL_LOCK() from HAL_xxx_RegisterCallback()/HAL_xxx_UnRegisterCallback().
- HAL IRDA update
  - Remove __HAL_LOCK() from HAL_xxx_RegisterCallback()/HAL_xxx_UnRegisterCallback().
- HAL SMARTCARD update
  - Remove __HAL_LOCK() from HAL_xxx_RegisterCallback()/HAL_xxx_UnRegisterCallback().
- HAL I2C update
  - Update HAL I2C driver to prefetch data before starting the transmission: implementation of errata sheet workaround I2C2-190208 : Transmission stalled after first byte.
  - Update I2C_IsErrorOccurred to return error if timeout is detected.
  - Clear the ADDRF flag only when direction is confirmed as changed, to prevent that the ADDRF flag is cleared too early when the restart is received.
  - Duplicate the test condition after timeout detection to avoid false timeout detection.
  - Update [HAL_I2C_IsDeviceReady] API to support 10_bit addressing mode: Update done on the macro I2C_GENERATE_START.
  - Update HAL I2C driver to disable all interrupts after end of transaction.
  - Update HAL_I2C_Init API to clear ADD10 bit in 7 bit addressing mode.
  - Solve Slave No stretch not functional by using HAL Slave interface.
- HAL SMBUS update
  - Update HAL I2C driver to prefetch data before starting the transmission: implementation of errata sheet workaround I2C2-190208 : Transmission stalled after first byte.
- HAL SDMMC update
  - Add UNUSED() macro to avoid the generation of a warning related to the unused argument ‘Speed’.
  - Add missing clear of the static data flags for DMA process in HAL_MMC_IRQHandler().
  - Relocate SD_HighSpeed() to avoid MISRAC2012-Rule-8.5_b violation.
- HAL SPI update
  - Fix driver to don’t update state in case of error. (HAL_SPI_STATE_READY will be set only in case of HAL_TIMEOUT).
- HAL USB OTG update
  - ll_usb.c: remove useless software setting to setup the frame interval at 80%.
  - ll_USB.c fix added to USB_ClearInterrupts() and USB_HC_Halt() APIs.
- HAL DCMI update
  - Put __DCMI_HandleTypeDef definition under a compilation condition to avoid MISRAC2012-Rule-2.4 violation.
- LL CRS update
  - Update LL_CRS_ConfigSynchronization() API to add missing shift of HSI48CalibrationValue parameter value.
- HAL USB FS update
  - (PCD): Update RX count mask to avoid overwriting the received bytes.

V1.13.3 / 15-April-2022

## Main Changes

- Maintenance release of HAL and Low Layer drivers to fix mainly HAL OSPI driver issue
- HAL code quality enhancement for MISRA-C Rule-8.13 by adding const qualifiers

## Contents

- HAL RCC
  - Fix HCLK prescaler update in HAL_RCC_ClockConfig() to avoid issue with CPU clock being out of range versus the Flash latency.
  - Wait PLL1RDY to be off before clearing PLL1 source
- HAL FLASH
  - Complete description of USERConfig, member of structure FLASH_OBProgramInitTypeDef.
- HAL EXTI
  - Fix EXTI_GPIOG defined value issue.
- HAL DSI
  - Update to align DSI ULPS entry and exit sequences with reference manual.
- HAL/LL TIM
  - Manage configuration of the Capture/compare DMA request source
  - Add related new exported constants (TIM_CCDMAREQUEST_CC, TIM_CCDMAREQUEST_UPDATE).
  - Create a new macro __HAL_TIM_SELECT_CCDMAREQUEST() allowing to program the TIMx_CR2.CCDS bitfield.
  - Update __LL_TIM_CALC_PSC() macro to round up the evaluated value when the fractional part of the division is greater than 0.5.
- HAL LTDC
  - Update HAL_LTDC_DeInit() to fix MCU Hang up during LCD turn OFF.
- HAL QSPI
  - Update HAL_QSPI_Abort() and HAL_QSPI_Abort_IT() APIs to check on QSPI BUSY flag status before executing the abort procedure.
- HAL OSPI
  - Update HAL_OSPI_Init() to fix DelayBlockBypass parameter configuration issue.
- HAL I2C
  - Timeout issue using HAL MEM interface through FreeRTOS
- HAL CAN
  - Removal of never reached code
- HAL USB OTG
  - PCD: add handling of USB OUT Endpoint disable interrupt
  - PCD: fix device IN endpoint isoc incomplete transfer interrupt handling
  - PCD: fix USB device Isoc OUT Endpoint incomplete transfer interrupt handling
  - HAL: HCD: fix handling of ODDFRM bit in OTG_HCCHARx for Isochronous IN transactions
  - HAL: PCD: added fix to correct received transfer length with USB DMA activated
- HAL USB FS
  - PCD: add supporting multi packets transfer on Interrupt endpoint
  - Set DCD timeout to minimum of 300ms before starting BCD primary detection process.
  - HAL: PCD: software correction added to avoid unexpected STALL condition during EP0 multi packet OUT transfer.

V1.13.2 / 26-November-2021

## Main Changes

- Maintenance release of HAL and Low Layer drivers to include latest corrections

## Contents

- RCC_HAL
  - Update IS_RCC_PERIPHCLOCK() macro definition depending on targeted derivative.
  - Add new HAL_RCC_GetResetSource() API to get all reset sources and clear flags.
  - Update PLL clock source configuration to fix warnings with the GCC compiler
- EXTI_HAL
  - Update HAL_EXTI_GetConfigLine() API to set default configuration value of Trigger and GPIOSel before checking each corresponding registers.
- FLASH_HAL
  - Disable ICache while Flash programming.
  - Update HAL_FLASHEx_Erase() to remove __HAL_FLASH_INSTRUCTION_CACHE_DISABLE().
- GPIO_HAL
  - Update HAL_GPIO_Init() API to avoid the configuration of PUPDR register when Analog mode is selected.
  - Optimize assertion control for GPIO Pull mode in HAL_GPIO_Init() API.
  - Reorder EXTI configuration sequence in order to avoid unexpected level detection.
- ADC_HAL/LL
  - Update of the TEMPSENSOR_CAL2_TEMP value in the ll_adc.h file.
  - Remove useless binary mask.
  - Update LL_ADC driver to prevent unused argument compilation warning.
- RTC_BKP_HAL/LL
  - Update __HAL_RTC_…(HANDLE, …) macros to access registers through (HANDLE)->Instance pointer and avoid "unused variable" warnings.
  - Fix bad reference to RTC handle in LL_RTC_TIME_Init() & LL_RTC_DATE_Init() APIs
- CAN_HAL
  - Update HAL_CAN_Init() API to be aligned with reference manual and to avoid timeout error:
    - Update CAN Initialization sequence to set "request initialization" bit before exit from sleep mode.
- SPI_HAL/LL
  - General update to fix MISRA-C 2012 Rule-13.2 issue.
  - Update LL_SPI_TransmitData8() API to avoid casting the result to 8 bits.
- I2C_HAL
  - Fix written reserved bit 28 in I2C_CR2 register
  - Updated I2C_IsAcknowledgeFailed() API to avoid I2C in busy state if NACK received after transmitting register address.
  - Update to handle errors in polling mode.
    - Rename I2C_IsAcknowledgeFailed() to I2C_IsErrorOccurred() and correctly manage when error occurs.
  - Update to fix issue detected due to low system frequency execution (HSI).
  - Declare an internal macro link to DMA macro to check remaining data: I2C_GET_DMA_REMAIN_DATA
- SMBUS_HAL
  - Update to fix issue of mismatched data received by master in case of data size to be transmitted by the slave is greater than the data size to be received by the master.
    - Add flush on TX register.
  - Add the support of wake up capability.
    - Add new APIs:
      - HAL_SMBUSEx_EnableWakeUp()
      - HAL_SMBUSEx_DisableWakeUp()
- UART_HAL
  - Fix erroneous UART’s handle state in case of error returned after DMA reception start within UART_Start_Receive_DMA().
  - Correction on UART ReceptionType management in case of ReceptionToIdle API are called from RxEvent callback
  - Handling of UART concurrent register access in case of race condition between Tx and Rx transfers (HAL UART and LL LPUART)
  - Improve header description of UART_WaitOnFlagUntilTimeout() function
  - Add a check on the UART parity before enabling the parity error interruption.
  - Add const qualifier for read only pointers.
  - Fix wrong cast when computing the USARTDIV value in UART_SetConfig().
- LPUART_LL
  - Remove TXFECF reference from LL LPUART driver
- USART_HAL/LL
  - Handling of UART concurrent register access in case of race condition between Tx and Rx transfers (HAL UART and LL LPUART)
  - Fix compilation warnings generated with ARMV6 compiler
  - Improve header description of USART_WaitOnFlagUntilTimeout() function
  - Add a check on the USART parity before enabling the parity error interrupt.
  - Add const qualifier for read only pointers.
- SMARTCARD_HAL
  - Improve header description of SMARTCARD_WaitOnFlagUntilTimeout() function
  - Add const qualifier for read only pointers.
  - Fix wrong cast when computing the USARTDIV value in SMARTCARD_SetConfig().
- IRDA_HAL
  - Improve header description of IRDA_WaitOnFlagUntilTimeout() function
  - Add a check on the IRDA parity before enabling the parity error interrupt.
  - Add const qualifier for read only pointers.
  - Fix wrong cast when computing the USARTDIV value in IRDA_SetConfig().
- DSI_HAL
  - Update HAL_DSI_Read() to avoid HAL_TIMEOUT when a DSI read command is issued to the panel and the read data is not captured by the DSI Host which returns Packet Size Error.
- TIM_HAL
  - Fix compilation warnings on MDK-ARM
  - Update HAL_TIMEx_ConfigBreakInput to use CMSIS TIM1_OR2_BKDF1BK0E_Pos definition instead of its hard coded value.
- LPTIM_HAL
  - Add __HAL_LPTIM_RESET_COUNTER and __HAL_LPTIM_RESET_COUNTER_AFTERREAD macros managing the synchronous/asynchronous LPTIM counter reset.
  - Add check on PRIMASK register to prevent from enabling unwanted global interrupts within LPTIM_Disable() and LL_LPTIM_Disable()
- NOR_HAL
  - Align HAL_NOR_Init() API with core of the function when write operation is disabled to avoid HardFault.
- SDMMC_HAL
  - Fix Incorrect command sent in MMC_PowerOn
    - Update SEND_OP_COND (CMD1) to indicate as argument that the sector mode is supported by the host.
- PKA_HAL
  - Update to fix Montgomery multiplication in PKA.
- USB_FS_HAL
  - HAL PCD: add fix transfer complete for IN Interrupt transaction in single buffer mode
- USB_OTG_HAL
  - Add new API HAL_PCD_EP_Abort() to abort current USB endpoint transfer.
- IWDG_HAL
  - Update HAL_IWDG_Init() API in order to fix HAL_GetTick() timeout vulnerability issue.
  - Add LSI startup time in default IWDG timeout calculation (HAL_IWDG_DEFAULT_TIMEOUT).

V1.13.1 / 24-September-2021

## Main Changes

- Patch release only of ** USB HAL and Low Layer** drivers to include latest corrections

## Contents

HAL drivers changes

- HAL USB PCD driver
  - Fix double buffer mode isochronous IN transfer
  - Optimize USB IRQ handler by removing multiple reads from USB interrupt registers
- HAL USB HCD driver
  - Optimize USB IRQ handler by removing multiple reads on USB interrupt registers

LL drivers changes

- LL USB driver
  - Correction added on USB_ReadPacket() to ensure a byte by byte read from USB FiFO

V1.13.0 / 11-February-2021

## Main Changes

- Maintenance release of HAL and Low Layer drivers to include latest corrections
  - Update of HAL SMBUS driver to introduce fast mode and fast mode plus
    - Add extension files stm32l4xx_hal_smbus_ex.h/.c for new APIs:
      - HAL_SMBUSEx_EnableFastModePlus()
      - HAL_SMBUSEx_DisableFastModePlus()
  - Update of HAL UART driver introducing enhanced reception services
    - HAL_StatusTypeDef HAL_UARTEx_ReceiveToIdle()
    - HAL_StatusTypeDef HAL_UARTEx_ReceiveToIdle_IT()
    - HAL_StatusTypeDef HAL_UARTEx_ReceiveToIdle_DMA()

## Contents

### HAL/LL generic updates

- stm32l4xx_hal_timebase_tim_template.c
  - Update Tick priority handling in HAL_Init_Tick()

### HAL Drivers updates

- HAL ADC driver
  - Fix delay computation of the local variable wait_loop_index at low system core clock frequency
  - Fix to avoid Error state returned by IRQ handler in case of injected conversion + IT mode + trigger timer
  - Update HAL_ADC_DeInit() description and behaviour to call MspDeInit() only when all ADC instances sharing the same common ADC instance are disabled
  - Update timeout mechanism to avoid false timeout detection in case of preemption
  - Extend internal regulator stabilization time from 10us to 20us
- HAL COMP driver
  - Fix delay computation of the local variable wait_loop_index at low system core clock frequency
- HAL EXTI driver
  - Replace macro parameter __LINE__ by __EXTI_LINE__ to avoid conflicts with standard C usage
- HAL GPIO driver
  - Add AF6 missing definitions : GPIO_AF6_OCTOSPIM_P1 / GPIO_AF6_OCTOSPIM_P2
- HAL IWDG driver
  - Update definition of HAL_IWDG_DEFAULT_TIMEOUT to avoid issue with the watchdog init procedure
- HAL LPTIM driver
  - Update external clock configuration to cover all ClockSource/CounterSource combinations
- HAL NAND driver
  - Update address calculation in HAL_NAND_Read_SpareArea_16b() and HAL_NAND_Write_SpareArea_16b()
  - Fix issue in the access to NAND 8-bits memories with 16-bits APIs
- HAL OPAMP driver
  - Align OPAMP PowerMode definitions with others series
- HAL RCC driver
  - Update IS_RCC_CRS_HSI48CALIBRATION() definition to have specific maximum value for STM32L412xx/L422xx devices
  - Update RCC_HSICALIBRATION_DEFAULT definition depending on devices
- HAL RTC driver
  - Update the description of HAL_RTC_SetTime() to mention that the DayLightSaving attribute of sTime should not be used
  - Add Daylight Saving Time service
  - Update HAL_RTC_DeactivateAlarm() to fix issue during Alarm Autoclear
  - Update HAL_RTC_SetTime() to add back assert_param() functions checking daylight saving parameters
- HAL SDMMC driver
  - Update driver to enable interrupt after treating the single write command or multiple write command
  - Update eMMC High Speed Mode management
- HAL SMSBUS driver
  - Implementation of fast mode and fast mode plus
    - Add extension files stm32l4xx_hal_smbus_ex.h/.c for new APIs:
      - HAL_SMBUSEx_EnableFastModePlus()
      - HAL_SMBUSEx_DisableFastModePlus()
- HAL SPI driver
  - Fix SPI_WaitFifoStateUntilTimeout()
- HAL TIM driver
  - Update callback function invoked upon Half DMA transfer completion
  - Fix in HAL_TIM_OnePulse_Start() to handle OutputChannel parameter
  - Update HAL_TIM_IC_Start_DMA() to ensure correct behavior of counter value latch delay at high frequency
- HAL TSC driver
  - Add assertion when fordidden configurations of bit value PGPSC versus bit value CTPL are requested by user
- HAL UART driver
  - Remove FifoMode use in UART_SetConfig()
  - Add a HAL UART service to enable RTO interrupt
  - Implementation of HAL UART enhanced reception services (ReceptionToIdle)
    - HAL_StatusTypeDef HAL_UARTEx_ReceiveToIdle()
    - HAL_StatusTypeDef HAL_UARTEx_ReceiveToIdle_IT()
    - HAL_StatusTypeDef HAL_UARTEx_ReceiveToIdle_DMA()
- HAL UART/USART/IRDA/SMARTCARD drivers
  - Fix typos in State definition description
  - Update parameter array to be always declared as static const
- HAL SMARTCARD driver
  - Remove FifoMode use in SMARTCARD_SetConfig()
- HAL USB driver
  - Fix regression in HAL USB double buffer mode
- HAL WWDG driver
  - Update HAL WWDG driver description

### LL Drivers updates

- LL DMA driver
  - Update LL_DMA_ClearFlag_GIx() to add text informing user not to clear GIx when channel is ON
- LL FMC driver
  - Fix compilation warning with gcc -Wpedantic compiler option
- LL GPIO driver
  - Update GPIO configuration order to avoid a glitch on the bus-lines when using CAN
- LL OPAMP driver
  - Align OPAMP PowerMode definitions with others series
- LL RCC driver
  - Update RCC private functions declaration to static
- LL SPI driver
  - Update LL_SPI_Init() to et Rx FIFO to Quarter (1 Byte) in case of 8 Bits mode
- LL TIM driver
  - Update return value of LL_TIM_GetCounterMode()
  - Update LL_TIM_ONEPULSEMODE_SINGLE and LL_TIM_ONEPULSEMODE_REPETITIVE defines description
- LL USART driver
  - Update LL_USART_ClockInit() to allow the configuration of clock phase and polarity even if CR2_CLKEN is cleared
  - Remove useless IS_LL_USART_BRR_MAX() macro

V1.12.0 / 26-June-2020

## Main Changes

- Maintenance release of HAL and Low Layer drivers to include latest corrections
- Update of HAL OSPI driver introducing compatibility break with previous versions

## Contents

### HAL/LL generic updates

- Remove the use of keyword register in HAL/LL drivers

### HAL Drivers updates

- HAL CAN driver
  - Update HAL_CAN_GetRxMessage() to remove shift on RTR field of the structure CAN_RxHeaderTypeDef
- HAL DAC driver
  - Update HAL_DAC_ConfigChannel() to add correction on timout handling for sample and hold configuration on CHANNEL_2
  - Update HAL_DAC_Stop_DMA() to return HAL_OK value and avoid HAL_DAC_STATE_ERROR return value in case HAL_DMA_Abort return HAL_ERROR
- HAL DCMI driver
  - Update HAL_DCMI_Start_DMA() to manage DMA transfers larger than 0xFFFF
- HAL DMA driver
  - Update HAL_DMA_PollForTransfer() to move the UNLOCK process once the transfer is completed
- HAL FLASH driver
  - Correct MISRA C:2012-Rule-8.5 warning in HAL FLASH driver
  - Update __HAL_FLASH_GET_FLAG macro to correct the return value (when the flag ECCD is set to 1)
- HAL GPIO driver
  - Add definition of GPIO_AF14_TIM2 missing for STM32L4R5xx products
  - Fix HAL_GPIO_TogglePin() to manage several pins
- HAL driver
  - Add HAL_TickFreqTypeDef type definition for HAL_SetTickFreq() parameter and HAL_GetTickFreq() function
- HAL I2C driver
  - Update of HAL I2C driver to correct some typo in comments
- HAL LPTIM driver
  - Update HAL_LPTIM_Init() to allow digital filter configuration for external clock whatever the LPTIM clock source is
- HAL NAND/NOR driver
  - Correct MISRA C:2012-Rule-7.2 warning in HAL NAND/NOR drivers
  - Correct MISRA C:2012-Rule-10.4_a / 14.4_d / 18.4 warnings in HAL NOR drivers
  - Update address calculation in HAL_NOR_ProgramBuffer()
  - Update HAL_NOR_ProgramBuffer() to fix CodeSonar warnings
- HAL OPAMP driver
  - Update HAL_OPAMP_Init() to fix CodeSonar warnings
- HAL OSPI driver
  - Update HAL_OSPIM_Config() to adapt the assert checks with OCTOSPI selected mode
  - The following updates introduce compatibility break with previous version of HAL OSPI driver
    - The wrap functionality is no more supported by the STM32L4+ products :
      - Remove WrapSize field of the initialization structure OSPI_InitTypeDef
      - Remove HAL_OSPI_OPTYPE_WRAP_CFG value for OperationType field within regular command structure OSPI_RegularCmdTypeDef
    - The delay block can be bypassed in the STM32L4+ products :
      - Add DelayBlockBypass field within the initialization structure OSPI_InitTypeDef
    - The multiplex mode is allowed in the OSPI IO manager for the STM32L4+ 1M products :
      - Add MaxTran field within the initialization structure OSPI_InitTypeDef
- HAL RCC driver
  - Update IS_RCC_PLLSAI1N_VALUE() and IS_RCC_PLLSAI2N_VALUE() macros with new RCC_PLLSAI1N_MUL_8_127_SUPPORT and RCC_PLLSAI2N_MUL_8_127_SUPPORT definitions
  - Update RCC_HSICALIBRATION_DEFAULT definition
  - Update __HAL_RCC_APB1_FORCE_RESET() and __HAL_RCC_APB1_RELEASE_RESET() macros to handle RCC_APB1RSTR1 and RCC_APB1RSTR2 updates
- HAL SDMMC driver
  - Add support of Sanitize and FTRIM/discard functions for HAL eMMC functionality
  - Add new API function HAL_MMC_GetCardExtCSD() to allow the user application to get the Extended CSD register
  - Update HAL_MMC_InitCard() and HAL_SD_InitCard() to fix CodeSonar warnings
  - Update MMC_ReadExtCSD() and MMC_PwrClassUpdate() to fix STM32CubeIDE compilation warnings
- HAL SMARTCARD driver
  - Update NACK management in HAL_SMARTCARD_Transmit(), HAL_SMARTCARD_Transmit_IT() and HAL_SMARTCARD_Transmit_DMA() functions
- HAL SMBUS driver
  - Update of HAL SMBUS driver to correct some typo in comments
- HAL SPI driver
  - Correct MISRA C:2012-Rule-17.8 warning in HAL SPI driver
  - Update HAL_SPI_Transmit(), HAL_SPI_Receive() functions to fix in 3-wires communication (disable and enable SPI)
  - Update SPI_DMAReceiveCplt() to disable Rx/Tx DMA Request (done by default to handle the case master rx direction 2 lines)
  - Update HAL SPI driver to fix timeout management inside SPI DMA xfer complete handler
  - Update HAL_SPI_Init() to handle assert on BaudRatePrescaler in Slave Motorola mode
- HAL TIM driver
  - Correct MISRA C:2012-Rule-2.2 warning in HAL TIM driver
  - Update DMA management when DMA requests are used for several channels of the same timer
  - Update HAL_TIM_IC_Stop_DMA() to stop DMA prior to disabling the channel
  - Add new HAL_TIM_DMABurst_MultiWriteStart() and HAL_TIM_DMABurst_MultiReadStart() API in HAL TIM driver
  - Update all HAL_TIM_xxx_Start() functions to allow the check of the TIMx_SMCR.SMS bit if the timer instance is slave mode capable
  - Update references to TIM_DMABASE_AF1 and TIM_DMABASE_AF2
  - Update HAL_TIM_DMABurst_WriteStop() and HAL_TIM_DMABurst_ReadStop() to modify calls to HAL_DMA_Abort_IT().
- HAL TSC driver
  - Correct MISRA C:2012-Rule-2.4 warning in HAL TSC driver
  - Update IS_TSC_GROUP() macro definition to manage when field ChannelIOs or ShieldIOs or SamplingIOs are set to 0
- HAL UART driver
  - Rework BRR register value computation in HAL_UART_Init() for ROM size gain
  - Update HAL_UART_IRQHandler() to handle UART Receive Timeout interruption in the ISR function
- HAL USART driver
  - Update HAL_USARTEx_DisableSlaveMode() to correct SlaveMode field value
- HAL WWDG driver
  - Update WWDG clock frequency, min, and max timeout values in header description

### LL Drivers updates

- LL FMC driver
  - Correct MISRA C:2012-Rule-7.2 warning in LL FMC driver
- LL GPIO driver
  - Fix LL_GPIO_TogglePin() to manage several pins
  - Update LL_GPIO_TogglePin() to use the BSRR register rather than reading / modifying the ODR.
- LL I2C driver
  - Update of LL I2C driver to correct some typo in comments
- LL RCC driver
  - Update LL_RCC_HSI_SetCalibTrimming definition
- LL TIM driver
  - Update RepetitionCounter parameter in LL_TIM_StructInit()
  - Invert LL_TIM_COUNTERMODE_CENTER_DOWN and LL_TIM_COUNTERMODE_CENTER_UP definitions

V1.11.1 / 07-February-2020

## Main Changes

- Patch release of HAL and Low Layer drivers to include latest corrections

## Contents

HAL drivers changes

- HAL GPIO driver
  - Update HAL_GPIO_Init() initialization sequence to modify the order of GPIO registers update
- HAL I2C driver
  - Update I2C_Enable_IRQ() function to remove incorrect interrupts enable when InterruptRequest = I2C_XFER_CPLT_IT
  - Update I2C_DMAXferCplt(), I2C_DMAError() and I2C_DMAAbort() functions to avoid null pointer exceptions
  - Update HAL_I2C_Master_Seq_Transmit/Receive_IT/DMA() functions to set correct condition range
  - Update I2C_ITMasterCplt() to remove C++ compilation warning due to unused variable
- HAL RTC driver
  - Correct MISRA C:2012-Rule-3.1 warning in RTC driver
- HAL SDMMC driver
  - Update MMC_InitCard() function to add missing correction for eMMC card size computation issue
  - Update SD_UltraHighSpeed() and SD_DDR_Mode() functions to remove useless assignment
  - Correct MISRA C:2012 warnings in SDMMC driver (rules 10.4_a, 10.7, 13.5, 15.7, 2.2_c)
- HAL SMBUS driver
  - Update IS_SMBUS_TRANSFER_OPTIONS_REQUEST macro definition to include transfers with PEC
  - Correct MISRA C:2012-Rule-2.4 warning in structure __SMBUS_HandleTypeDef definition

LL drivers changes

- LL UTILS driver
  - Change private UTILS_SetFlashLatency() function into LL_SetFlashLatency() public function
  - Update LL_PLL_ConfigSystemClock_MSI/HSI/HSE() functions to set expected AHB prescaler value

V1.11.0 / 22-November-2019

## Main Changes

- Release of HAL and Low Layer drivers to add support of STM32L4P5xx/STM32L4Q5xx devices
  - New PKA and PSSI peripherals supported in new HAL/LL PKA and HAL PSSI drivers
- Superset features device STM32L4Q5xx API User Manual available (STM32L4Q5xx_User_Manual.chm)
- Correction of several issues applicable to other devices

## Contents

HAL drivers changes

- HAL driver
  - Add the following constants and macros definitions in stm32l4xx_hal.h for STM32L4P5xx/STM32L4Q5xx devices
    - SYSCFG_BOOT_FMC
    - SYSCFG_BOOT_OCTOPSPI1
    - SYSCFG_BOOT_OCTOPSPI2
    - __HAL_SYSCFG_REMAPMEMORY_FMC()
    - __HAL_SYSCFG_REMAPMEMORY_OCTOSPI1()
    - __HAL_SYSCFG_REMAPMEMORY_OCTOSPI2()
- HAL ADC driver
  - Update IS_ADC_CHANNEL() macro in stm32l4xx_hal_adc_ex.h to encompass all ADC2 channels for STM32L4P5xx/STM32L4Q5xx devices
  - Correct channel status mask computation in DMA_CalcDMAMUXChannelBaseAndMask() function
- HAL DAC driver
  - Correct HAL_DAC_UnRegisterCallback() API to fix compilation error when USE_HAL_DAC_REGISTER_CALLBACKS is equal to 1
- HAL DFSDM driver
  - Update the return check of HAL_DMA_Abort() in HAL_DFSDM_FilterRegularStop_DMA() and HAL_DFSDM_FilterInjectedStop_DMA() APIs
- HAL DMA driver
  - Define DMAMUX request constant DMA_REQUEST_PSSI in stm32l4xx_hal_dma.h to enable PSSI peripheral DMA transfers for STM32L4P5xx/STM32L4Q5xx devices
  - Correct channel status mask computation in DMA_CalcDMAMUXChannelBaseAndMask() function
- HAL DMA2D driver
  - Remove unused DMA2D_ColorTypeDef structure from stm32l4xx_hal_dma2d.h
  - Add new HAL_DMA2D_CLUTStartLoad() and HAL_DMA2D_CLUTStartLoad_IT() APIs to improve code compactness, code size and heap usage when loading CLUT
  - Add @note to HAL_DMA2D_CLUTLoad(), HAL_DMA2D_CLUTLoad_IT() and HAL_DMA2D_ConfigCLUT() APIs to inform the user the latter are marked as obsolete and kept only to maintain compatibility with legacy
- HAL FLASH driver
  - Correct FLASH_FLAG_SR_ERRORS and remove FLASH_FLAG_PEMPTY constants definitions in stm32l4xx_hal_flash.h for STM32L496xx/STM32L4A6xx since FLASH_SR PEMPTY bit is not defined for these devices
  - Update declaration of APIs HAL_FLASHEx_EnableRunPowerDown(), HAL_FLASHEx_DisableRunPowerDown() and HAL_FLASHEx_OB_DBankConfig() in stm32l4xx_flash_ramfunc.h and stm32l4xx_flash_ramfunc.c to implement new __RAM_FUNC definition
  - Correct API FLASH_PageErase() in stm32l4xx_hal_flash_ex.c to make sure DBANK bit of FLASH_OPTR register is tested before a page erasure for STM32L4P5xx/STM32L4Q5xx devices
- HAL FMC driver
  - Add PSRAM chip select counter management for STM32L4P5xx/STM32L4Q5xx devices in the following APIs
    - FMC_NORSRAM_Init()
    - FMC_NORSRAM_DeInit()
- HAL GENERIC driver
  - Correct __RAM_FUNC define in stm32l4xx_hal_def.h in order not to impose function type
- HAL GPIO driver
  - Add GPIO_AF11_SDMMC2 and GPIO_AF12_SDMMC2 alternate functions definitions in stm32l4xx_hal_gpio_ex.h for STM32L4P5xx/STM32L4Q5xx devices
  - Define PSSI alternalte functions definitions GPIO_AF4_PSSI, GPIO_AF5_PSSI and GPIO_AF10_PSSI for STM32L4P5xx/STM32L4Q5xx devices
- HAL HASH driver
  - Correct phase management issue when performing two successive hash operations on two different buffers
  - Enhance digest computation in polling mode in authorizing hashing of empty buffers
  - Fix Misra C:2012 Rule-5.1 warning on identifiers to be distinct in the first 31 characters in renaming all HAL_HASH_xxx_Accumulate_yy() and HAL_HASHEx_xxx_Accumulate_yy() APIs respectively into HAL_HASH_xxx_Accmlt_yy() and HAL_HASHEx_xxx_Accmlt_yy()
  - Create new APIs to wrap-up multi-buffer hashing processing in polling and interrupt modes
    - HAL_HASH_MD5_Accmlt_End()
    - HAL_HASH_SHA1_Accmlt_End()
    - HAL_HASHEx_SHA224_Accmlt_End()
    - HAL_HASHEx_SHA256_Accmlt_End()
    - HAL_HASH_MD5_Accmlt_End_IT()
    - HAL_HASH_SHA1_Accmlt_End_IT()
    - HAL_HASHEx_SHA224_Accmlt_End_IT()
    - HAL_HASHEx_SHA256_Accmlt_End_IT()
  - Update example 32L4P5GDISCOVERY/Examples/HASH/HASH_HMAC_SHA224SHA256_MultiBuffer_DMA to illustrate how to use one of these APIs listed above
  - Ensure processing suspension flag is reset to HAL_HASH_SUSPEND_NONE value in HAL_HASH_Init() API
- HAL I2C driver
  - Fix slave interrupt handling issue in checking STOPF bit at the beginning of the interrupt handling and no more at the end. Correction done in both I2C_Slave_ISR_IT() and I2C_Slave_ISR_DMA() static functions to consider interrupt and DMA cases.
  - Fix Misra C:2012 Rule-2.2_c warning on value assigned to a never used variable in I2C_Slave_ISR_IT() static function
- HAL MMC driver
  - Implement DDR mode and High Speed feature for STM32L4P5xx/STM32L4Q5xx and STM32L4Rx/STM32L4Sx devices
    - Add new API HAL_MMC_ConfigSpeedBusOperation() to configure the speed bus
  - Correct BLOCKSIZE constant into MMC_BLOCKSIZE in HAL_MMCEx_ConfigDMAMultiBuffer() API
  - Implement DDR mode and high speed feature, applicable only to STM32L4P5xx/STM32L4Q5xx and STM32L4Rx/STM32L4Sx devices
  - eMMC card size computation issue correction
  - Multi-block write issue correction
- HAL OCTOSPI driver
  - Add OCTOSPI_DCR4_REFRESH register management for STM32L4P5xx/STM32L4Q5xx devices
- HAL PCD driver
  - Update PCD_EP_ISR_Handler() API to re-enable EP OUT before copying data from IP buffer PMA to SRAM in order to improve data throughput
- HAL PKA driver (NEW)
  - New stm32l4xx_hal_pka.h, stm32l4xx_hal_pka.c files (driver enabled with HAL_PKA_MODULE_ENABLED in stm32l4xx_hal_conf.h file)
- HAL PSSI driver (NEW)
  - New stm32l4xx_hal_pssi.h, stm32l4xx_hal_pssi.c files (driver enabled with HAL_PSSI_MODULE_ENABLED in stm32l4xx_hal_conf.h file)
- HAL PWR driver
  - Add new API HAL_PWREx_SetSRAM2ContentRetention() offering finer SRAM2 area retention in Standby mode for STM32L4P5xx/L4Q5xx devices (no retention, full retention or 4 Kbytes retention only) compared with other STM32L4 devices (no retention or full retention only)
- HAL RCC driver
  - Add PSSI peripheral related macros
    - __HAL_RCC_PSSI_CLK_ENABLE()
    - __HAL_RCC_PSSI_CLK_DISABLE()
    - __HAL_RCC_PSSI_IS_CLK_ENABLED()
    - __HAL_RCC_PSSI_IS_CLK_DISABLED()
    - __HAL_RCC_PSSI_FORCE_RESET()
    - __HAL_RCC_PSSI_RELEASE_RESET()
    - __HAL_RCC_PSSI_CLK_SLEEP_ENABLE()
    - __HAL_RCC_PSSI_CLK_SLEEP_DISABLE()
    - __HAL_RCC_PSSI_IS_CLK_SLEEP_ENABLED()
    - __HAL_RCC_PSSI_IS_CLK_SLEEP_DISABLED()
  - Add HAL_RCCEx_OCTOSPIDelayConfig() API to manage RCC_DLYCFGR register to configure OCTOSPI instances DQS delays. Applicable only to STM32L4P5xx/STM32L4Q5xx and STM32L4Rx/STM32L4Sx devices.
  - Correct HAL_RCC_OscConfig() API
    - to make sure Flash latency is decreased only when MSI is the system clock source
    - to ensure the PLL source is not updated when already used as PLLSAI(s) clock source
  - Add the following macros to test whether or not OctoSPI clocks are enabled
    - __HAL_RCC_OSPI1_IS_CLK_ENABLED()
    - __HAL_RCC_OSPI2_IS_CLK_ENABLED()
    - __HAL_RCC_OSPI1_IS_CLK_DISABLED()
    - __HAL_RCC_OSPI2_IS_CLK_DISABLED()
  - Correct MISRA C:2012-Rule-21.1 warning in updating the defines created to prevent recursive inclusion in stm32l4xx_hal_rcc.h and stm32l4xx_hal_rcc_ex.h
- HAL RNG driver
  - Deliver new APIs HAL_RNGEx_SetConfig(), HAL_RNGEx_GetConfig() and HAL_RNGEx_LockConfig() to open entropy configuration for new hardware peripheral version available on STM32L4P5xx/L4Q5xx APIs declared and defined in new files stm32l4xx_hal_rng_ex.h and stm32l4xx_hal_rng_ex.c
  - Update HAL_RNG_GenerateRandomNumber() and HAL_RNG_ReadyDataCallback() APIs comments to reflect the peripheral behavior when output random data are available in an output buffer
  - Correct seed or clock error setting in HAL_RNG_IRQHandler() API
  - Align all defines related to NISTN bit to new NISTC naming. Applicable only to STM32L4P5xx/STM32L4Q5xx devices.
- HAL RTC driver
  - Correct tamper management in HAL_RTCEx_SetTamper() and HAL_RTCEx_SetTamper_IT() APIs to allow individual configuration of the fields Interrupt Enable IE, NOERASE and Mask Flag MF for each tamper channel
  - Correct HAL_RTC_SetAlarm_IT() API so that alarm can be set without having to be deactivated beforehand
  - Remove redundant condition from HAL_RTC_Init() to correct CodeSonar warning
  - Implement binary mode feature specific to STM32L4P5xx/STM32L4Q5xx devices
    - Add new field BinaryAutoClr in RTC_AlarmTypeDef structure
    - Add new fields BinMode and BinMixBcdU in RTC_InitTypeDef structure
  - Implement sub-second register underflow feature specific to STM32L4P5xx/STM32L4Q5xx devices
    - Create new APIs
      - HAL_RTCEx_SetSSRU_IT()
      - HAL_RTCEx_DeactivateSSRU()
      - HAL_RTCEx_SSRUIRQHandler()
      - HAL_RTCEx_SSRUEventCallback()
- HAL SAI driver
  - Update code to remove tests on part numbers replaced on tests on SAI2 instance
  - Update the return check of HAL_DMA_Abort() in HAL_SAI_DMAStop() and HAL_SAI_Abort() APIs
- HAL TIM driver
  - Add TIM update interrupt flag remap constants definitions
    - TIM_UIFREMAP_DISABLE
    - TIM_UIFREMAP_ENABLE
  - Add TIM encoder input polarity constants definitions
    - TIM_INPUTCHANNELPOLARITY_RISING
    - TIM_INPUTCHANNELPOLARITY_FALLING
  - Add macros to force a continuous copy of the update interrupt flag (UIF) into the timer counter register (bit 31)
    - __HAL_TIM_UIFREMAP_ENABLE()
    - __HAL_TIM_UIFREMAP_DISABLE()
  - Add __HAL_TIM_GET_UIFCPY() macro to retrieve update interrupt flag (UIF) copy status
  - Add macros to manage fast mode for a given channel
    - __HAL_TIM_ENABLE_OCxFAST()
    - __HAL_TIM_DISABLE_OCxFAST()
- HAL UART driver
  - Add new APIs HAL_UART_ReceiverTimeout_Config(), HAL_UART_EnableReceiverTimeout() and HAL_UART_DisableReceiverTimeout() to update on the fly the receiver timeout value in RTOR register
  - Remove redundant condition on UART_CLOCKSOURCE_UNDEFINED in UART_SetConfig() API
  - Update HAL_UART_Transmit() and HAL_UART_Receive() functions to avoid deadlock problem while mixing polling Transmit and Receive requests
  - Update API description of HAL_UART_Transmit(), HAL_UART_Receive(), HAL_UART_Transmit_IT(), HAL_UART_Receive_IT(), HAL_UART_Transmit_DMA(), HAL_UART_Receive_DMA()
  - Correct MISRA C:2012-Rule-21.1 warning in updating the defines created to prevent recursive inclusion in stm32l4xx_hal_uart.h and stm32l4xx_hal_uart_ex.h
  - Correct MISRA C:2012-Rule-2.2_c warning in removing unnecessary initializations in stm32l4xx_hal_uart.c and stm32l4xx_hal_uart_ex.c
  - Correct MISRA C:2012-Rule-18.4 in HAL_UART_Transmit() and HAL_UART_Receive() APIs so that `+=’ operator is not applied to a pointer
  - Correct MISRA C:2012-Rule15.7 warning to remove all empty else clauses in stm32l4xx_hal_uart.c and stm32l4xx_hal_uart_ex.h
  - Correct MISRA C:2012-Rule-17.7 warning in all calls of HAL_DMA_Abort() API so that its return value is not discarded
  - Correct MISRA C:2012-Rule-13.5 for all tests with logical operators
  - Correct MISRA C:2012-Rule-18.1_x to ensure numerator[] and denominator[] arrays in static function UARTEx_SetNbDataToProcess() are not out of bounds
  - Correct MISRA C:2012-Rule-10.6 warning in suppressing implicit widening and unused value in UART_SetConfig() API in stm32l4xx_hal_uart.c
  - Correct MISRA C:2012-Rule-10.4_a warning in suppressing superfluous mask in HAL_UART_Receive() API in stm32l4xx_hal_uart.c
- HAL USART driver
  - Update USART_SetConfig() to remove functions as argument out of macros

LL drivers changes

- LL ADC driver
  - Add new macros to respectively set and remove internal channels from the ADC peripheral configuration
    - LL_ADC_SetCommonPathInternalChAdd()
    - LL_ADC_SetCommonPathInternalChRem()
- LL DMA driver
  - Define DMAMUX request constant LL_DMAMUX_REQ_PSSI in stm32l4xx_ll_dmamux.h to enable PSSI peripheral DMA transfers for STM32L4P5xx/STM32L4Q5xx devices
- LL FMC driver
  - Fix MS Visual 2017 compilation error in FMC_NORSRAM_Init() in removing the compilation switch from the macro definition
- LL PKA driver (NEW)
  - New stm32l4xx_ll_pka.h, stm32l4xx_ll_pka.c files
- LL PWR driver
  - Add new APIs LL_PWR_SetSRAM2ContentRetention() and LL_PWR_GetSRAM2ContentRetention() offering finer SRAM2 area retention in Standby mode for STM32L4P5xx/L4Q5xx devices (no retention, full retention or 4 Kbytes retention only) compared with other STM32L4 devices (no retention or full retention only)
- LL RNG driver
  - Align all defines and macros related to NISTN bit to new NISTC naming. Applicable only to STM32L4P5xx/STM32L4Q5xx devices.
- LL RCC driver
  - Add LL_RCC_OCTOSPI1_DelayConfig() and LL_RCC_OCTOSPI2_DelayConfig() API to manage RCC_DLYCFGR register to configure OCTOSPI instances DQS delays. Applicable only to STM32L4P5xx/STM32L4Q5xx and STM32L4Rx/STM32L4Sx devices.
  - Add LL_AHB2_GRP1_PERIPH_PKA constant definition in stm32l4xx_ll_bus.h for new PKA driver
- LL RTC driver
  - Implement binary mode feature specific to STM32L4P5xx/STM32L4Q5xx devices
    - Create new APIs for binary mode management
      - LL_RTC_SetBinaryMode()
      - LL_RTC_GetBinaryMode()
      - LL_RTC_SetBinMixBCDU()
      - LL_RTC_GetBinMixBCDU()
    - Create new APIS for binary mode autoclear
      - LL_RTC_ALMA_SetBinAutoClr()
      - LL_RTC_ALMA_GetBinAutoClr()
      - LL_RTC_ALMB_SetBinAutoClr()
      - LL_RTC_ALMB_GetBinAutoClr()
  - Implement sub-second register underflow feature specific to STM32L4P5xx/STM32L4Q5xx devices
    - Create new APIS
      - LL_RTC_IsActiveFlag_SSRU()
      - LL_RTC_ClearFlag_SSRU()
      - LL_RTC_IsActiveFlag_SSRUM()
      - LL_RTC_EnableIT_SSRU()
      - LL_RTC_DisableIT_SSRU()
      - LL_RTC_IsEnabledIT_SSRU()
  - Correct LL_RTC_SCR_ALRAF constant misspelling
- LL TIM driver
  - Add new macro LL_TIM_IsActiveUIFCPY() to indicate whether update interrupt flag (UIF) copy is set
- LL UART driver
  - Correct MISRA C:2012-Rule-21.1 warning in updating the defines created to prevent recursive inclusion in stm32l4xx_ll_uart.h
  - Correct MISRA C:2012-Rule-12.1 warning in adding parentheses around RXThreshold and TXThreshold in LL_LPUART_ConfigFIFOsThreshold() API
  - Correct comment on BBR check in stm32l4xx_ll_uart.c
  - Add mask in LL_LPUART_ReceiveData8() API in stm32l4xx_ll_uart.h to ensure proper cast operation
  - Ensure proper return value in LL_LPUART_GetBaudRate() API in stm32l4xx_ll_uart.h
- LL USART driver
  - Add mask in LL_USART_ReceiveData8() API in stm32l4xx_ll_usart.h to ensure proper cast operation
- LL USB driver
  - Correct USB_DeactivateEndpoint() and USB_DeactivateDedicatedEndpoint() APIs in stm32l4xx_ll_usb.c file to make sure the end point is disabled during deactivation
  - Correct local variable wEpRegVal type in USB_ActivateEndpoint() API

V1.10.0 / 03-April-2019

## Main Changes

- Delivery of the new HAL MMC driver

## Contents

HAL drivers changes

- HAL ADC driver
  - Ensure channel number is properly cast in uint32_t in LL_ADC_SetChannelSamplingTime() macro calls
  - Ensure offset parameter is properly cast in uint32_t in ADC_OFFSET_SHIFT_RESOLUTION() macro calls
  - Correct ADC_EXTERNALTRIG_T4_TRGO constant definition in stm32l4xx_hal_adc.h
  - Correct MISRA C:2012-Rule-2.4 warning in structure __ADC_HandleTypeDef definition
- HAL COMP driver
  - Correct MISRA C:2012 Rule-2.4 warning in structure __COMP_HandleTypeDef definition
- HAL CRC driver
  - Correct MISRA C:2012 Rule-21.1 warning in removing underscores at the beginning of the defines set to prevent recursive inclusion
- HAL CRYP driver
  - In HAL_CRYPEx_Read_SuspendRegisters() API, ensure that check of AES_SR_BUSY flag before processing suspension is done only in GCM mode
- HAL DAC driver
  - Correct HAL_DAC_Start() in SW trigger mode for STM32L4Rx/STM32L4Sx products
  - Fix callback identifiers enum values
- HAL DFSDM driver
  - Correct MISRA C:2012 Rule-2.4 warning in structures __DFSDM_Channel_HandleTypeDef and __DFSDM_Filter_HandleTypeDef definitions
- HAL DMA driver
  - Correct HAL_DMA_Abort() to add check of HAL_DMA_STATE_BUSY state
- HAL DSI driver
  - Correct MISRA C:2012 Rule-18.3 and Rule-2.4 warning in structure __DSI_HandleTypeDef definition
  - Correct HAL_DSI_ShortWrite() and HAL_DSI_Read to fix lock issue
  - Correct HAL_DSI_Read() to be able to read more than two parameters
- HAL FLASH driver
  - Correct the address of PCROP area management in FLASH_OB_GetPCROP() API to include the last double-word
  - Correct IS_OB_USER_TYPE() macro to include nBoot0 and nSwBoot0 for STM32L496xx/L4A6xx devices
  - Correct FLASH_SIZE constant definition when 0x1FFF75E0 address content is undefined
  - Correct FLASH_Program_Fast() to ensure Interrupt mask is not lost during Fast Programming sequence
  - Update FLASH_Program_DoubleWord() to ensure programming is performed in 2 steps, in the right order, independently of compiler optimizations
  - Correct MISRA C:2012 Rule-8.5_b related to multiple declarations of externally-linked object
- HAL GENERIC driver
  - Correct HAL_SYSCFG_EnableMemorySwappingBank() API for proper memory swapping
  - Update stm32l4xx_hal_conf_template.h to add HAL_EXTI_MODULE_ENABLED following HAL EXTI creation in V1.9.0
  - Update stm32l4xx_hal_conf_template.h to add HAL_MMC_MODULE_ENABLED following HAL MMC creation
- HAL GFXMMU driver
  - Correct MISRA C:2012 Rule-2.4 warning in structure __GFXMMU_HandleTypeDef definition
- HAL GPIO driver
  - Enhance reentrancy robustness for HAL_GPIO_TogglePin() API
  - Update the external interrupt or event clear operation in HAL_GPIO_DeInit()API
  - Add comment in HAL_GPIO_LockPin() API to justify an unused read of a register
  - Correct IAR v8.30.1 warning in IS_GPIO_PIN_ACTION() macro
- HAL HASH driver
  - Add HAL_HASH_SHA1_Accumulate_IT(), HAL_HASH_MD5_Accumulate_IT(), HAL_HASHEx_SHA224_Accumulate_IT() and HAL_HASHEx_SHA256_Accumulate_IT() manage multi-buffer messages in interrupt mode.
  - Correct HASH handle state management in DMA transfer mode
  - Add comments to describe case of messages made of several parts, not all with length multiple of 4 bytes
  - Fix comments in HAL_HASH_DMAFeed_ProcessSuspend()
- HAL HCD driver
  - Rework usb modules define protection
  - Correct MISRA C:2012 Rule-21.1 warning in removing underscores at the beginning of the defines set to prevent recursive inclusion
  - Correct CodeSonar warning in HAL_HCD_Init()
  - Update HAL_HCD_HC_Init() in order to not expose HCD high speed in case hardware supports only FS mode
- HAL IRDA driver
  - Correct IAR v8.30.1 warning in IRDA_GETCLOCKSOURCE() macro and IRDA_SetConfig() static function
- HAL IWDG driver
  - Correct MISRA C:2012 Rule-21.1 warning in removing underscores at the beginning of the defines set to prevent recursive inclusion
  - Correct __IWDG_HandleTypeDef structure definition in stm32l4xx_hal_iwdg.h
- HAL LPTIM driver
  - Correct __HAL_LPTIM_REPETITIONCOUNTER_GET() macro parameter description
  - Correct LPTIM_Disable() so that __HAL_RCC_LPTIM1_CONFIG uses RCC constants instead of 0UL value
- HAL LTDC driver
  - Correct MISRA C:2012 Rule-2.4 issue
- HAL MMC driver (NEW)
  - New stm32l4xx_hal_mmc.h, stm32l4xx_hal_mmc.c, stm32l4xx_hal_mmc_ex.h, stm32l4xx_hal_mmc_ex.c files (driver enabled with HAL_MMC_MODULE_ENABLED in stm32l4xx_hal_conf.h file)
- HAL OCTOSPI driver
  - Correct MISRA C:2012 Rule-5.4_c99 warning in stm32l4xx_hal_ospi.h
- HAL OPAMP driver
  - Fix callback identifiers enum values
- HAL PCD driver
  - Rework usb modules define protection
  - Correct mask to clear USB RX number of blocks
  - Correct cast used in HAL_PCD_EP_GetRxCount() API
  - Clear status phase received interrupt in HAL_PCD_IRQHandler() API
  - Correct MISRA C:2012 Rule-21.1 warning in removing underscores at the beginning of the defines set to prevent recursive inclusion
  - Correct MISRA C:2012 Rule-8.3_b, Rule-8.3_b and Rule-2.3 warnings
  - Update error handling management in HAL_PCD_Init() and HAL_PCD_Stop()
  - Correct PCD_WriteEmptyTxFifo() to handle transfer size equal to FIFO length
  - Correct maximum of EP number according to the allocated buffers on hpcd structure
  - Correct timing setting for BCD
  - Correct HCD_HC_OUT_IRQHandler() to ensure correct toggle for output interrupt during transfer complete
  - Correct USB interrupt handler to handle EP0 OUT transfers in USB DMA mode
  - Ensure proper management of the BCD feature for OTG instance
  - Remove PCD_GET_DB_DIR() macro
  - Prevent enabling USB DMA for OTG FS instance
  - Update PCD_EP_ISR_Handler() to prevent reading from PMA to NULL pointer addr
  - Correct ep table size for device only IP
  - Fix USB exti wakeup macros
  - Correct HAL_PCD_IRQHandler() to ensure correct OTG core speed usage
  - Correct CodeSonar warning in HAL_PCD_Init()
- HAL PWR driver
  - Correct PWR_CR3 bit name EN_ULP into ENULP
- HAL QSPI driver
  - Correct MISRA C:2012 Rule-2.4 warning in structure __QSPI_HandleTypeDef definition
  - Remove the compilation switches related to QUADSPI1 and QUADSPI2 as all STM32 families have only one instance called QUADSPI
  - Fix HAL_QSPI_TIMEOUT_DEFAULT_VALUE misspelling
- HAL RCC driver
  - Correct HAL_RCCEx_GetPeriphCLKFreq() to LSIPREDIV bit is taken into account when reporting LSI-clocked peripheral frequency
  - Update HAL_RCC_OscConfig() to not report an error if same PLL configuration is requested
  - Correct __HAL_RCC_PLLxx_CONFIG() macros to preserve output clock(s) enable state
  - Correct HAL_RCC_GetSysClockFreq() to prevent rounding errors
- HAL RTC driver
  - Correct HAL_RTCEx_SetWakeUpTimer_IT() to ensure __HAL_RTC_WAKEUPTIMER_EXTI_ENABLE_IT() is called upon an interruption
  - Remove use of ALRBWF and ALRAWF bits
  - Correct cast setting of BYPSHAD bit in HAL_RTCEx_EnableBypassShadow() API
  - Rename RTC_IT_MASK into RTC_FLAG_MASK
  - Add management of INITF flag rising occurrence too early when entering init mode
  - Correct WUTWF flag management in HAL_RTCEx_SetWakeUpTimer() API
  - ensure HAL RCC doesn’t overwrite Tick priority
- HAL SAI driver
  - Add calls of registered callbacks in HAL_SAI_IRQHandler() API
- HAL SD driver
  - Correct MISRA C:2012 Rule-10.4a and Rule-10.5 warnings
  - Correct pointer dereferencing in HAL_SD_ReadBlocks() and HAL_SD_WriteBlocks() APIs
  - Correct gcc warning in HAL_SD_Init() API
- HAL SMARTCARD driver
  - Correct IAR v8.30.1 warnings related to GTPR register writing
  - Declare ErrorCode field of __SMARTCARD_HandleTypeDef structure as volatile
  - Correct MISRA C:2012 Rule-13.5 warnings in HAL_SMARTCARD_IRQHandler() API
- HAL SPI driver
  - Correct SPI communication abort procedure in HAL_SPI_Abort() API
  - Correct comments in SPI_AbortRx_ISR()
  - Correct MISRA C:2012 Rule-10.3 warnings
- HAL SWPMI driver
  - Correct MISRA C:2012 Rule-2.4 warning in structure __SWPMI_HandleTypeDef definition
- HAL TIM driver
  - Correct all MISRA C:2012 warnings
  - Add XferHalfCpltCallback interrupt callback
  - Update HAL_TIMEx_ConfigCommutationEvent() to disable IT and DMA
  - Update comments to stress ClearInputPrescaler value must be 0 when clearing the OCxREF signal on an external event
  - Ensure external clock mode 2 is not selected in encoder mode
  - Ensure gated mode is not used if TI1F_ED is selected as the trigger input
  - Update the list of DMABurst related constants to match the capabilities of the Timer instances supported by the devices of the family
- HAL TSC driver
  - Correct all MISRA C:2012 warnings
  - Correct __HAL_TSC_GET_GROUP_STATUS() macro definition
- HAL USART driver
  - Update USART_RxISR_8BIT(), USART_RxISR_16BIT(), USART_RxISR_8BIT_FIFOEN() and USART_RxISR_16BIT_FIFOEN() to ensure TXFT interrupt is handled in all cases

LL drivers changes

- LL ADC driver
  - Correct potential infinite wait in while loop of LL_ADC_DeInit()
  - Redefinition of memory-mapped peripheral registers address into volatile (_IO)
  - Correct LL_ADC_INJ_ConfigQueueContext() so that default edge is not included by default into trigger value
- LL CRC driver
  - Add comment to report derogation to Misra C:2012 R.11.5 rule in API LL_CRC_FeedData16()
- LL DMA2D driver
  - Correct all MISRA C:2012 warnings
- LL GPIO driver
  - Enhance reentrancy robustness for HAL_GPIO_TogglePin() API
  - Update the external interrupt or event clear operation in HAL_GPIO_DeInit() API
  - Add comment in LL_GPIO_LockPin() API to justify an unused read of a register
- LL LPTIM driver
  - Correct LL_LPTIM_Init() not returns an error status while LPTIM is disabled
- LL OPAMP driver
  - Correct MISRA C:2012 Rule-2.7 and Rule-8.13 warnings
- LL PWR driver
  - Correct PWR_CR3 bit name EN_ULP into ENULP
  - Change compilation switch to trigger LL_PWR_EnableVddUSB(), LL_PWR_DisableVddUSB() and LL_PWR_IsEnabledVddUSB() APIs definition
  - Redefinition of memory-mapped peripheral registers address into volatile (_IO)
- LL RCC driver
  - Correct LL_RCC_GetLPTIMClockFreq() to LSIPREDIV bit is taken into account when reporting LSI-clocked peripheral frequency
  - Update LL_RCC_DeInit() to be fully operational when compiled with gcc -O3
- LL RTC driver
  - Remove use of ALRBWF and ALRAWF bits
  - Correct month management in LL_RTC_DATE_Init() API and IS_LL_RTC_MONTH() macro
- LL SWPMI driver
  - Correct return value for LL_SWPMI_ClearFlag_RDY(), LL_SWPMI_EnableIT_RDY() and LL_SWPMI_DisableIT_RDY() APIs
- LL TIM driver
  - Redefinition of memory-mapped peripheral registers address into volatile (_IO)
  - Correct LL_TIM_OC_(Get/Set)CompareCH5 and LL_TIM_SetCH5CombinedChannels
- LL USART driver
  - Correct all MISRA C:2012 warnings
  - Correct LL_USART_ReceiveData8() to ensure proper cast value
- LL USB driver
  - Rework usb modules define protection
  - Correct USB Vbus sensing
  - Correct MISRA C:2012 Rule-21.1 warning in removing underscores at the beginning of the defines set to prevent recursive inclusion
  - Correct MISRA C:2012 Rule-8.3_b, Rule-8.3_b and Rule-2.3 warnings
  - Update error handling management in LL APIs
  - Correct maximum of EP number according to the allocated buffers on hpcd structure
  - Improve USB_HostInit() to manage device low speed mode
  - Correct USB_CoreInit() to ensure proper management of the BCD feature for OTG instance
  - Correct USB_EPClearStall() to manage TX EP state during ep clear stall
  - Correct ep table size for device only IP
  - Correct USB_EP0StartXfer() and USB_EPStartXfer() to prevent enabling TX fifo IT before endpoint enable
  - Ensure correct OTG core speed usage

V1.9.0 / 27-July-2018

## Main Changes

- Release of HAL and Low Layer drivers to add support of STM32L412xx/STM32L422xx
- Superset features device STM32L422xx API User Manual available (STM32L422xx_User_Manual.chm)
- MISRA C:2012 corrections

## Contents

HAL drivers changes

MISRA C:2012 corrections listed hereafter are applicable to LL driver as well.

- HAL ADC driver

  - Replace private macro using concurrent volatile access (generating MIRSA errors) by temporary variables or LL helper macro
  - Correct MISRA C:2012 warnings reported by rules 2.2_c, 8.13, 10.1_R2, 10.1_R3, 10.1_R6, 10.4_a, 10.4_b, 10.5, 14.4_c, 12.2, 15.7
  - stm32l4xx_hal_adc.c and stm32l4xx_hal_adc_ex.c
    - Change of time-out duration computation when expressed in microseconds to manage low system clock frequencies
  - stm32l4xx_hal_adc.c
    - Remove useless stabilization delay in ADC_Enable() when enabling ADC
    - In HAL_ADC_Stop_DMA(), HAL_DMA_Abort() API is called only if DMA is busy
  - stm32l4xx_hal_adc.h
    - Typo correction in ADC_AnalogWDGConfTypeDef FilteringConfig field description
  - stm32l4xx_hal_adc.c, stm32l4xx_hal_adc.h
    - Clarify comments in HAL_ADC_AnalogWDGConfig for analog watchdog thresholds checks when oversampling is enabled
- HAL CAN driver
  - Correct MISRA C:2012 warnings reported by rules 2.2_c, 10.3, 10.4_a, 10.6, 12.2, 13.3, 13.5, 15.7, 17.7, 18.1_b
  - stm32l4xx_hal_can.c, stm32l4xx_hal_can.h
    - Tx abort procedure correction
  - stm32l4xx_hal_can.c
    - Correct implementation of test on pending message in HAL_CAN_IsTxMessagePending()
    - Update HAL_CAN_Stop() to reset any previous sleep mode request to avoid maintaining the sleep mode request active at next HAL_CAN_Start()
- HAL COMP driver
  - Correct MISRA C:2012 warnings reported by rules 10.1, 10.3, 10.4, 13.5
  - stm32l4xx_hal_comp.c
    - Change of time-out duration computation when expressed in microseconds to manage low system clock frequencies
- HAL CRC driver
  - Correct MISRA C:2012 warnings reported by rules 10.3, 12.1, 12.2
- HAL CRYP driver
  - Correct MISRA C:2012 warnings reported by rules 2.2_c, 8.13, 10.3, 10.4, 10.6, 10.7, 10.8, 12.1, 13.5, 15.7, 17.7, 18.4
  - stm32l4xx_hal_cryp_ex.c: CodeSonar warning correction
- HAL DAC driver
  - Correct MISRA C:2012warnings
- HAL DCMI driver
  - Correct MISRA C:2012 warnings reported by rules 2.2_c, 8.4, 10.4_a, 12.1, 17.7, 18.4
- HAL DMA driver
  - Correct MISRA C:2012 warnings
- HAL DSI driver
  - stm32l4xx_hal_dsi.h: add __HAL_DSI_RESET_HANDLE_STATE() macro
- HAL EXTI driver (NEW)
  - New stm32l4xx_hal_exti.h and stm32l4xx_hal_exti.c files (driver enabled with HAL_EXTI_MODULE_ENABLED in stm32l4xx_hal_conf.h file)
- HAL FIREWALL driver
  - Correct MISRA C:2012 warnings reported by rules 10.4
- HAL GPIO driver
  - Correct MISRA C:2012 warnings reported by rules 10.3, 21.1
- HAL HASH driver
  - Correct MISRA C:2012 warnings reported by rules 1.3_k, 2.2_c, 9.1_f, 10.3, 12.1, 13.4_b, 13.5, 15.7, 17.7, 21.1
  - stm32l4xx_hal_hash.c:
    - in HASH_Start_DMA(), test on HASH_CR_MDMAT bit before checking input buffer length in case of multi-buffer processing
    - Fill-up empty statement in HAL_HASH_DMAFeed_ProcessSuspend() to correct CodeSonar warning
- HAL I2C driver
  - Correct MISRA C:2012 warnings
  - stm32l4xx_hal_i2c.c: remove extra definition of I2C_GET_DMA_REMAIN_DATA() macro
- HAL IRDA driver
  - Correct MISRA C:2012 warnings reported by rules 2.1, 2.2_c, 2.4, 2.3, 8.9_a, 10.3, 10.4_a, 10.5, 10.6, 10.7, 11.3, 13.3, 13.5, 15.7, 17.7, 17.8, 18.4, 21.1
- HAL IWDG driver
  - Correct MISRA C:2012 warnings reported by rules 2.7, 10.3, 10.4_a
- HAL LPTIM driver
  - Add repetition counter management for STM32L412xx/L422xx devices
  - New field RepetitionCounter added in LPTIM_InitTypeDef structure
- HAL OSPI driver
  - stm32l4xx_hal_ospi.h: update memory type definition to support new octal PSRAM from APMemory
- HAL OPAMP driver
  - Correct MISRA C:2012 warnings

- HAL PWR driver

  - Update conversion mechanism from duration in us in number of cycles to manage low system frequencies
  - Correct MISRA C:2012 warnings reported by rules 2.2_c, 10.3, 10.4_a, 13.5, 16.3, 17.7

- HAL RCC driver

  - stm32l4xx_hal_rcc.c, stm32l4xx_hal_rcc.h: compilation switches update to ensure full STM32L412xx/L422xx devices support
  - Correct MISRA C:2012 warnings reported by rules 2.2_c, 8.13, 8.9_a, 10.1_R2, 10.4_a, 10.3, 10.7, 11.9, 12.1, 12.2, 13.5, 14.4_c, 15.7, 21.2

- HAL RTC driver

  - New HAL_RTCEx_SetLowPowerCalib() API for STM32L412xx/L422xx devices
  - HAL_RTC_AlarmIRQHandler() API optimization

- HAL SAI driver

  - stm32l4xx_hal_sai.c: remove empty if statements to fix CodeSonar warning
  - stm32l4xx_hal_sai.h, stm32l4xx_hal_sai.c: add check on master clock divider parameter, remove SAI_FIFO_SIZE definition

- HAL SMARTCARD driver

  - Correct MISRA C:2012 warnings reported by rules 2.2_c, 8.9_a, 10.3, 10.4_a, 10.5, 10.6, 10.7, 12.1, 12.2, 13.3, 13.5, 15.7, 17.7, 17.8, 18.1, 21.1

- HAL SPI driver

  - Correct MISRA C:2012 warnings

- HAL SWPMI driver

  - Correct MISRA C:2012 warnings reported by rules 2.2_c, 2.7, 10.3, 10.4_a, 13.3, 13.5, 15.7, 17.7, 17.8, 21.1

- HAL TSC driver

  - Correct MISRA C:2012 warnings reported by rule 21.1

- HAL USART driver

  - Correct MISRA C:2012 warnings reported by rule 10.4_a, 10.6, 12.2

LL Drivers changes

- LL ADC driver

  - stm32l4xx_ll_dmamux.h: clarify comments when oversampling is enabled

- LL DMA driver

  - stm32l4xx_ll_dmamux.h: remove test on DMAMUX1

- LL RCC driver

  - stm32l4xx_ll_rcc.c,stm32l4xx_ll_rcc.h: compilation switches update to ensure full STM32L412xx/L422xx devices support

- LL RTC driver

  - stm32l4xx_ll_rtc.h: add new macros LL_RTC_WAKEUP_SetAutoClr(), LL_RTC_WAKEUP_GetAutoClr() applicable to STM32L412xx/L422xx devices only

V1.8.3 / 22-May-2018

## Main Changes

Maintenance Release of HAL and Low Layer drivers

Add support of HAL callback registration feature

- The feature disabled by default is available for the following HAL drivers:

- ADC, CAN, COMP, CRYP, DAC, DCMI, DFSDM, DMA2D, DSI, GFXMMU, HASH, HCD, I2C, IRDA, LPTIM, LTDC, OPAMP, OSPI, PCD, QSPI, RNG, RTC, SAI, SD, SMARTCARD, SMBUS, SPI, SWPMI, TIM, TSC, UART, USART and WWDG

- The feature may be enabled individually per HAL PPP driver by setting the corresponding definition USE_HAL_PPP_REGISTER_CALLBACKS to 1U in stm32l4xx_hal_conf.h project configuration file (template file stm32l4xx_hal_conf_template.h available from Drivers/STM32L4xx_HAL_Driver/Inc)

- Once enabled, the user application may resort to HAL_PPP_RegisterCallback() to register specific callback function(s) and unregister it(them) with HAL_PPP_UnRegisterCallback().

MISRA C:2012 corrections

## Contents

HAL drivers changes

- HAL generic driver

  - stm32l4xx_hal_conf_template.h update to add callback registration feature support (disabled by default)
  - stm32l4xx_hal_def.h: UNUSED() macro update for g++ compilation

- HAL ADC driver

  - Fix to enable ADC internal channels (VrefInt, temperature sensor and Vbat) without being too restrictive

  - Update internal ADC calibration timeout value

  - Add callback registration feature

    - Add HAL_ADC_RegisterCallback() and HAL_ADC_UnRegisterCallback() APIs
    - Add callback identifiers in HAL_ADC_CallbackIDTypeDef enumerated typedef

- HAL CAN driver

  - Add callback registration feature

    - Add HAL_CAN_RegisterCallback() and HAL_CAN_UnRegisterCallback() APIs
    - Add callback identifiers in HAL_CAN_CallbackIDTypeDef enumerated typedef

- HAL COMP driver

  - Add callback registration feature
    - Add HAL_COMP_RegisterCallback() and HAL_COMP_UnRegisterCallback APIs
    - Add callback identifiers in HAL_COMP_CallbackIDTypeDef enumerated typedef

- HAL CRYP driver

  - Add callback registration feature

    - Add HAL_CRYP_RegisterCallback() and HAL_CRYP_UnRegisterCallback APIs
    - Add callback identifiers in HAL_CRYP_CallbackIDTypeDef enumerated typedef

- HAL DAC driver

  - Add callback registration feature

    - Add HAL_DAC_RegisterCallback() and HAL_DAC_UnRegisterCallback APIs
    - Add callback identifiers in HAL_DAC_CallbackIDTypeDef enumerated typedef

- HAL DCMI driver

  - Add callback registration feature

    - Add HAL_DCMI_RegisterCallback() and HAL_DCMI_UnRegisterCallback APIs
    - Add callback identifiers in HAL_DCMI_CallbackIDTypeDef enumerated typedef

- HAL DFSDM driver

  - Add callback registration feature

    - Add HAL_DFSDM_Channel_RegisterCallback(), HAL_DFSDM_Channel_UnRegisterCallback(), HAL_DFSDM_Filter_RegisterCallback(), HAL_DFSDM_Filter_UnRegisterCallback(), HAL_DFSDM_Filter_RegisterAwdCallback() and HAL_DFSDM_Filter_UnRegisterAwdCallback APIs
    - Add callback identifiers in HAL_DFSDM_Channel_CallbackIDTypeDef and HAL_DFSDM_Filter_CallbackIDTypeDef enumerated typedef

- HAL DM2D driver

  - Add callback registration feature

    - Add HAL_DMA2D_RegisterCallback() and HAL_DMA2D_UnRegisterCallback APIs
    - Add callback identifiers in HAL_DMA2D_CallbackIDTypeDef enumerated typedef

- HAL DSI driver

  - Add callback registration feature

    - Add HAL_DSI_RegisterCallback() and HAL_DSI_UnRegisterCallback APIs
    - Add callback identifiers in HAL_DSI_CallbackIDTypeDef enumerated typedef

- HAL GFXMMU driver

  - Add callback registration feature

    - Add HAL_GFXMMU_RegisterCallback() and HAL_GFXMMU_UnRegisterCallback APIs
    - Add callback identifiers in HAL_GFXMMU_CallbackIDTypeDef enumerated typedef

- HAL HASH driver

  - Add callback registration feature

    - Add HAL_HASH_RegisterCallback() and HAL_HASH_UnRegisterCallback APIs
    - Add callback identifiers in HAL_HASH_CallbackIDTypeDef enumerated typedef

- HAL HCD driver

  - Add new user notification callbacks

    - HAL_HCD_PortEnabled_Callback() and HAL_HCD_PortDisabled_Callback()

  - Add callback registration feature

    - Add HAL_HCD_RegisterCallback(), HAL_HCD_UnRegisterCallback(), HAL_HCD_RegisterHC_NotifyURBChangeCallback() and HAL_HCD_UnRegisterHC_NotifyURBChangeCallback APIs
    - Add callback identifiers in HAL_HCD_CallbackIDTypeDef enumerated typedef

- HAL I2C driver

  - I2C slave enhancement when master sends RESTART instead of STOP

    - Add HAL_I2C_Master_Sequential_Transmit_DMA(), HAL_I2C_Master_Sequential_Receive_DMA(), HAL_I2C_Slave_Sequential_Transmit_DMA() and HAL_I2C_Slave_Sequential_Receive_DMA() APIs

  - Add callback registration feature

    - Add HAL_I2C_RegisterCallback(), HAL_I2C_UnRegisterCallback(), HAL_I2C_RegisterAddrCallback() and HAL_I2C_UnRegisterAddrCallback APIs
    - Add callback identifiers in HAL_I2C_CallbackIDTypeDef enumerated typedef

- HAL IRDA driver

  - Add callback registration feature

    - Add HAL_IRDA_RegisterCallback() and HAL_IRDA_UnRegisterCallback APIs
    - Add callback identifiers in HAL_IRDA_CallbackIDTypeDef enumerated typedef

- HAL LPTIM driver

  - Add callback registration feature

    - Add HAL_LPTIM_RegisterCallback() and HAL_LPTIM_UnRegisterCallback APIs
    - Add callback identifiers in HAL_LPTIM_CallbackIDTypeDef enumerated typedef

- HAL LTDC driver

  - Add callback registration feature

    - Add HAL_LTDC_RegisterCallback() and HAL_LTDC_UnRegisterCallback APIs
    - Add callback identifiers in HAL_LTDC_CallbackIDTypeDef enumerated typedef

- HAL NAND driver

  - Add new configuration API HAL_NAND_ConfigDevice()

  - Add new APIs for 8-bit and 16-bit accesses

    - HAL_NAND_Read_Page_8b(), HAL_NAND_Write_Page_8b(), HAL_NAND_Read_SpareArea_8b() and HAL_NAND_Write_SpareArea_8b()

    - HAL_NAND_Read_Page_16b(), HAL_NAND_Write_Page_16b(), HAL_NAND_Read_SpareArea_16b() and HAL_NAND_Write_SpareArea_16b()

- HAL OPAMP driver

  - Add callback registration feature

    - Add HAL_OPAMP_RegisterCallback() and HAL_OPAMP_UnRegisterCallback APIs
    - Add callback identifiers in HAL_OPAMP_CallbackIDTypeDef enumerated typedef

- HAL OSPI driver

  - Add callback registration feature

    - Add HAL_OSPI_RegisterCallback() and HAL_OSPI_UnRegisterCallback APIs
    - Add callback identifiers in HAL_OSPI_CallbackIDTypeDef enumerated typedef

- HAL PCD driver

  - Fix USB double buffer issue in PCD_SET_EP_DBUF1_CNT() macro

  - Add callback registration feature

    - Add HAL_PCD_RegisterCallback(),
      HAL_PCD_UnRegisterCallback(), HAL_PCD_RegisterDataOutStageCallback(), HAL_PCD_UnRegisterDataOutStageCallback(), HAL_PCD_RegisterDataInStageCallback(), HAL_PCD_UnRegisterDataInStageCallback(), HAL_PCD_RegisterIsoOutIncpltCallback(), HAL_PCD_UnRegisterIsoOutIncpltCallback(), HAL_PCD_RegisterIsoInIncpltCallback(), HAL_PCD_UnRegisterIsoInIncpltCallback(), HAL_PCD_RegisterBcdCallback(), HAL_PCD_UnRegisterBcdCallback(), HAL_PCD_RegisterLpmCallback() and HAL_PCD_UnRegisterLpmCallback APIs
    - Add callback identifiers in HAL_PCD_CallbackIDTypeDef enumerated typedef

- HAL QSPI driver

  - Fix HAL_QSPI_Receive_IT() to avoid early clear of TE and TC flags

  - Add callback registration feature

    - Add HAL_QSPI_RegisterCallback() and HAL_QSPI_UnRegisterCallback APIs
    - Add callback identifiers in HAL_QSPI_CallbackIDTypeDef enumerated typedef

- HAL RCC driver

  - Fix HAL_RCCEx_GetPeriphCLKFreq() for all peripheral clock frequency derivated from PLLSAI1 and PLLSAI2 when PLLSAI1M and PLLSAI2M dividers are present

- HAL RNG driver

  - Add callback registration feature

    - Add HAL_RNG_RegisterCallback(), HAL_RNG_UnRegisterCallback(), HAL_RNG_RegisterReadyDataCallback() and HAL_RNG_UnRegisterReadyDataCallback APIs
    - Add callback identifiers in HAL_RNG_CallbackIDTypeDef enumerated typedef

- HAL RTC driver

  - Add callback registration feature

    - Add HAL_RTC_RegisterCallback() and HAL_RTC_UnRegisterCallback APIs
    - Add callback identifiers in HAL_RTC_CallbackIDTypeDef enumerated typedef

- HAL SAI driver

  - Add callback registration feature

    - Add HAL_SAI_RegisterCallback() and HAL_SAI_UnRegisterCallback APIs
    - Add callback identifiers in HAL_SAI_CallbackIDTypeDef enumerated typedef

- HAL SMBUS driver

  - Add callback registration feature

    - Add HAL_SMBUS_RegisterCallback(), HAL_SMBUS_UnRegisterCallback(), HAL_SMBUS_RegisterAddrCallback() and HAL_SMBUS_UnRegisterAddrCallback APIs
    - Add callback identifiers in HAL_SMBUS_CallbackIDTypeDef enumerated typedef
- HAL SD driver
  - Fix DMA write issue
  - Fix to send the "Stop transfer" command only in case of multiple read or write operations

  - Fix typo in FileFormatGroup field of HAL_SD_CardCSDTypedef

  - Add callback registration feature

    - Add HAL_SD_RegisterCallback(), HAL_SD_UnRegisterCallback(), HAL_SD_RegisterTransceiverCallback() and HAL_SD_UnRegisterTransceiverCallback APIs
    - Add callback identifiers in HAL_SD_CallbackIDTypeDef enumerated typedef

- HAL SMARTCARD driver

  - Add callback registration feature

    - Add HAL_SMARTCARD_RegisterCallback() and HAL_SMARTCARD_UnRegisterCallback APIs
    - Add callback identifiers in HAL_SMARTCARD_CallbackIDTypeDef enumerated typedef

- HAL SPI driver

  - Add callback registration feature

    - Add HAL_SPI_RegisterCallback() and HAL_SPI_UnRegisterCallback APIs
    - Add callback identifiers in HAL_SPI_CallbackIDTypeDef enumerated typedef

- HAL SWPMI driver

  - Fix in HWL_SWPMI_EnableLoopback() to enable entering loopback mode after SWPMI initialization

  - Add callback registration feature

    - Add HAL_SWPMI_RegisterCallback() and HAL_SWPMI_UnRegisterCallback APIs
    - Add callback identifiers in HAL_SWPMI_CallbackIDTypeDef enumerated typedef

- HAL TIM driver

  - Add callback registration feature

    - Add HAL_TIM_RegisterCallback() and HAL_TIM_UnRegisterCallback APIs
    - Add callback identifiers in HAL_TIM_CallbackIDTypeDef enumerated typedef

- HAL TSC driver

  - Add callback registration feature

    - Add HAL_TSC_RegisterCallback() and HAL_TSC_UnRegisterCallback APIs
    - Add callback identifiers in HAL_TSC_CallbackIDTypeDef enumerated typedef

- HAL UART driver

  - Add wakeup capability from Stop mode when clocked by LSE

    - Add HAL_UARTEx_EnableClockStopMode() and HAL_UARTEx_DisableClockStopMode APIs

  - Remove the following APIs since only applicable to HAL USART and not HAL UART

  - HAL_UARTEx_EnableSlaveMode(), HAL_UARTEx_DisableSlaveMode() and HAL_UARTEx_ConfigNSS()

  - Add callback registration feature

    - Add HAL_UART_RegisterCallback() and HAL_UART_UnRegisterCallback APIs
    - Add callback identifiers in HAL_UART_CallbackIDTypeDef enumerated typedef

- HAL USART driver

  - Add callback registration feature

    - Add HAL_USART_RegisterCallback() and HAL_USART_UnRegisterCallback APIs
    - Add callback identifiers in HAL_USART_CallbackIDTypeDef enumerated typedef

- HAL WWDG driver

  - Add callback registration feature

    - Add HAL_WWDG_RegisterCallback() and HAL_WWDG_UnRegisterCallback APIs
    - Add callback identifiers in HAL_WWDG_CallbackIDTypeDef enumerated typedef

LL drivers changes

- LL ADC driver

  - Fix temperature sensor calibration factor value for STM32L4 devices other than STM32L47x/L48x

- LL LPUART driver

  - Add wakeup capability from Stop mode when clocked by LSE

    - Add LL_LPUART_EnableClockInStopMode(), LL_LPUART_DisableClockInStopMode() and LL_LPUART_IsClockEnabledInStopMode APIs

- LL RTC driver

  - Code optimization done in LL_RTC_TIME_GetHour(), LL_RTC_TIME_GetMinute(), LL_RTC_TIME_GetSecond(), LL_RTC_DATE_GetYear(), LL_RTC_DATE_GetMonth(), LL_RTC_DATE_GetDay(), LL_RTC_ALMA_GetDay(), LL_RTC_ALMA_GetHour(), LL_RTC_ALMA_GetMinute(), LL_RTC_ALMA_GetSecond(), LL_RTC_ALMB_GetDay(), LL_RTC_ALMB_GetHour(), LL_RTC_ALMB_GetMinute() and LL_RTC_ALMB_GetSecond APIs

- LL SPI driver

  - Fix GCC warnings in LL_SPI_TransmitData8() and LL_SPI_TransmitData16()

- LL USART driver

  - Rename LL_USART_ICR_NCF flag to LL_USART_ICR_NECF
  - Add wakeup capability from Stop mode when clocked by LSE
    - Add LL_USART_EnableClockInStopMode(), LL_USART_DisableClockInStopMode() and LL_USART_IsClockEnabledInStopMode APIs

V1.8.2 / 22-December-2017

## Main Changes

- Maintenance Release of HAL and Low Layer drivers

## Contents

HAL drivers changes

- HAL CAN driver

Rework of HAL CAN driver (compatibility break)

A new HAL CAN driver has been redesigned with new APIs, to bypass limitations on CAN Tx/Rx FIFO management present with previous HAL CAN driver version.

The new HAL CAN driver is the recommended version. It is located as usual in Drivers/STM32L4xx_HAL_Driver/Src and drivers/STM32L4xx_HAL_Driver/Inc folders. It can be enabled through switch HAL_CAN_MODULE_ENABLED in stm32l4xx_hal_conf.h

The legacy HAL CAN driver is also present in the release in drivers/STM32L4xx_HAL_Driver/Src/Legacy and drivers/STM32L4xx_HAL_Driver/Inc/Legacy folders for software compatibility reasons. Its usage is not recommended as deprecated. It can however be enabled through switch HAL_CAN_LEGACY_MODULE_ENABLED in stm32l4xx_hal_conf.h

Short migration guide:

Fields of CAN_InitTypeDef structure are renamed

- SJW to SyncJumpWidth, BS1 to TimeSeg1, BS2 to TimeSeg2, TTCM to TimeTriggeredMode, ABOM to AutoBusOff, AWUM to AutoWakeUp, NART to AutoRetransmission (inversed), RFLM to ReceiveFifoLocked and TXFP to TransmitFifoPriority

- HAL_CAN_Init() is split into both HAL_CAN_Init() and HAL_CAN_Start()
- HAL_CAN_Transmit() is replaced by HAL_CAN_AddTxMessage() to place Tx request, then HAL_CAN_GetTxMailboxesFreeLevel() for polling until completion
- HAL_CAN_Transmit_IT() is replaced by HAL_CAN_ActivateNotification() to enable transmission with interrupt mode, then HAL_CAN_AddTxMessage() to place Tx request
- HAL_CAN_Receive() is replaced by HAL_CAN_GetRxFifoFillLevel() for polling until reception, then HAL_CAN_GetRxMessage() to get Rx message
- HAL_CAN_Receive_IT() is replaced by HAL_CAN_ActivateNotification() to enable reception with interrupt mode, then HAL_CAN_GetRxMessage() in the receive callback to get Rx message
- HAL_CAN_Sleep() is renamed to HAL_CAN_RequestSleep()
- HAL_CAN_TxCpltCallback() is split into HAL_CAN_TxMailbox0CompleteCallback(), HAL_CAN_TxMailbox1CompleteCallback() and HAL_CAN_TxMailbox2CompleteCallback()

- HAL_CAN_RxCpltCallback() is split into HAL_CAN_RxFifo0MsgPendingCallback() and HAL_CAN_RxFifo1MsgPendingCallback()

More complete "how to use the new driver" is detailed in the driver header section itself.

- HAL CORTEX driver

  - HAL_MPU_Enable() and HAL_MPU_Disable() functions moved to stm32l4xx_hal_cortex.c

- HAL CRC driver

  - Fix GCC warning

- HAL FLASH driver

  - HAL_FLASH_Unlock() updated to not return HAL_ERROR if flash is already unlocked

- HAL OSPI driver

  - Cleanup IO Manager ports

- HAL RCC driver

  - RCC_RTCCLKSOURCE_NO_CLK enamed to RCC_RTCCLKSOURCE_NONE

  - HAL_RCC_DeInit() updates

    - Clear of status flags
    - Wait for PLLs disable flags to clear PLLs configuration registers

  - Fix MISRA C-2004 rule 10.6 ('U' suffix)

- HAL TIM driver

  - Fix MISRA C-2004 rule 10.6 ('U' suffix)

LL drivers changes

- LL CRC driver

  - Fix GCC warning

- LL RCC driver

  - Add LL_RCC_PLL_SetMainSource() and LL_RCC_HSI_IsEnabledInStopMode() APIs

  - LL_RCC_DeInit() update

    - Clear of status flags
    - Wait for PLLs disable flags to clear PLLs configuration registers

  - Fix IS_LL_RCC_I2C_CLKSOURCE() assert macro

V1.8.1 / 13-October-2017

## Main Changes

- Maintenance Release of HAL and Low Layer drivers

## Contents

HAL drivers changes

- HAL generic driver

  - Fix compilation issue with ARMCC --gnu option on __packed declaration in stm32l4xx_hal_def.h

- HAL ADC driver

  - Reuse LL ADC definitions
  - Fix MISRA C-2004 rule 19.10

- HAL DSI driver

  - Fix timing issue at highest optimization level on IAR on DSI Host, DSI Wrapper, DSI PLL and DSI regulator enable/disable macros
  - Add macro __HAL_DSI_RESET_HANDLE_STATE()

- HAL FLASH driver

  - HAL_FLASH_Unlock() shall not return an error when Flash already unlocked

- HAL I2C driver

  - Fix race condition in HAL_I2C_Master_Receive() and HAL_I2C_Slave_Receive()

- Fix RD_WRN bit management in case of I2C_NO_STARTSTOP request

- HAL OSPI driver

  - Add note on limitation of HAL_OSPI_AutoPolling() and HAL_OSPI_AutoPolling_IT() usage in octal mode (cf. Errata Sheet)
  - Fix compilation warning in C++

- HAL QSPI driver

  - Fix MISRA C-2004 rules 10.3, 11.4 and 12.6

- HAL RCC driver

  - Update SDMMC1 clock source selection on STM32L4Rx/STM32L4Sx devices to select PLL divider "P" output instead of internal multiplexor on MSI, HSI48, PLLSAI1 or PLL "Q" outputs as SDMMC1 kernel clock source
  - Fix __HAL_RCC_GPIOB_IS_CLK_ENABLED() macro definition

- HAL SDMMC driver

  - Fix management of peripheral flags depending on command or data transfers.

- HAL SMBUS driver

  - Fix RD_WRN bit management in case of SMBUS_NO_STARTSTOP request

LL drivers changes

- **LLDAC driver

  - Add missing definition for external triggers from TIM and LPTIM instances

- LL DMA2D driver

  - Fix CodeSonar warning in LL_DMA2D_StructInit()

- LL I2C driver

  - Fix RD_WRN bit management in case of LL_I2C_GENERATE_NOSTARTSTOP request in LL_I2C_HandleTransfer()

- LL RCC driver

  - Update SDMMC1 clock source selection on STM32L4Rx/STM32L4Sx devices to select PLL divider "P" output instead of internal multiplexor on MSI, HSI48, PLLSAI1 or PLL "Q" outputs as SDMMC1 kernel clock source

  - Add LL_RCC_SetSDMMCKernelClockSource(), LL_RCC_GetSDMMCKernelClockSource() and LL_RCC_GetSDMMCKernelClockFreq() APIs

V1.8.0 / 25-August-2017

## Main Changes

- Release of HAL and Low Layer drivers to add support of STM32L4R5xx/STM32L4R7xx/STM32L4R9xx/STM32L4S5xx/STM32L4S7xx/STM32L4S9xx devices

- New OctoSPI, DSI, LTDC, GFXMMU peripherals supported in new HAL OSPI, HAL DSI, HAL LTDC and HAL GFXMMU drivers

- Superset features device STM32L4S9xx API User Manual available (STM32L4S9xx_User_Manual.chm)

## Contents

HAL drivers changes

- HAL DSI driver (NEW): stm32l4xx_hal_dsi.h/.c files
- HAL GFXMMU driver (NEW):stm32l4xx_hal_gfxmmu.h/.c files
- HAL LTDC driver (NEW):stm32l4xx_hal_ltdc.h/.c and extension stm32l4xx_hal_ltdc_ex.h/.c files

- HAL OSPI driver (NEW):stm32l4xx_hal_ospi.h/.c files

- HAL generic driver

  - Add HAL_GetUIDw0(), HAL_GetUIDw1() and HAL_GetUIDw2 APIs
  - Default HAL_Delay() implementation updated to insure minimum requested delay
  - Add __HAL_SYSCFG_SRAM2_WRP_0_31_ENABLE() and __HAL_SYSCFG_SRAM2_WRP_32_63_ENABLE() macros to set respectively SRAM2 page protection attribute for page 0 to 31 and page 32 to 63

- HAL CAN driver

  - Add FIFOs overrun error management (new error codes HAL_CAN_ERROR_FOV0 and HAL_CAN_ERROR_FOV1)

- HAL CRYP driver

  - Fix zero padding in case of Data type
  - Fix phase setting related to payload suspension
  - Fix to not be too restrictive on input parameters in HAL_CRYPEx_AES_Auth() and HAL_CRYPEx_AES_Auth_DMA()

- HAL DAC driver

  - Fix Sample & Hold configuration in case of multi-channel
  - Rename DAC_HIGH_FREQUENCY_INTERFACE_MODE_ENABLE to DAC_HIGH_FREQUENCY_INTERFACE_MODE_ABOVE_80MHZ

- HAL DMA driver

  - Fix DMAMUX synchronization signal configuration in HAL_DMAEx_ConfigMuxSync()

  - Support of DMAMUX1 peripheral via new DMA Extension APIs

  - HAL_DMAEx_ConfigMuxRequestGenerator()
  - HAL_DMAEx_EnableMuxRequestGenerator(), HAL_DMAEx_DisableMuxRequestGenerator()
  - HAL_DMAEx_ConfigMuxSync()

  - HAL_DMAEx_MUX_IRQHandler()

- HAL DFSDM driver extension (new stm32l4xx_hal_dfsdm_ex.h/.c)

  - New APIs HAL_DFSDMEx_ChannelSetPulsesSkipping() and HAL_DFSDMEx_ChannelGetPulsesSkipping()

- HAL DFSDM driver

  - Fix cast issue to return possible negative value in HAL_DFSDM_FilterGetRegularValue(), HAL_DFSDM_FilterGetInjectedValue(), HAL_DFSDM_FilterGetExdMaxValue() and HAL_DFSDM_FilterGetExdMinValue()

- HAL FLASH driver

  - Add new LVE pin management in HAL_FLASHEx_ConfigLVEPin()
  - Fix timeout issue in private FLASH_WaitForLastOperation() API
  - Fix error status of HAL_FLASHEx_OBProgram(

- HAL FMC driver

  - New field NBLSetupTime added in FMC_NORSRAM_InitTypeDef structure
  - New field DataHoldTime added in FMC_NORSRAM_TimingTypeDef structure

- HAL HASH driver

  - Update of context swap mechanism implemented in HAL_HASH_DMAFeed_ProcessSuspend() when input data are fed to the IP by DMA

- HAL HCD/PCD driver

  - Add support of STM32L4R5xx/STM32L4R7xx/STM32L4R9xx/ STM32L4S5xx/STM32L4S7xx/STM32L4S9xx devices

- HAL IRDA driver

  - Add Clock Prescaler management for STM32L4Rx/STM32L4Sx devices only

  - IRDA_InitTypeDef structure update to add ClockPrescaler parameter

- HAL PCD driver

  - Fix USB PCD lock/unlock and flush TX fifo during device reset

- HAL PWR driver

  - Add PWR_REGULATOR_VOLTAGE_SCALE1_BOOST new parameter value for HAL_PWREx_ControlVoltageScaling() to use higher supply voltage (1.28V) with main regulator voltage in range 1 above 80Mhz (maximum frequency equals to 120Mhz) for STM32L4Rx/STM32L4Sx devices

  - Add SRAM3 retention management APIs: HAL_PWREx_EnableSRAM3ContentRetention() and HAL_PWREx_DisableSRAM3ContentRetention()

  - Add DSI pins pull-down management

  - new HAL_PWREx_EnableDSIPinsPDActivation() and HAL_PWREx_DisableDSIPinsPDActivation APIs

- HAL RCC driver

  - Add clock management of new peripherals: DSI, GFXMMU, LTDC, OSPI1, OSPI2, OSPIM
  - Add OctoSPI peripherals clock source frequency computation in HAL_RCCEx_GetPeriphCLKFreq()
  - Fix issue with main PLL divider M value to allow 1 to 16 value range on STM32L4Rx/STM32L4Sx devices
  - Fix SDMMC1 clock source selection possibilities in HAL_RCCEx_PeriphCLKConfig(), __HAL_RCC_SDMMC1_CONFIG() and __HAL_RCC_GET_SDMMC1_SOURCE()

  - Fix HAL_RCCEx_GetPeriphCLKFreq() to take into account PLLSAI1 and PLLSAI2 divider M values (1 to 16 range) on STM32L4Rx/STM32L4Sx devices

  - Add undershoot/overshoot management in HAL_RCC_ClockConfig() when switching to/from system clock from main PLL above 80Mhz

- HAL RNG driver

  - Add support of Clock Error detection and Bypass mode management in new RNG_InitTypeDef and HAL_RNG_Init() API

  - parameters ClockErrorDetection and BypassMode added in new RNG_InitTypeDef

- HAL RTC driver

  - Fix HAL_RTC_Init() to wait for synchronization and avoid RTC registers access timing issues

- HAL SAI driver

  - Add FIFO flush in HAL_SAI_DMAStop()

  - Fix HAL_SAI_Transmit_DMA() to follow the slave TX mode sequence described in the Reference Manual

- HAL SD driver

  - Major rework of HAL SD driver aligned with STM32F7 series

  - BlockSize parameter removed in Read&Write block APIs since 512 byte size is always read&write.

- HAL SMARTCARD driver

  - Add Clock Prescaler management for STM32L4Rx/STM32L4Sx devices only

  - SMARTCARD_InitTypeDef structure update to add ClockPrescaler parameter

  - Add FIFO mode management for STM32L4Rx/STM32L4Sx devices only

  - new HAL_SMARTCARDEx_EnableFifoMode(), HAL_SMARTCARDEx_DisableFifoMode(), HAL_SMARTCARDEx_SetTxFifoThreshold(), HAL_SMARTCARDEx_SetRxFifoThreshold(), HAL_SMARTCARDEx_RxFifoFullCallback() and HAL_SMARTCARDEx_TxFifoEmptyCallback APIs

- HAL SMBUS driver

  - Add Analog and digital filter configuration APIs: HAL_SMBUS_ConfigAnalogFilter() and HAL_SMBUS_ConfigDigitalFilter()
  - Add error management if occurring during STOP process

- HAL SPI driver

  - Add control of RXFIFO empty at end of transmissing in Master transmission 2 lines mode

- HAL SWPMI driver

  - Fix missing clock initialization before register update in HAL_SWPMI_Init()

- HAL TIM driver

  - Add TIM_TIM1_ETR_GPIO and TIM_TIM8_ETR_GPIO definitions
  - Add TIM_TIM16_TI1_MSI, TIM_TIM16_TI1_HSE_32 and TIM_TIM16_TI1_MCO definitions for STM32L4Rx/STM32L4Sx
  - Add new AutoReloadPreload parameter in TIM_Base_InitTypeDef (user code impacted)
  - Fix wrong MOE disable conditions with new macro __HAL_TIM_MOE_DISABLE_UNCONDITIONALLY()

- HAL UART driver

  - Add Clock Prescaler management for STM32L4Rx/STM32L4Sx devices only
  - UART_InitTypeDef structure update to add ClockPrescaler parameter

  - Add FIFO mode management for STM32L4Rx/STM32L4Sx devices only

  - new HAL_UARTEx_EnableFifoMode(), HAL_UARTEx_DisableFifoMode(), HAL_UARTEx_SetTxFifoThreshold(), HAL_UARTEx_SetRxFifoThreshold(), HAL_UARTEx_RxFifoFullCallback() and HAL_UARTEx_TxFifoEmptyCallback APIs

  - Add SPI Slave mode management for STM32L4Rx/STM32L4Sx devices only

  - new HAL_UARTEx_EnableSlaveMode(), HAL_UARTEx_DisableSlaveMode() and HAL_UARTEx_ConfigNSS()

- HAL USART driver (new stm32l4xx_hal_usart_ex.c)

  - Add Clock Prescaler management for STM32L4Rx/STM32L4Sx devices only

  - USART_InitTypeDef structure update to add ClockPrescaler parameter

  - Add FIFO mode management for STM32L4Rx/STM32L4Sx devices only

  - new HAL_USARTEx_EnableFifoMode(), HAL_USARTEx_DisableFifoMode(), HAL_USARTEx_SetTxFifoThreshold(), HAL_USARTEx_SetRxFifoThreshold(), HAL_USARTEx_RxFifoFullCallback() and HAL_USARTEx_TxFifoEmptyCallback APIs

  - Add SPI Slave mode management for STM32L4Rx/STM32L4Sx devices only

  - new HAL_USARTEx_EnableSlaveMode(), HAL_USARTEx_DisableSlaveMode() and HAL_USARTEx_ConfigNSS()

LL drivers changes

LL DMAMUX driver (NEW): stm32l4xx_ll_dmamux.h

All LL drivers update to remove usage of CMSIS POSITION_VAL() macro and resort to xx_Pos position bit definition

- LL ADC

  - Fix legacy APIs LL_ADC_REG_SetTrigSource() and LL_ADC_INJ_SetTrigSource()

- LL BUS

  - Add management of new peripherals: DSI, GFXMMU, LTDC, OSPI1, OSPI2, OSPIM

- LL DMA

  - Fix simple write register access to clear DMA flags in LL_DMA_ClearFlag_XXX APIs

- LL DMA2D

  - Add management of output swapping mode (regular or bytes two by two) and line offset mode (pixel or byte)

- LL EXTI

  - Add management of EXTI line 40 (I2C4)

- LL I2C

  - Fix LL_I2C_Init() to not set OAEN1 bit when Own Address 1 value is 0

- LL LPUART / LL USART

  - Add management of Rx FIFO and Tx FIFO

- LL PWR

  - Add SRAM3 retention management APIs

  - LL_PWR_EnableSRAM3Retention(), LL_PWR_DisableSRAM3Retention() and LL_PWR_IsEnabledSRAM3Retention()

  - Add voltage range 1 boost mode APIs

  - LL_PWR_EnableRange1BoostMode(), LL_PWR_DisableRange1BoostMode() and LL_PWR_IsEnabledRange1BoostMode()

  - For compatibility purpose across STM32 series, rename LL_PWR_IsActiveFlag_VOSF() to LL_PWR_IsActiveFlag_VOS()

  - Add DSI pins pull-down management

  - new LL_PWR_EnableDSIPinsPDActivation(), LL_PWR_DisableDSIPinsPDActivation() and LL_PWR_IsEnabledDSIPinsPDActivation APIs

- LL RCC

  - Add management of new peripheral clock sources for DSI, LTDC, OSPI1, OSPI2 and SDMMC

  - Add new definitions for main PLL divider M values above LL_RCC_PLLM_DIV_8 and up to LL_RCC_PLLM_DIV_16 for STM32L4Rx/STM32L4Sx devices

  - Fix in __LL_RCC_CALC_PLLCLK_SAI_FREQ(), __LL_RCC_CALC_PLLSAI1_SAI_FREQ(), __LL_RCC_CALC_PLLSAI1_48M_FREQ(), __LL_RCC_CALC_PLLSAI1_ADC_FREQ(), __LL_RCC_CALC_PLLSAI2_SAI_FREQ()

  - Fix in LL_RCC_PLLSAI1_ConfigDomain_48M(), LL_RCC_PLLSAI1_ConfigDomain_SAI(), LL_RCC_PLLSAI1_ConfigDomain_ADC(), LL_RCC_PLLSAI1_GetP(), LL_RCC_PLLSAI2_ConfigDomain_SAI() and LL_RCC_PLLSAI2_GetP()

  - Fix LL_RCC_GetSDMMCClockFreq() to take into account all SDMMC1 possible clock sources

  - Add HSI48 oscillator clock source value for RNG and USB:

    - LL_RCC_RNG_CLKSOURCE_HSI48 and update LL_RCC_GetRNGClockFreq()
    - LL_RCC_USB_CLKSOURCE_HSI48 and update LL_RCC_GetUSBClockFreq()

  - General fixes

    - Renaming of RCC_DFSDM1CLKSOURCE_PCLK to RCC_DFSDM1CLKSOURCE_PCLK2
    - Renaming of RCC_SWPMI1CLKSOURCE_PCLK to RCC_SWPMI1CLKSOURCE_PCLK1
    - Renaming of RCC_LPTIMxCLKSOURCE_PCLK to RCC_LPTIMxCLKSOURCE_PCLK1

- LL RNG

  - Add Clock Error detection and Bypass mode management in new LL_RNG_InitTypeDef and new LL_RNG_Init() API

    - new LL_RNG_EnableClkErrorDetect(), LL_RNG_DisableClkErrorDetect() and LL_RNG_IsEnableClkErrorDetect()
    - new LL_RNG_EnableBypassMode(), LL_RNG_DisableBypassMode() and LL_RNG_IsEnabledBypassMode

- LL RTC

  - LL_RTC_TIME_Get() and LL_RTC_DATE_Get() implementations optimization (single register read access)

- LL SYSTEM

  - Add SRAM2 page write protection APIs: LL_SYSCFG_EnableSRAM2PageWRP_0_31() and LL_SYSCFG_EnableSRAM2PageWRP_32_63()

- LL TIM

  - Fix definition of TIM break input polarity (inverse values LL_TIM_BKIN_POLARITY_LOW / LL_TIM_BKIN_POLARITY_HIGH)
  - Fix LL_TIM_EnableUpdateEvent(), LL_TIM_DisableUpdateEvent() and LL_TIM_IsEnabledUpdateEvent()

- LL UTILS

  - Add management of new flash latency ranges in UTILS_SetFlashLatency()
  - Add undershoot management when switching to system clock from main PLL above 80Mhz in LL_PLL_ConfigSystemClock_MSI(), LL_PLL_ConfigSystemClock_HSI() and LL_PLL_ConfigSystemClock_HSE()

V1.7.2 / 16-June-2017

## Main Changes

- Maintenance Release of HAL and Low Layer drivers

## Contents

HAL drivers changes

- HAL CAN driver

  - Add overrun error management by the error callback

- HAL CRC driver

  - Update of HAL_CRCEx_Polynomial_Set() to return an error when a non-supported polynomial length is passed as parameter
- HAL CRYP driver
  - Update zero padding management with respect to data type
  - Phase setting and comments correction in case of payload phase suspension
  - Correct input parameters tests in HAL_CRYPEx_AES_Auth() and HAL_CRYPEx_AES_Auth_DMA APIs
  - Correct interruptions and IP enabling flags setting for key derivation in IT mode

- HAL DCMI driver

  - Comments correction to describe image size management when larger than maximum authorized DMA transfer size

- HAL FLASH driver

  - Add software work - around in HAL_FLASH_Unlock() to clear OPTVERR flag on STM32L45x/L46x parts when initially improperly raised
  - Correct timeout issue in FLASH_WaitForLastOperation()

- HAL HASH driver

  - Update of context swap mechanism implemented in HAL_HASH_DMAFeed_ProcessSuspend() when input data are fed to the IP by DMA

LL drivers changes

- LL RCC

  - Correct duplication of aRCC_APBAHBPrescTable

- LL RTC

  - Simplification of implementation of function LL_RTC_DATE_Get()

- LL TIM

  - Fix LL_TIM_EnableUpdateEvent(), LL_TIM_DisableUpdateEvent() and LL_TIM_IsEnabledUpdateEvent()

V1.7.1 / 21-April-2017

## Main Changes

- Maintenance Release of HAL and Low Layer drivers

## Contents

HAL drivers changes

- HAL generic driver

  - Add HAL_GetUIDw0(), HAL_GetUIDw1() and HAL_GetUIDw2 APIs

- HAL DAC driver

  - Fix Sample & Hold configuration in case of multi-channel

- HAL HASH driver

  - Fix to ensure proper DMA-based HASH processing suspension/resumption

- HAL PCD driver

  - Fix USB PCD lock/unlock and flush TX fifo during device reset

- HAL RTC driver

  - Add wait for synchronization in HAL_RTC_Init() to insure RTC time initialization

LL drivers changes

- LL ADC

  - Fix legacy APIs LL_ADC_REG_SetTrigSource() and LL_ADC_INJ_SetTrigSource()

- LL DMA

  - Write only operation on IFCR register

V1.7.0 / 17-February-2017

## Main Changes

- Release of HAL and Low Layer drivers to add support of STM32L496xx/STM32L4A6xx devices
- New DCMI, DMA2D, HASH peripherals supported in new HAL DCMI, HAL & LL DMA2D and HAL HASH drivers
- New CAN2 instance supported in HAL CAN
- Superset features device STM32L4A6xx API User Manual available (STM32L4A6xx_User_Manual.chm)

## Contents

HAL drivers changes

- HAL DCMI driver (NEW): stm32l4xx_hal_dcmi.h/.c files
- HAL DMA2D driver (NEW): stm32l4xx_hal_dma2d.h/.c files
- HAL HASH driver (NEW): stm32l4xx_hal_hash.h/.c and extension stm32l4xx_hal_hash_ex.h/.c files

The following changes done on the HAL drivers require an update on the application code based on older HAL versions

- HAL SD update

Overall rework of the driver for a more efficient implementation

- Modify initialization API and structures
- Modify Read / Write sequences: separate transfer process and SD Cards state management
- Adding interrupt mode for Read / Write operations]
- Update the HAL_SD_IRQHandler function by optimizing the management of interrupt errors

Refer to the following examples in STM32CubeL4 firmware package V1.7.0 to identify the changes: BSP example and USB_Device/MSC_Standalone application

- HAL generic update

  - stm32l4xx_hal_conf_template.h updated for new HAL DCMI, HAL DMA2D and HAL HASH

  - #define HAL_DCMI_MODULE_ENABLED
  - #define HAL_DMA2D_MODULE_ENABLED

  - #define HAL_HASH_MODULE_ENABLED

  - HAL_Delay() updated to guarantee minimum delay

- HAL CAN driver

  - Add support of CAN2 instance

- HAL GPIO driver

  - Add support of GPIOI port and STM32L496xx/STM32L4A6xx alternate functions

- HAL PWR driver

  - Add support of GPIOI port pull-up/pull-down state in Standby and Shutdown modes

- HAL QSPI driver

  - Fix QSPI_HandleTypeDef structure to handle data size as uint32_t

- HAL RCC driver

  - Add new macros for new peripherals clock and reset for CAN2, DCMI, DMA2D, GPIOI and HASH

  - Fix HAL_RCCEx_GetPeriphCLKFreq() to compute peripheral frequencies from MSI frequency

  - Fix HAL_RCCEx_GetPeriphCLKFreq() to compute DFSDM1 frequency from PCLK2 frequency

  - Rename some peripheral clock sources to specify the corresponding APB clock:

  - RCC_DFSDM1CLKSOURCE_PCLK to RCC_DFSDM1CLKSOURCE_PCLK2

  - RCC_SWPMI1CLKSOURCE_PCLK to RCC_SWPMI1CLKSOURCE_PCLK1

  - RCC_LPTIMxCLKSOURCE_PCLK to RCC_LPTIMxCLKSOURCE_PCLK1

- HAL RTC driver

  - Fix wrong clear of time and date registers in HAL_RTCEx_TamperTimeStampIRQHandler()

- HAL SPI driver

  - Add internal timeout to exit HAL_SPI_Abort() and HAL_SPI_Abort_IT()

- HAL TIM driver

  - Fix wrong MOE disable conditions with new macro __HAL_TIM_MOE_DISABLE_UNCONDITIONALLY()

- HAL SWPMI driver

  - Fix peripheral clock management sequence in HAL_SWPMI_Init()

LL drivers changes

- LL DMA2D driver (NEW)

- LL BUS

  - Add management of new peripherals: CAN2, DCMI, DMA2D, GPIOI and HASH

- LL PWR

  - For compatibility purpose across STM32 series, rename LL_PWR_IsActiveFlag_VOSF() to LL_PWR_IsActiveFlag_VOS()

- LL RCC

  - Fix LL_RCC_GetDFSDMClockFreq() to compute frequency from PCLK2 frequency

- LL SDMMC

  - Add new internal functions after HAL SD rework

- LL TIM

  - Fix definition of TIM break input polarity (fix values LL_TIM_BKIN_POLARITY_LOW / LL_TIM_BKIN_POLARITY_HIGH)

V1.6.0 / 28-October-2016

## Main Changes

- Release of HAL and Low Layer drivers to add support of STM32L451xx/STM32L452xx/STM32L462xx devices
- Superset features device STM32L462xx API User Manual available (STM32L462xx_User_Manual.chm)

## Contents

HAL drivers changes

- HAL CRYP driver

  - HAL CRYP exported macros alignment with other STM32 series to use CRYP handle address as parameter in:

  - __HAL_CRYP_ENABLE(), __HAL_CRYP_DISABLE(), __HAL_CRYP_SET_OPERATINGMODE(), __HAL_CRYP_SET_CHAININGMODE(), __HAL_CRYP_GET_FLAG(), __HAL_CRYP_CLEAR_FLAG(), __HAL_CRYP_GET_IT_SOURCE(), __HAL_CRYP_GET_IT(), __HAL_CRYP_CLEAR_IT(), __HAL_CRYP_ENABLE_IT() and __HAL_CRYP_DISABLE_IT()

- HAL FLASH driver

  - Temporary data cache deactivation on

    - Flash programming in HAL_FLASH_Program() and HAL_FLASH_Program_IT()
    - Flash erase in HAL_FLASHEx_Erase() and HAL_FLASHEx_Erase_IT()

  - To insure LSB/MSB address order in C compiler assembly output, split 64-bit programming in 2 double-word write operations

- HAL I2C driver

  - Fix to reset HAL I2C handle LISTEN state option in transfer direction change with HAL_I2C_Slave_Sequential_Transmit_IT() and HAL_I2C_Slave_Sequential_Receive_IT()

- HAL SMBUS driver

  - Add support of Zone read/write feature thanks to new XferOptions parameter values SMBUS_OTHER_FRAME_NO_PEC, SMBUS_OTHER_FRAME_WITH_PEC, SMBUS_OTHER_AND_LAST_FRAME_NO_PEC and SMBUS_OTHER_AND_LAST_FRAME_WITH_PEC that may be used in HAL_SMBUS_Master_Transmit_IT(), HAL_SMBUS_Master_Receive_IT(), HAL_SMBUS_Slave_Transmit_IT() and HAL_SMBUS_Slave_Receive_IT()

- HAL RTC driver

  - Fix race conditions on EXTI flags clearing in HAL_RTC_AlarmIRQHandler(), HAL_RTCEx_TamperTimeStampIRQHandler() and HAL_RTCEx_WakeUpTimerIRQHandler()

- Fix CodeSonar warnings in

  - HAL ADC, HAL CRC, HAL CRYP, HAL I2C, HAL IRDA, HAL SMARTCARD, HAL SMBUS, HAL OPAMP, HAL RTC, HAL UART, HAL USART

LL drivers changes

- LL I2C driver

  - Add I2C4 management in LL_I2C_DeInit()

- LL SYSTEM driver

  - Application shall be responsible to write the correct key sequence in SYSCFG_SKR register prior to call LL_SYSCFG_EnableSRAM2Erase()

- LL TIM driver

  - New APIs to insure BDTR register initialization in a single write operation

  - LL_TIM_BDTR_StructInit()

  - LL_TIM_BDTR_Init()

- LL UTILS driver

  - Fix LL_RCC_PLLSOURCE_HSE in LL_PLL_ConfigSystemClock_HSE()

V1.5.2 / 12-September-2016

## Contents

HAL drivers changes

- HAL ADC driver

  - No need to configure number of discontinuous conversions if discontinuous mode is not enabled
  - HAL_ADCEx_MultiModeConfigChannel() returns HAL_ERROR if no Slave instance defined

- HAL DAC driver

  - Fix calibration with correct handling of DAC_SR_CAL_FLAGx bits in HAL_DACEx_SelfCalibrate()

- HAL FLASH driver

  - Change in HAL_FLASHEx_OBGetConfig() to not return PCROP and/or WRP data if their respective areas are not defined
  - Fix error management in HAL_FLASH_IRQHandler() to simply call HAL_FLASH_OperationErrorCallback() instead of calling both HAL_FLASH_EndOfOperationCallback() and HAL_FLASH_OperationErrorCallback()

- HAL I2C driver

  - Fix wrong state check in HAL_I2C_Master_Sequential_Transmit_IT()
  - Add new option I2C_FIRST_AND_NEXT_FRAME to manage a sequencewith start condition, address and data to transfer without a final stop condition allowing successive calls to HAL_I2C_Master_Sequential_Transmit_IT()

- HAL IRDA driver

  - Add transfer abort functions and associated callbacks in interrupt mode

    - HAL_IRDA_Abort(), HAL_IRDA_AbortTransmit(), HAL_IRDA_AbortReceive()
    - HAL_IRDA_Abort_IT(), HAL_IRDA_AbortTransmit_IT(), HAL_IRDA_AbortReceive_IT()
    - HAL_IRDA_AbortCpltCallback(), HAL_IRDA_AbortTransmitCpltCallback(), HAL_IRDA_AbortReceiveCpltCallback()
    - IRQ Handler + DMA model optimizations

- HAL RTC driver

  - Fix missing wakeup flag clear in HAL_RTCEx_SetWakeUpTimer_IT()

- HAL SMARTCARD driver

  - Add transfer abort functions and associated callbacks in interrupt mode

    - HAL_SMARTCARD_Abort(), HAL_SMARTCARD_AbortTransmit(), HAL_SMARTCARD_AbortReceive()
    - HAL_SMARTCARD_Abort_IT(), HAL_SMARTCARD_AbortTransmit_IT(), HAL_SMARTCARD_AbortReceive_IT()
    - HAL_SMARTCARD_AbortCpltCallback(), HAL_SMARTCARD_AbortTransmitCpltCallback(), HAL_SMARTCARD_AbortReceiveCpltCallback()

  - IRQ Handler + DMA model optimizations

- HAL SMBUS driver

  - Fix issue on last data reception in host or device modes

- HAL SPI driver

  - USE_SPI_CRCcompilation define added to provide the mean to optimize the HAL SPI driver when CRC feature is not used (when CRC is used, application must be changed to set USE_SPI_CRC in stm32l4xx_hal_conf.h (see Inc\stm32l4xx_hal_conf_template.h))

  - Add transfer abort functions and associated callbacks in interrupt mode
    - HAL_SPI_Abort()
    - HAL_SPI_Abort_IT()
    - HAL_SPI_AbortCpltCallback()

- HAL SWPMI driver

  - Fix SWPMI peripheral errors management in DMA (resort to HAL_DMA_Abort_IT() and DMA XferAbortCallback in HAL_SWPMI_IRQHandler())

- HAL UART driver

  - New APIs to abort UART transfer with associated callbacks added
    - HAL_UART_Abort(), HAL_UART_AbortTransmit(), HAL_UART_AbortReceive(), HAL_UART_Abort_IT(), HAL_UART_AbortTransmit_IT(), HAL_UART_AbortReceive_IT(), HAL_UART_AbortCpltCallback(), HAL_UART_AbortTransmitCpltCallback() and HAL_UART_AbortReceiveCpltCallback()

- HAL USART driver

  - New APIs to abort USART transfer with associated callbacks added

    - HAL_USART_Abort(), HAL_USART_Abort_IT() and HAL_USART_AbortCpltCallback()

LL drivers changes

- LL COMP driver

  - Fis LL_COMP_INPUT_PLUS_IO3 definition

V1.5.1 / 31-May-2016

## Contents

HAL drivers changes

- HAL ADC driver

  - Bypass multimode assert_param macro calls depending on configuration

- HAL CRC driver

  - HAL_CRC_DeInit() resets CRC_IDR register to reset value

LL drivers changes

- LL BUS driver
  - LL_APB1_GRP1_PERIPH_USBFS renamed to LL_APB1_GRP1_PERIPH_USB
- LL SYSTEMdriver
  - Fix typo on LL_DBGMCU_APB1_xxx and LL_DBGMCU_APB2_xxx

V1.5.0 / 29-April-2016

## Main Changes

- Maintenance Release of HAL and Low Layer drivers

## Contents

HAL drivers changes

Enhance HAL delay and timebase implementation

- Add new driver stm32l4xx_hal_timebase_tim_template.c which overrides the native HAL time base functions (defined as weak) to use the TIM peripheral as time base tick source. For more details about the usage of this driver, please refer to HAL\HAL_TimeBase example and FreeRTOS-based applications

The following changes done on the HAL drivers require an update on the application code based on HAL V1.4.0.

- HAL RCC driver

  - To use PLLSAI1 and PLLSAI2 indidependently from main system PLL, PLLSAI1 & PLLSAI2 initialization enriched to add PLL entry clock source and divider M

  - RCC_PLLSAI1InitTypeDef includes PLLSAI1Source and PLLSAI1M new fields

  - RCC_PLLSAI2InitTypeDef includes PLLSAI2Source and PLLSAI2M new fields

  - Add missing RTC clock source definition RCC_RTCCLKSOURCE_NO_CLK

  - DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility)
    - All macros __HAL_RCC_DFSDM_xxx() renamed to __HAL_RCC_DFSDM1_xxx()
    - DfsdmClockSelection field of RCC_PeriphCLKInitTypeDef renamed to Dfsdm1ClockSelection
    - RCC_PERIPHCLK_DFSDM renamed to RCC_PERIPHCLK_DFSDM1
    - RCC_DFSDMCLKSOURCE_PCLK renamed to RCC_DFSDM1CLKSOURCE_PCLK
    - RCC_DFSDMCLKSOURCE_SYSCLK renamed to RCC_DFSDM1CLKSOURCE_SYSCLK
    - __HAL_RCC_DFSDM_CONFIG() renamed to __HAL_RCC_DFSDM1_CONFIG()
    - __HAL_RCC_GET_DFSDM_SOURCE() renamed to __HAL_RCC_GET_DFSDM1_SOURCE()

  - Add missing RTC clock source definition RCC_RTCCLKSOURCE_NO_CLK

- HAL I2C driver

  - Update to avoid waiting on STOPF/BTF/AF flag under DMA ISR by using the PPP end of transfer interrupt in the DMA transfer process. This requires the following updates on user application:

  - Configure and enable the I2Cx IRQ in HAL_I2C_MspInit() function

  - In stm32l4xx_it.c file, I2Cx_IRQHandler() function: add a call to HAL_I2C_IRQHandler() function

- HAL UART/USART drivers

  - IRQ Handler global optimization
  - Add error management in case of DMA transfer through HAL_DMA_Abort_IT() and DMA XferAbortCallback()
    - Polling management update
    - The user Timeout value must be estimated for the overall process duration

- HAL IRDA/SMARTCARD drivers

  - Polling management update
    - The user Timeout value must be estimated for the overall process duration

- HAL SPI driver

  - Add SPI error management during DMA process: this requires the following updates in the user application:
  - Configure and enable the SPIx IRQ in HAL_SPI_MspInit() function
  - In stm32l4xx_it.c file, SPIx_IRQHandler() function: add a call to HAL_SPI_IRQHandler() function
  - Add and customize the Error Callback API: HAL_SPI_ErrorCallback()]

- HAL QSPI driver

  - Add QSPI error management during DMA process
  - Improve the DMA transmit process by using QSPI TC interrupt instead of waiting on TC flag under DMA ISR
  - These two improvements require the following updates on user application:
    - Configure and enable the QSPI IRQ in HAL_QSPI_MspInit() function
    - In stm32l4xx_it.c file, QSPI_IRQHandler() function: add a call to HAL_QSPI_IRQHandler() function
    - Add and customize the Error Callback API: HAL_QSPI_ErrorCallback()

  - Add the management of non-blocking transfer abort service: HAL_QSPI_Abort_IT(). In this case the user must:

    - Add new callback HAL_QSPI_AbortCpltCallback() to inform user at the end of abort process
    - A new value of State in the HAL_QSPI_StateTypeDef provides the current state during the abort phase
  - Polling management update:
    - The user Timeout value must be estimated for the overall process duration
  - Fix wrong data size management in HAL_QSPI_Receive_DMA()
    - New API HAL_QSPI_SetFifoThreshold() and HAL_QSPI_GetFifoThreshold()

- HAL IWDG driver

  - New simplified HAL IWDG driver:
    - remove HAL_IWDG_Start(), HAL_IWDG_MspInit() and HAL_IWDG_GetState() APIs
  - API functions are:
    - HAL_IWDG_Init(): this function insures the configuration and the start of the IWDG counter
    - HAL_IWDG_Refresh(): this function insures the reload of the IWDG counter
  - Refer to the following example to identify the changes: IWDG_Example

- HAL WWDG driver

  - New simplified HAL WWDG driver: remove HAL_WWDG_Start(), HAL_WWDG_Start_IT(), HAL_WWDG_MspDeInit() and HAL_WWDG_GetState() APIs
    - Update HAL_WWDG_Refresh() API to remove counter parameter
    - New field EWIMode in WWDG_InitTypeDef to specify need for Early Wakeup Interrupt
  - API functions are: HAL_WWDG_Init(), HAL_WWDG_MspInit(), HAL_WWDG_Refresh(), HAL_WWDG_IRQHandler() and HAL_WWDG_EarlyWakeupCallback()

- HAL DMA driver

  - Global driver code optimization to reduce memory footprint

  - New APIs HAL_DMA_RegisterCallback() and HAL_DMA_UnRegisterCallback() to register/unregister the different possible callbacks identified by enum typedef HAL_DMA_CallbackIDTypeDef
  - New API HAL_DMA_Abort_IT() to abort DMA transfer in non-blocking mode for interrupt context
  - The new registered Abort callback is called when DMA transfer abortion is completed
  - Add new Error Codes: HAL_DMA_ERROR_NO_XFER and HAL_DMA_ERROR_NOT_SUPPORTED

  - Add __HAL_DMA_GET_COUNTER() macro

- HAL COMP driver
  - EXTI configuration done in HAL_COMP_Init() based on TriggerMode field of COMP_InitTypeDef structure; HAL_COMP_Start()/HAL_COMP_Stop() APIs are sufficient to start and stop comparators (HAL_COMP_Start_IT() and HAL_COMP_Stop_IT() are preserved for legacy compatibility)
  - Add comparator startup time and scaler bridge stabilization time in HAL_COMP_Init()
  - Fix to call HAL_COMP_TriggerCallback() only once when the 2 comparators are configured in window mode
  - Inverting & Non-inverting inputs renaming (previous definitions preserved for legacy compatibility)
    - COMP_INVERTING_xxx definitions renamed to COMP_INPUT_MINUS_xxx
    - COMP_NONINVERTING_xxx definitions renamed to COMP_INPUT_PLUS_xxx
  - Blanking sources renaming to highlight Comparator & Timer instances connections (previous definitions preserved for legacy compatibility)
    - COMP_BLANKINGSRCE_TIM1OC5 renamed to COMP_BLANKINGSRC_TIM1_OC5_COMP1
    - COMP_BLANKINGSRCE_TIM2OC3 renamed to COMP_BLANKINGSRC_TIM2_OC3_COMP1
    - COMP_BLANKINGSRCE_TIM3OC3 renamed to COMP_BLANKINGSRC_TIM3_OC3_COMP1
    - COMP_BLANKINGSRCE_TIM3OC4 renamed to COMP_BLANKINGSRC_TIM3_OC4_COMP2
    - COMP_BLANKINGSRCE_TIM8OC5 renamed to COMP_BLANKINGSRC_TIM8_OC5_COMP2
    - COMP_BLANKINGSRCE_TIM15OC1 renamed to COMP_BLANKINGSRC_TIM15_OC1_COMP2
    - COMP_BLANKINGSRCE_NONE renamed to COMP_BLANKINGSRC_NONE
- HAL CRYP driver
  - Software workaround for AES issue on GCM encryption with payload length not a multiple of 128 bits
  - Add support of payload length not multiple of 32 bits

- HAL GPIO driver

  - Add missing GPIO_AF6_COMP1 for STM32L431xx/STM32L432xx/STM32L433xx/STM32L442xx/STM32L443xx
  - DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility)
    - GPIO_AF6_DFSDM renamed to GPIO_AF6_DFSDM1
- HAL HCD driver
  - Clear NACK flag before re-enabling the channel for new IN request

- HAL PCD driver

  - Host mode
    - Use HCLK frequency to set TRDT value
  - Device mode
    - Force suspend and low-power mode before going to L1 state
  - Unmask Start Of Frame interrupt

- HAL TIM driver

  - DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility)
  - TIM_BREAKINPUTSOURCE_DFSDM renamed to TIM_BREAKINPUTSOURCE_DFSDM1

- HAL SAI driver

  - Update HAL_SAI_IRQHandler:

  - Add error management in case of DMA transfer through HAL_DMA_Abort_IT() and DMAXferAbortCallback()

- HAL SWPMI driver

  - Update initialization sequence in voltage class B

LL drivers changes

- LL ADC driver
  - Fix injected conversion configuration with SW start in LL_ADC_INJ_ConfigQueueContext()
- LL BUS driver
  - DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility)
  - LL_APB2_GRP1_PERIPH_DFSDM renamed to LL_APB2_GRP1_PERIPH_DFSDM1
- LL COMP driver
  - Window mode renaming to highlight Comparator instances connection (previous definitions preserved for legacy compatibility)
  - LL_COMP_WINDOWMODE_ENABLE renamed to LL_COMP_WINDOWMODE_COMP1_INPUT_PLUS_COMMON
  - Blanking sources renaming to highlight Comparator & Timer instances connections (previous definitions preserved for legacy compatibility)
  - LL_COMP_BLANKINGSRCE_TIM1OC5 renamed to LL_COMP_BLANKINGSRC_TIM1_OC5_COMP1
  - LL_COMP_BLANKINGSRCE_TIM2OC3 renamed to LL_COMP_BLANKINGSRC_TIM2_OC3_COMP1
  - LL_COMP_BLANKINGSRCE_TIM3OC3 renamed to LL_COMP_BLANKINGSRC_TIM3_OC3_COMP1
  - LL_COMP_BLANKINGSRCE_TIM3OC4 renamed to LL_COMP_BLANKINGSRC_TIM3_OC4_COMP2
  - LL_COMP_BLANKINGSRCE_TIM8OC5 renamed to LL_COMP_BLANKINGSRC_TIM8_OC5_COMP2
  - LL_COMP_BLANKINGSRCE_TIM15OC1 renamed to LL_COMP_BLANKINGSRC_TIM15_OC1_COMP2
- LL I2C driver
  - Add SMBus feature support
    - LL_I2C_InitTypeDef structure enriched with new PeripheralMode field to indicate I2C or SMBus modes
    - New APIs LL_I2C_EnableSMBusAlert(), LL_I2C_DisableSMBusAlert(), LL_I2C_IsEnabledSMBusAlert(), LL_I2C_EnableSMBusPEC(), LL_I2C_DisableSMBusPEC(), LL_I2C_IsEnabledSMBusPEC(), LL_I2C_ConfigSMBusTimeout(), LL_I2C_EnableSMBusTimeout(), LL_I2C_DisableSMBusTimeout(), LL_I2C_IsEnabledSMBusTimeout(), LL_I2C_SetSMBusTimeoutA(), LL_I2C_GetSMBusTimeoutA(), LL_I2C_SetSMBusTimeoutAMode(), LL_I2C_GetSMBusTimeoutAMode(), LL_I2C_SetSMBusTimeoutB(), LL_I2C_GetSMBusTimeoutB(), LL_I2C_SetSMBusTimeoutBMode(), LL_I2C_GetSMBusTimeoutBMode(), LL_I2C_IsActiveSMBusFlag_PECERR(), LL_I2C_IsActiveSMBusFlag_TIMEOUT(), LL_I2C_IsActiveSMBusFlag_ALERT(), LL_I2C_ClearSMBusFlag_PECERR(), LL_I2C_ClearSMBusFlag_TIMEOUT(), LL_I2C_ClearSMBusFlag_ALERT(), LL_I2C_EnableSMBusPECCompare(), LL_I2C_IsEnabledSMBusPECCompare() and LL_I2C_GetSMBusPEC()
  - New APIs LL_I2C_SetMode() and LL_I2C_GetMode()
  - New APIs LL_I2C_EnableAutoEndMode(), LL_I2C_DisableAutoEndMode() and LL_I2C_IsEnabledAutoEndMode()
  - New APIs LL_I2C_EnableReloadMode(), LL_I2C_DisableReloadMode() and LL_I2C_IsEnabledReloadMode()
  - New APIs LL_I2C_EnableSlaveByteControl(), LL_I2C_DisableSlaveByteControl() and LL_I2C_IsEnabledSlaveByteControl()
  - New APIs LL_I2C_SetTransferRequest(), LL_I2C_GetTransferRequest(), LL_I2C_SetSlaveAddr() and LL_I2C_GetSlaveAdd()
  - New APIs LL_I2C_SetTransferSize() and LL_I2C_GetTransferSize()
  - New APIs LL_I2C_GenerateStopCondition(), L_I2C_GenerateStartCondition()
  - New APIs LL_I2C_EnableAuto10BitRead(), LL_I2C_DisableAuto10BitRead() and LL_I2C_IsEnabledAuto10BitRead()
- LL PWR driver
  - New APIs LL_PWR_EnterLowPowerRunMode() and LL_PWR_ExitLowPowerRunMode()

- LL RCC driver

  - DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility)
  - LL_RCC_DFSDM_CLKSOURCE renamed to LL_RCC_DFSDM1_CLKSOURCE
  - LL_RCC_DFSDM_CLKSOURCE_PCLK renamed to LL_RCC_DFSDM1_CLKSOURCE_PCLK
  - LL_RCC_DFSDM_CLKSOURCE_SYSCLK renamed to LL_RCC_DFSDM1_CLKSOURCE_SYSCLK

- LL SYSTEM driver

- New API LL_FLASH_IsPrefetchEnabled()

- LL TIM driver
  - DFSDM renaming to DFSDM1 (previous definitions preserved for legacy compatibility)
  - LL_TIM_BKIN_SOURCE_DFBK renamed to LL_TIM_BKIN_SOURCE_DF1BK
  - New OCRef clear input selection definitions LL_TIM_OCREF_CLR_INT_NC and LL_TIM_OCREF_CLR_INT_ETR
  - New OCRef clear API LL_TIM_SetOCRefClearInputSource()

V1.4.0 / 26-February-2016

## Main Changes

- Release of HAL and Low Layer drivers to add support of STM32L431xx/STM32L432xx/STM32L433xx/STM32L442xx/STM32L443xx devices
- Low Layer driver initialization/de-initialization APIs applicable to all STM32L4xx devices
- CRS peripheral implemented as an extension of HAL RCC (HAL_RCCEx_CRS_xxxx APIs)
- Superset features device STM32L443xx API User Manual available (STM32L443xx_User_Manual.chm)

## Contents

HAL drivers changes

- HAL generic update

  - Add default HSI48_VALUE in stm32l4xx_hal_conf_template
- HAL CRYP update
  - New error code HAL_CRYP_BUSY_ERROR to reject new request while ongoing processing

- HAL IRDA/SMARTCARD/UART/USART update

  - Improvement of baud rate computation at initialization

LL drivers changes

- New C files requiring to use USE_FULL_LL_DRIVER compilation switch in user project to benefit from new APIs
  - stm32l4xx_ll_crs.c
- LL BUS update
  - Add read-back register on clock enable functions to take into account any delay on bus

- LL ADC update

  - Trigger sources renaming:

    - LL_ADC_REG_TRIG_SW_START renamed to LL_ADC_REG_TRIG_SOFTWARE
    - LL_ADC_REG_TRIG_EXT_TIMx_CCy renamed to LL_ADC_REG_TRIG_EXT_TIMx_CHy
    - LL_ADC_INJ_TRIG_SW_START renamed to LL_ADC_INJ_TRIG_SOFTWARE
    - LL_ADC_INJ_TRIG_EXT_TIMx_CCy renamed to LL_ADC_INJ_TRIG_EXT_TIMx_CHy

  - Oversamping data shift renaming:

    - LL_ADC_OVS_DATA_SHIFT_NONE renamed to LL_ADC_OVS_SHIFT_NONE
    - LL_ADC_OVS_DATA_SHIFT_xxx renamed to LL_ADC_OVS_SHIFT_xxx
- LL DAC update

  - Trigger sources renaming:

    - LL_DAC_TRIGGER_SOFTWARE renamed to LL_DAC_TRIG_SOFTWARE
    - LL_DAC_TRIGGER_TIMx_TRGO renamed to LL_DAC_TRIG_EXT_TIMx_TRGO
    - LL_DAC_TRIGGER_EXT_IT9 renamed to LL_DAC_TRIG_EXT_EXTI_LINE9
- LL LPUART update
  - Improvement of LPUARTDIV value in baud rate computation in __LL_LPUART_DIV() macro
- LL USART update
  - Improvement of USARTDIV value in baud rate computation in __LL_USART_DIV_SAMPLING8() and __LL_USART_DIV_SAMPLING16() macros

V1.3.0 / 29-January-2016

## Main Changes

- New Low Layer driver initialization/de-initialization APIs
  - Naming rule is LL_PPP_Init(), LL_PPP_StructInit(), LL_PPP_DeInit() and more initialization APIs when applicable for peripheral PPP: ADC, COMP, CRC, DAC, DMA, EXTI, GPIO, I2C, LPTIM, LPUART, OPAMP, PWR, RCC, RNG, RTC, SPI, SWPMI, TIM and USART.
- New C files requiring to use USE_FULL_LL_DRIVER compilation switch in user project to benefit from new APIs
  - stm32l4xx_ll_adc.c, stm32l4xx_ll_comp.c, stm32l4xx_ll_crc.c, stm32l4xx_ll_dac.c, stm32l4xx_ll_dma.c, stm32l4xx_ll_exti.c, stm32l4xx_ll_gpio.c, stm32l4xx_ll_i2c.c, stm32l4xx_ll_lptim.c, stm32l4xx_ll_lpuart.c, stm32l4xx_ll_opamp.c, stm32l4xx_ll_pwr.c, stm32l4xx_ll_rcc.c, stm32l4xx_ll_rng.c, stm32l4xx_ll_rtc.c, stm32l4xx_ll_spi.c, stm32l4xx_ll_swpmi.c, stm32l4xx_ll_tim.c and stm32l4xx_ll_usart.c
  - stm32l4xx_ll_utils.c contains some Low Layer utilities for SysTick, Flash latency and clock configuration.
- Fix "parameter unused" GCC compilation warnings on __weak functions

## Contents

HAL drivers changes

- HAL generic update

  - Declare uwTick as global variable to allow weak HAL_IncTick() API updates in user application
  - Add new API HAL_SYSCFG_EnableIOAnalogSwitchBooster() and HAL_SYSCFG_DisableIOAnalogSwitchBooster()

- HAL COMP update

  - Allow comparator lock from the reset state with HAL_COMP_Lock()

- HAL CRYP update

  - Fix state issue to resume AES calculations

- HAL DMA update

  - Fix state issue after DMA transfer error

- HAL FLASH update

  - Fix __HAL_FLASH_INSTRUCTION_CACHE_RESET() and __HAL_FLASH_DATA_CACHE_RESET() to allow multiple resets

- HAL I2C update

  - Add support of repeated start feature with the following new APIs
    - HAL_I2C_Master_Sequential_Transmit_IT(), HAL_I2C_Master_Sequential_Receive_IT() and HAL_I2C_Master_Abort_IT(),
    - HAL_I2C_Slave_Sequential_Transmit_IT() and HAL_I2C_Slave_Sequential_Receive_IT()
    - HAL_I2C_EnableListen_IT() and HAL_I2C_DisableListen_IT()
    - New user callbacks HAL_I2C_ListenCpltCallback() and HAL_I2C_AddrCallback()
  - Fix acknowledge failure error management (STOP being automatically generated)
  - Review state machine and provide new API HAL_I2C_GetMode() to return HAL_I2C_MODE_MASTER, HAL_I2C_MODE_SLAVE or HAL_I2C_MODE_NONE

- HAL IRDA update

  - Add missing IRDA_CLEAR_IDLEF definition for IDLE flag clear with __HAL_IRDA_CLEAR_FLAG()

- HAL SD update

  - Fix SD card capacity calculation for cards with capacity over 4GB in HAL_SD_Get_CardInfo()

- HAL SMARTCARD update

  - Add missing SMARTCARD_STOPBITS_0_5 definition for frame with 0.5 stop bit
  - HAL SMARTCARD guardtime correction to not expect a minimum of 12 etu

- HAL UART update

  - Add missing UART_STOPBITS_0_5 definition for frame with 0.5 stop bit
  - RX Buffer flush request should not be called at each RXNE processing
  - Fix wrong macro used in assert_param in HAL_LIN_SendBreak()

- HAL USART update

  - Add missing USART_STOPBITS_0_5 definition for frame with 0.5 stop bit

LL drivers changes

- LL UTILS update (user code impacted!)

  - Move the following functions declaration from stm32l4xx_ll_utils.h to stm32l4xx_ll_utils.c file

  - LL_mDelay(), LL_Init1msTick() and LL_SetSystemCoreClock()

- LL ADC update

  - FLAG & IT definition name change

- LL COMP update

  - Rename InputInverting and InputNonInverting APIs

    - LL_COMP_Set{/Get}InputNonInverting() renamed to LL_COMP_Set{/Get}InputMinus
    - LL_COMP_Set{/Get}InputInverting() renamed to LL_COMP_Set{/Get}InputPlus

  - Remove LL_COMP_SetWindowMode() and LL_COMP_GetWindowMode()

- LL DMA update

  - Add helper macro __LL_DMA_GET_CHANNEL_INSTANCE()

- LL GPIO update

  - Fix definition LL_GPIO_OUTPUT_OPENDRAIN
  - Add the explicit possible values in the API description of LL_GPIO_GetPinMode(), LL_GPIO_GetPinOutputType(), LL_GPIO_GetPinSpeed(), LL_GPIO_GetPinPull(), LL_GPIO_GetAFPin_0_7() and LL_GPIO_GetAFPin_8_15()
  - Add GPIO speed definitions LL_GPIO_SPEED_FREQ_LOW, LL_GPIO_SPEED_FREQ_MEDIUM, LL_GPIO_SPEED_FREQ_HIGH and LL_GPIO_SPEED_FREQ_VERY_HIGH to align with HAL GPIO

- LL I2C update

  - Add missing function LL_I2C_ConfigFilters() to configure noise filters

- LL LPTIM update

  - Add missing functions

    - LL_LPTIM_IsEnabled()
    - LL_LPTIM_SetWaveform()
    - LL_LPTIM_SetPolarity()

- LL OPAMP update

  - Rename power range APIs

    - LL_OPAMP_Get{/Set}PowerRange() renamed to LL_OPAMP_Get{/Set}CommonPowerRange()

- LL SPI update

  - Fix LL_SPI_IsEnabled(), LL_SPI_IsEnabledCRC() and LL_SPI_IsEnabledNSSPulse()
  - Remove LL_SPI_Set{/Get}HalfDuplexDirection() functions: this is managed with TransferDirection parameter in LL_SPI_Set{/Get}TransferDirection()

- LL SWPMI update

  - Add missing function LL_SWPMI_IsActivated()

- LL TIM update

  - Add missing functions

    - LL_TIM_CC_IsEnabledChannel()
    - LL_TIM_OC_IsEnabledFast(), LL_TIM_OC_IsEnabledPreload() and LL_TIM_OC_IsEnabledClear()
    - LL_TIM_IsEnabledMasterSlaveMode()
    - LL_TIM_EnableExternalClock(), LL_TIM_DisableExternalClock() and LL_TIM_IsEnabledExternalClock()

- LL USART update

  - Add LL_USART_STOPBITS_0_5 definition for usage in LL_USART_Set{/Get}StopBitsLength() and LL_USART_ConfigCharacter()

V1.2.0 / 25-November-2015

## Main Changes

- HAL generic update
  - Reduce default HSE startup timeout value to 100ms in Inc\stm32l4xx_hal_conf_template.h file
- HAL PWR update (User application code impacted)
  - Stop 1 with main regulator renamed into Stop 0, to be aligned with latest version of Reference Manual
  - Change HAL_PWREx_EnterSTOP1Mode(uint32_t Regulator, uint8_t STOPEntry) into HAL_PWREx_EnterSTOP1Mode(uint8_t STOPEntry)
  - Application code using HAL_PWREx_EnterSTOP1Mode(PWR_LOWPOWERREGULATOR_ON, STOPEntry) must be updated to use HAL_PWREx_EnterSTOP1Mode(STOPEntry)
  - Add new API HAL_PWREx_EnterSTOP0Mode(uint8_t STOPEntry)
  - Application code using HAL_PWREx_EnterSTOP1Mode(PWR_MAINREGULATOR_ON, STOPEntry) must be updated to use HAL_PWREx_EnterSTOP0Mode(STOPEntry)

- HAL OPAMP update

  - Provide capability to run calibration despite PGA mode by switching temporary to standalone mode
- HAL SAI update

  - update SAI block synchronization selection (User application code impacted)

  - Replace incomplete SAI_SYNCHRONOUS_EXT value for with SAI_SYNCHRONOUS_EXT_SAI1 and SAI_SYNCHRONOUS_EXT_SAI2

  - Update external synchronization input selection (User application code impacted)

  - Remove useless SAI_SYNCEXT_IN_ENABLE value for SynchroExt field in SAI_InitTypeDef structure

  - Add support of 24bits configuration in PCM protocol

  - Add codec not ready interrupt management

  - Fix computation of data size, frame length, active frame length, slot size and first bit offset in I2S protocol

  - Fix mute counter setting in HAL_SAI_EnableRxMuteMode()

  - Fix ambiguous clock strobing values: fix HAL_SAI_Init() to set correct CKSTR bits in SAI_xCR1 according to ClockStrobing and AudioMode parameters

  - Fill in the Fifo before enable interrupt in HAL_SAI_Transmit_IT()

  - Fix assert on active slot selection in HAL_SAI_Init()

  - Fix companding mode management in HAL_SAI_Init()

- HAL TSC update

  - Improve IODefault state management

- HAL NOR/HAL SRAM/FMC update

  - WriteFifo field of FMC_NORSRAM_InitTypeDef structure is not applicable on STM32L47x/STM32L48x devices

- LL PWR update (User application code impacted)

  - LL PWR API change to add new Stop 0 mode and update Stop 1 mode definition

  - Change LL_PWR_SetPowerMode(uint32_t LowPowerMode) possible LowPowerMode]{style=“font-style: italic;”} values** update

  - LL_PWR_MODE_STOP1_LP_REGU renamed into LL_PWR_MODE_STOP1

  - Application code using LL_PWR_SetPowerMode(LL_PWR_MODE_STOP1_LP_REGU) must be updated to use LL_PWR_SetPowerMode(LL_PWR_MODE_STOP1)

  - LL_PWR_MODE_STOP1_MAIN_REGU renamed into LL_PWR_MODE_STOP0

  - Application code using LL_PWR_SetPowerMode(LL_PWR_MODE_STOP1_MAIN_REGU) must be updated to use LL_PWR_SetPowerMode(LL_PWR_MODE_STOP0)

V1.1.1 / 16-October-2015

## Main Changes

- HAL generic update

  - Fine tuning of Inc\stm32l4xx_hal_conf_template.h file to keep Flash prefetch off as default system configuration (PREFETCH_ENABLE set to 0)

- HAL TIM update

  - Removed useless assert_param() macro check on input parameters in HAL_TIM_OC_ConfigChannel(), HAL_TIM_PWM_ConfigChannel() and HAL_TIM_ConfigClockSource(),

- LL ADC update

  - Fix LL_ADC_GetAnalogWDMonitChannels() for AWD2 and AWD3

- LL RCC update

  - Add new API LL_RCC_LSE_DisableCSS()

- LL UTILS update

  - Fix LL_GetPackageType()

V1.1.0 / 26-September-2015

## Main Changes

Add Low Layer drivers allowing performance and footprint optimization

- Low Layer drivers APIs provide register level programming: they require deep knowledge of peripherals described in STM32L4x6 Reference Manual

- Low Layer drivers are available for: ADC, COMP, Cortex, CRC, DAC, DMA, EXTI, GPIO, I2C, IWDG, LPYIM, LPUART, OPAMP, PWR, RCC, RNG, RTC, SPI, SWPMI, TIM, USART, WWDG peripherals and additional Low Level Bus, System and Utilities APIs.

- Low Layer drivers APIs are implemented as static inline function in new Inc/stm32l4xx_ll_ppp.h files for PPP peripherals, there is no configuration file and each stm32l4xx_ll_ppp.h file must be included in user code.

## Contents

- HAL ADC update

  - Channel 5 is not usable for ADC3

- HAL CAN update

  - Update HAL_CAN_IRQHandler() to clear ERRI bit prior to call HAL_CAN_ErrorCallback()

- HAL COMP update

  - Update HAL_COMP_Init() for low power optimization in case of COMP_INVERTINGINPUT_VREFINT

- HAL CRC update

  - Add new API HAL_CRYPEx_ProcessSuspend()

- HAL DMA update

  - Update HAL_DMA_IRQHandler() to set HAL_DMA_ERROR_TE error bit in handle ErrorCode field

- HAL FLASH update

  - Add option byte OB_USER_nRST_SHDW to be used with HAL_FLASHEx_OBProgram()

- HAL GPIO update

  - Rename GPIO speed definitions to GPIO_SPEED_FREQ_LOW, GPIO_SPEED_FREQ_MEDIUM, GPIO_SPEED_FREQ_HIGH and GPIO_SPEED_FREQ_VERY_HIGH
  - Fix macro __HAL_GPIO_EXTI_GENERATE_SWIT()

- HAL PWR update

  - Fix HAL_PWR_DisableWakeUpPin() to clear only appropriate bits in PWR CR3 register
  - Combination of GPIO pins possible in HAL_PWREx_EnableGPIOPullUp(), HAL_PWREx_DisableGPIOPullUp(), HAL_PWREx_EnableGPIOPullDown() and HAL_PWREx_DisableGPIOPullDown()

- HAL RCC update

  - Add LSE Clock Security System (CSS) management with new APIs: HAL_RCCEx_EnableLSECSS_IT(), HAL_RCCEx_LSECSS_IRQHandler() and HAL_RCCEx_LSECSS_Callback()
  - Add RCC_MCO1SOURCE_NOCLOCK to provide capability to disable MCO output in HAL_RCC_MCOConfig()
  - Update HAL_RCC_OscConfig() and HAL_RCCEx_PeriphCLKConfig() to keep backup domain enabled when configuring respectively LSE and RTC clock source
  - Update HAL_RCCEx_DisablePLLSAI1() and HAL_RCCEx_DisablePLLSAI2() to disable respectively PLLSAI1 and PLLSAI2 clock outputs

  - Update HAL_RCCEx_GetPeriphCLKFreq() to return the frequency in Hz applied to peripherals via HAL_RCCEx_PeriphCLKConfig()

  - Update HAL_RCC_DeInit() to set default MSI range

  - Remove old workaround on LSE drive medium configuration values

- HAL SPI update

  - Fix issue to receive CRC in RX 2 lines mode 8-bit dataSize and even buffer size.

- HAL TIM update

  - Fix macro __HAL_TIM_SET_COMPARE()

- HAL UART update

  - Remove enable of Error interrupt in HAL_UART_Transmit_IT()

V1.0.0 / 26-June-2015

## Main Changes

- First official release of STM32L4xx HAL Drivers for STM32L471xx/STM32L475xx/STM32L476xx/STM32L485xx and STM32L486xx devices