# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U575AGIx
GenU5.menu.pnum.GENERIC_U575AGIX=Generic U575AGIx
GenU5.menu.pnum.GENERIC_U575AGIX.upload.maximum_size=1048576
GenU5.menu.pnum.GENERIC_U575AGIX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575AGIX.build.board=GENERIC_U575AGIX
GenU5.menu.pnum.GENERIC_U575AGIX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575AGIX.build.variant=STM32U5xx/U575A(G-I)I_U585AII
GenU5.menu.pnum.GENERIC_U575AGIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575AIIx
GenU5.menu.pnum.GENERIC_U575AIIX=Generic U575AIIx
GenU5.menu.pnum.GENERIC_U575AIIX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U575AIIX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575AIIX.build.board=GENERIC_U575AIIX
GenU5.menu.pnum.GENERIC_U575AIIX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575AIIX.build.variant=STM32U5xx/U575A(G-I)I_U585AII
GenU5.menu.pnum.GENERIC_U575AIIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U585AIIx
GenU5.menu.pnum.GENERIC_U585AIIX=Generic U585AIIx
GenU5.menu.pnum.GENERIC_U585AIIX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U585AIIX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U585AIIX.build.board=GENERIC_U585AIIX
GenU5.menu.pnum.GENERIC_U585AIIX.build.product_line=STM32U585xx
GenU5.menu.pnum.GENERIC_U585AIIX.build.variant=STM32U5xx/U575A(G-I)I_U585AII
GenU5.menu.pnum.GENERIC_U585AIIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U585.svd

