# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L052T6Yx
GenL0.menu.pnum.GENERIC_L052T6YX=Generic L052T6Yx
GenL0.menu.pnum.GENERIC_L052T6YX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L052T6YX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L052T6YX.build.board=GENERIC_L052T6YX
GenL0.menu.pnum.GENERIC_L052T6YX.build.product_line=STM32L052xx
GenL0.menu.pnum.GENERIC_L052T6YX.build.variant=STM32L0xx/L052T6Y_L052T8(F-Y)
GenL0.menu.pnum.GENERIC_L052T6YX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L052.svd

# Generic L052T8Yx
GenL0.menu.pnum.GENERIC_L052T8YX=Generic L052T8Yx
GenL0.menu.pnum.GENERIC_L052T8YX.upload.maximum_size=65536
GenL0.menu.pnum.GENERIC_L052T8YX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L052T8YX.build.board=GENERIC_L052T8YX
GenL0.menu.pnum.GENERIC_L052T8YX.build.product_line=STM32L052xx
GenL0.menu.pnum.GENERIC_L052T8YX.build.variant=STM32L0xx/L052T6Y_L052T8(F-Y)
GenL0.menu.pnum.GENERIC_L052T8YX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L052.svd

# Generic L052T8Fx
GenL0.menu.pnum.GENERIC_L052T8FX=Generic L052T8Fx
GenL0.menu.pnum.GENERIC_L052T8FX.upload.maximum_size=65536
GenL0.menu.pnum.GENERIC_L052T8FX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L052T8FX.build.board=GENERIC_L052T8FX
GenL0.menu.pnum.GENERIC_L052T8FX.build.product_line=STM32L052xx
GenL0.menu.pnum.GENERIC_L052T8FX.build.variant=STM32L0xx/L052T6Y_L052T8(F-Y)
GenL0.menu.pnum.GENERIC_L052T8FX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L052.svd

