# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L072KBUx
GenL0.menu.pnum.GENERIC_L072KBUX=Generic L072KBUx
GenL0.menu.pnum.GENERIC_L072KBUX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L072KBUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072KBUX.build.board=GENERIC_L072KBUX
GenL0.menu.pnum.GENERIC_L072KBUX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072KBUX.build.variant=STM32L0xx/L072K(B-Z)U_L082K(B-Z)U
GenL0.menu.pnum.GENERIC_L072KBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072KZUx
GenL0.menu.pnum.GENERIC_L072KZUX=Generic L072KZUx
GenL0.menu.pnum.GENERIC_L072KZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L072KZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072KZUX.build.board=GENERIC_L072KZUX
GenL0.menu.pnum.GENERIC_L072KZUX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072KZUX.build.variant=STM32L0xx/L072K(B-Z)U_L082K(B-Z)U
GenL0.menu.pnum.GENERIC_L072KZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L082KBUx
GenL0.menu.pnum.GENERIC_L082KBUX=Generic L082KBUx
GenL0.menu.pnum.GENERIC_L082KBUX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L082KBUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L082KBUX.build.board=GENERIC_L082KBUX
GenL0.menu.pnum.GENERIC_L082KBUX.build.product_line=STM32L082xx
GenL0.menu.pnum.GENERIC_L082KBUX.build.variant=STM32L0xx/L072K(B-Z)U_L082K(B-Z)U
GenL0.menu.pnum.GENERIC_L082KBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L082KZUx
GenL0.menu.pnum.GENERIC_L082KZUX=Generic L082KZUx
GenL0.menu.pnum.GENERIC_L082KZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L082KZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L082KZUX.build.board=GENERIC_L082KZUX
GenL0.menu.pnum.GENERIC_L082KZUX.build.product_line=STM32L082xx
GenL0.menu.pnum.GENERIC_L082KZUX.build.variant=STM32L0xx/L072K(B-Z)U_L082K(B-Z)U
GenL0.menu.pnum.GENERIC_L082KZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

