# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L475RCTx
GenL4.menu.pnum.GENERIC_L475RCTX=Generic L475RCTx
GenL4.menu.pnum.GENERIC_L475RCTX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L475RCTX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L475RCTX.build.board=GENERIC_L475RCTX
GenL4.menu.pnum.GENERIC_L475RCTX.build.product_line=STM32L475xx
GenL4.menu.pnum.GENERIC_L475RCTX.build.variant=STM32L4xx/L475R(C-E-G)T_L476R(C-E-G)T_L486RGT
GenL4.menu.pnum.GENERIC_L475RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L475.svd

# Generic L475RETx
GenL4.menu.pnum.GENERIC_L475RETX=Generic L475RETx
GenL4.menu.pnum.GENERIC_L475RETX.upload.maximum_size=524288
GenL4.menu.pnum.GENERIC_L475RETX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L475RETX.build.board=GENERIC_L475RETX
GenL4.menu.pnum.GENERIC_L475RETX.build.product_line=STM32L475xx
GenL4.menu.pnum.GENERIC_L475RETX.build.variant=STM32L4xx/L475R(C-E-G)T_L476R(C-E-G)T_L486RGT
GenL4.menu.pnum.GENERIC_L475RETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L475.svd

# Generic L475RGTx
GenL4.menu.pnum.GENERIC_L475RGTX=Generic L475RGTx
GenL4.menu.pnum.GENERIC_L475RGTX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L475RGTX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L475RGTX.build.board=GENERIC_L475RGTX
GenL4.menu.pnum.GENERIC_L475RGTX.build.product_line=STM32L475xx
GenL4.menu.pnum.GENERIC_L475RGTX.build.variant=STM32L4xx/L475R(C-E-G)T_L476R(C-E-G)T_L486RGT
GenL4.menu.pnum.GENERIC_L475RGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L475.svd

# Generic L476RCTx
GenL4.menu.pnum.GENERIC_L476RCTX=Generic L476RCTx
GenL4.menu.pnum.GENERIC_L476RCTX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L476RCTX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L476RCTX.build.board=GENERIC_L476RCTX
GenL4.menu.pnum.GENERIC_L476RCTX.build.product_line=STM32L476xx
GenL4.menu.pnum.GENERIC_L476RCTX.build.variant=STM32L4xx/L475R(C-E-G)T_L476R(C-E-G)T_L486RGT
GenL4.menu.pnum.GENERIC_L476RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L476.svd

# Generic L476RETx
GenL4.menu.pnum.GENERIC_L476RETX=Generic L476RETx
GenL4.menu.pnum.GENERIC_L476RETX.upload.maximum_size=524288
GenL4.menu.pnum.GENERIC_L476RETX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L476RETX.build.board=GENERIC_L476RETX
GenL4.menu.pnum.GENERIC_L476RETX.build.product_line=STM32L476xx
GenL4.menu.pnum.GENERIC_L476RETX.build.variant=STM32L4xx/L475R(C-E-G)T_L476R(C-E-G)T_L486RGT
GenL4.menu.pnum.GENERIC_L476RETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L476.svd

# Generic L476RGTx
GenL4.menu.pnum.GENERIC_L476RGTX=Generic L476RGTx
GenL4.menu.pnum.GENERIC_L476RGTX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L476RGTX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L476RGTX.build.board=GENERIC_L476RGTX
GenL4.menu.pnum.GENERIC_L476RGTX.build.product_line=STM32L476xx
GenL4.menu.pnum.GENERIC_L476RGTX.build.variant=STM32L4xx/L475R(C-E-G)T_L476R(C-E-G)T_L486RGT
GenL4.menu.pnum.GENERIC_L476RGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L476.svd

# Generic L486RGTx
GenL4.menu.pnum.GENERIC_L486RGTX=Generic L486RGTx
GenL4.menu.pnum.GENERIC_L486RGTX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L486RGTX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L486RGTX.build.board=GENERIC_L486RGTX
GenL4.menu.pnum.GENERIC_L486RGTX.build.product_line=STM32L486xx
GenL4.menu.pnum.GENERIC_L486RGTX.build.variant=STM32L4xx/L475R(C-E-G)T_L476R(C-E-G)T_L486RGT
GenL4.menu.pnum.GENERIC_L486RGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L486.svd

