# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L052R6Tx
GenL0.menu.pnum.GENERIC_L052R6TX=Generic L052R6Tx
GenL0.menu.pnum.GENERIC_L052R6TX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L052R6TX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L052R6TX.build.board=GENERIC_L052R6TX
GenL0.menu.pnum.GENERIC_L052R6TX.build.product_line=STM32L052xx
GenL0.menu.pnum.GENERIC_L052R6TX.build.variant=STM32L0xx/L052R(6-8)T_L053R(6-8)T_L063R8T
GenL0.menu.pnum.GENERIC_L052R6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L052.svd

# Generic L052R8Tx
GenL0.menu.pnum.GENERIC_L052R8TX=Generic L052R8Tx
GenL0.menu.pnum.GENERIC_L052R8TX.upload.maximum_size=65536
GenL0.menu.pnum.GENERIC_L052R8TX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L052R8TX.build.board=GENERIC_L052R8TX
GenL0.menu.pnum.GENERIC_L052R8TX.build.product_line=STM32L052xx
GenL0.menu.pnum.GENERIC_L052R8TX.build.variant=STM32L0xx/L052R(6-8)T_L053R(6-8)T_L063R8T
GenL0.menu.pnum.GENERIC_L052R8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L052.svd

# Generic L053R6Tx
GenL0.menu.pnum.GENERIC_L053R6TX=Generic L053R6Tx
GenL0.menu.pnum.GENERIC_L053R6TX.upload.maximum_size=32768
GenL0.menu.pnum.GENERIC_L053R6TX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L053R6TX.build.board=GENERIC_L053R6TX
GenL0.menu.pnum.GENERIC_L053R6TX.build.product_line=STM32L053xx
GenL0.menu.pnum.GENERIC_L053R6TX.build.variant=STM32L0xx/L052R(6-8)T_L053R(6-8)T_L063R8T
GenL0.menu.pnum.GENERIC_L053R6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L053.svd

# Generic L053R8Tx
GenL0.menu.pnum.GENERIC_L053R8TX=Generic L053R8Tx
GenL0.menu.pnum.GENERIC_L053R8TX.upload.maximum_size=65536
GenL0.menu.pnum.GENERIC_L053R8TX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L053R8TX.build.board=GENERIC_L053R8TX
GenL0.menu.pnum.GENERIC_L053R8TX.build.product_line=STM32L053xx
GenL0.menu.pnum.GENERIC_L053R8TX.build.variant=STM32L0xx/L052R(6-8)T_L053R(6-8)T_L063R8T
GenL0.menu.pnum.GENERIC_L053R8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L053.svd

# Generic L063R8Tx
GenL0.menu.pnum.GENERIC_L063R8TX=Generic L063R8Tx
GenL0.menu.pnum.GENERIC_L063R8TX.upload.maximum_size=65536
GenL0.menu.pnum.GENERIC_L063R8TX.upload.maximum_data_size=8192
GenL0.menu.pnum.GENERIC_L063R8TX.build.board=GENERIC_L063R8TX
GenL0.menu.pnum.GENERIC_L063R8TX.build.product_line=STM32L063xx
GenL0.menu.pnum.GENERIC_L063R8TX.build.variant=STM32L0xx/L052R(6-8)T_L053R(6-8)T_L063R8T
GenL0.menu.pnum.GENERIC_L063R8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L063.svd

