# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic C092CBTx
GenC0.menu.pnum.GENERIC_C092CBTX=Generic C092CBTx
GenC0.menu.pnum.GENERIC_C092CBTX.upload.maximum_size=131072
GenC0.menu.pnum.GENERIC_C092CBTX.upload.maximum_data_size=30720
GenC0.menu.pnum.GENERIC_C092CBTX.build.board=GENERIC_C092CBTX
GenC0.menu.pnum.GENERIC_C092CBTX.build.product_line=STM32C092xx
GenC0.menu.pnum.GENERIC_C092CBTX.build.variant=STM32C0xx/C092C(B-C)(T-U)
GenC0.menu.pnum.GENERIC_C092CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C092.svd

# Generic C092CBUx
GenC0.menu.pnum.GENERIC_C092CBUX=Generic C092CBUx
GenC0.menu.pnum.GENERIC_C092CBUX.upload.maximum_size=131072
GenC0.menu.pnum.GENERIC_C092CBUX.upload.maximum_data_size=30720
GenC0.menu.pnum.GENERIC_C092CBUX.build.board=GENERIC_C092CBUX
GenC0.menu.pnum.GENERIC_C092CBUX.build.product_line=STM32C092xx
GenC0.menu.pnum.GENERIC_C092CBUX.build.variant=STM32C0xx/C092C(B-C)(T-U)
GenC0.menu.pnum.GENERIC_C092CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C092.svd

# Generic C092CCTx
GenC0.menu.pnum.GENERIC_C092CCTX=Generic C092CCTx
GenC0.menu.pnum.GENERIC_C092CCTX.upload.maximum_size=262144
GenC0.menu.pnum.GENERIC_C092CCTX.upload.maximum_data_size=30720
GenC0.menu.pnum.GENERIC_C092CCTX.build.board=GENERIC_C092CCTX
GenC0.menu.pnum.GENERIC_C092CCTX.build.product_line=STM32C092xx
GenC0.menu.pnum.GENERIC_C092CCTX.build.variant=STM32C0xx/C092C(B-C)(T-U)
GenC0.menu.pnum.GENERIC_C092CCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C092.svd

# Generic C092CCUx
GenC0.menu.pnum.GENERIC_C092CCUX=Generic C092CCUx
GenC0.menu.pnum.GENERIC_C092CCUX.upload.maximum_size=262144
GenC0.menu.pnum.GENERIC_C092CCUX.upload.maximum_data_size=30720
GenC0.menu.pnum.GENERIC_C092CCUX.build.board=GENERIC_C092CCUX
GenC0.menu.pnum.GENERIC_C092CCUX.build.product_line=STM32C092xx
GenC0.menu.pnum.GENERIC_C092CCUX.build.variant=STM32C0xx/C092C(B-C)(T-U)
GenC0.menu.pnum.GENERIC_C092CCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C092.svd

