# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L476JEYx
GenL4.menu.pnum.GENERIC_L476JEYX=Generic L476JEYx
GenL4.menu.pnum.GENERIC_L476JEYX.upload.maximum_size=524288
GenL4.menu.pnum.GENERIC_L476JEYX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L476JEYX.build.board=GENERIC_L476JEYX
GenL4.menu.pnum.GENERIC_L476JEYX.build.product_line=STM32L476xx
GenL4.menu.pnum.GENERIC_L476JEYX.build.variant=STM32L4xx/L476J(E-G)Y_L485J(C-E)Y_L486JGY
GenL4.menu.pnum.GENERIC_L476JEYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L476.svd

# Generic L476JGYx
GenL4.menu.pnum.GENERIC_L476JGYX=Generic L476JGYx
GenL4.menu.pnum.GENERIC_L476JGYX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L476JGYX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L476JGYX.build.board=GENERIC_L476JGYX
GenL4.menu.pnum.GENERIC_L476JGYX.build.product_line=STM32L476xx
GenL4.menu.pnum.GENERIC_L476JGYX.build.variant=STM32L4xx/L476J(E-G)Y_L485J(C-E)Y_L486JGY
GenL4.menu.pnum.GENERIC_L476JGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L476.svd

# Generic L485JCYx
GenL4.menu.pnum.GENERIC_L485JCYX=Generic L485JCYx
GenL4.menu.pnum.GENERIC_L485JCYX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L485JCYX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L485JCYX.build.board=GENERIC_L485JCYX
GenL4.menu.pnum.GENERIC_L485JCYX.build.product_line=STM32L485xx
GenL4.menu.pnum.GENERIC_L485JCYX.build.variant=STM32L4xx/L476J(E-G)Y_L485J(C-E)Y_L486JGY
GenL4.menu.pnum.GENERIC_L485JCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4x5.svd

# Generic L485JEYx
GenL4.menu.pnum.GENERIC_L485JEYX=Generic L485JEYx
GenL4.menu.pnum.GENERIC_L485JEYX.upload.maximum_size=524288
GenL4.menu.pnum.GENERIC_L485JEYX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L485JEYX.build.board=GENERIC_L485JEYX
GenL4.menu.pnum.GENERIC_L485JEYX.build.product_line=STM32L485xx
GenL4.menu.pnum.GENERIC_L485JEYX.build.variant=STM32L4xx/L476J(E-G)Y_L485J(C-E)Y_L486JGY
GenL4.menu.pnum.GENERIC_L485JEYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4x5.svd

# Generic L486JGYx
GenL4.menu.pnum.GENERIC_L486JGYX=Generic L486JGYx
GenL4.menu.pnum.GENERIC_L486JGYX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L486JGYX.upload.maximum_data_size=131072
GenL4.menu.pnum.GENERIC_L486JGYX.build.board=GENERIC_L486JGYX
GenL4.menu.pnum.GENERIC_L486JGYX.build.product_line=STM32L486xx
GenL4.menu.pnum.GENERIC_L486JGYX.build.variant=STM32L4xx/L476J(E-G)Y_L485J(C-E)Y_L486JGY
GenL4.menu.pnum.GENERIC_L486JGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L486.svd

