# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F105V8Hx
GenF1.menu.pnum.GENERIC_F105V8HX=Generic F105V8Hx
GenF1.menu.pnum.GENERIC_F105V8HX.upload.maximum_size=65536
GenF1.menu.pnum.GENERIC_F105V8HX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F105V8HX.build.board=GENERIC_F105V8HX
GenF1.menu.pnum.GENERIC_F105V8HX.build.product_line=STM32F105xC
GenF1.menu.pnum.GENERIC_F105V8HX.build.variant=STM32F1xx/F105V(8-B)(H-T)_F105VCT
GenF1.menu.pnum.GENERIC_F105V8HX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F105.svd

# Generic F105VBHx
GenF1.menu.pnum.GENERIC_F105VBHX=Generic F105VBHx
GenF1.menu.pnum.GENERIC_F105VBHX.upload.maximum_size=131072
GenF1.menu.pnum.GENERIC_F105VBHX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F105VBHX.build.board=GENERIC_F105VBHX
GenF1.menu.pnum.GENERIC_F105VBHX.build.product_line=STM32F105xC
GenF1.menu.pnum.GENERIC_F105VBHX.build.variant=STM32F1xx/F105V(8-B)(H-T)_F105VCT
GenF1.menu.pnum.GENERIC_F105VBHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F105.svd

# Generic F105V8Tx
GenF1.menu.pnum.GENERIC_F105V8TX=Generic F105V8Tx
GenF1.menu.pnum.GENERIC_F105V8TX.upload.maximum_size=65536
GenF1.menu.pnum.GENERIC_F105V8TX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F105V8TX.build.board=GENERIC_F105V8TX
GenF1.menu.pnum.GENERIC_F105V8TX.build.product_line=STM32F105xC
GenF1.menu.pnum.GENERIC_F105V8TX.build.variant=STM32F1xx/F105V(8-B)(H-T)_F105VCT
GenF1.menu.pnum.GENERIC_F105V8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F105.svd

# Generic F105VBTx
GenF1.menu.pnum.GENERIC_F105VBTX=Generic F105VBTx
GenF1.menu.pnum.GENERIC_F105VBTX.upload.maximum_size=131072
GenF1.menu.pnum.GENERIC_F105VBTX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F105VBTX.build.board=GENERIC_F105VBTX
GenF1.menu.pnum.GENERIC_F105VBTX.build.product_line=STM32F105xC
GenF1.menu.pnum.GENERIC_F105VBTX.build.variant=STM32F1xx/F105V(8-B)(H-T)_F105VCT
GenF1.menu.pnum.GENERIC_F105VBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F105.svd

# Generic F105VCTx
GenF1.menu.pnum.GENERIC_F105VCTX=Generic F105VCTx
GenF1.menu.pnum.GENERIC_F105VCTX.upload.maximum_size=262144
GenF1.menu.pnum.GENERIC_F105VCTX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F105VCTX.build.board=GENERIC_F105VCTX
GenF1.menu.pnum.GENERIC_F105VCTX.build.product_line=STM32F105xC
GenF1.menu.pnum.GENERIC_F105VCTX.build.variant=STM32F1xx/F105V(8-B)(H-T)_F105VCT
GenF1.menu.pnum.GENERIC_F105VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F105.svd

