# Introduction

|  |  |
| --- | --- |
| IP quick facts | |
| Supported device families | Zynq®-7000, 7 series |
| Supported user interfaces | Custom, AXI Stream |
| **Provided with core** | |
| Design files | VHDL |
| Simulation model | **Yes** for AD96xx SPI interface; **No** for the IP itself (it can be simulated using the design files) |
| Constraints file | XDC |
| Software driver | **N**/A |
| **Tested design flows** | |
| Design entry | Vivado Design Suite - ML Editions 2021.1 |
| Synthesis | Vivado Synthesis 2021.1 |
| Implementation | Vivado Implementation 2021.1 |

This user guide describes the Digilent **Zmod SDR Controller** Intellectual Property. This IP interfaces directly with the Zmod SDR 1450 – 122 writing an initial configuration to the analog to digital converter (ADC) featured by these modules and one of the selected frequency configurations of the Clock Generator, demultiplexing the data received over the ADC’s parallel interface and forwarding it to the user logic. The **Zmod SDR** **Controller** is intended to be used as a stand-alone IP (the stand alone mode) in projects that do not require processor interaction or it can be used in conjunction with higher level IPs that may provide connectivity with the processing system.

# Features

* Initializes the hardware on the Zmod SDR 1450 – 122.
* Demultiplexes the double data rate (DDR) parallel interface outputted by the Zmod and exports two single data rate (SDR) channels to the user logic in the user clock domain.
* Provides the possibility of overwriting the initial ADC configuration by providing an optional upper level interface that allows indirect access to the ADC’s SPI interface.
* Configures the Clock Generator to output a clock signal to the ADC with a frequency from a set list

# Performance

This IP is designed to have a configurable width for the data interface and a configurable sampling rate so that it can manage the low-level communication with the Zmods enumerated in chapter 1 (Introduction). The parallel DDR data interface used to communicate with the ADC is 14 bit wide and the sampling rate has a set of 7 predefined values: 50MHz, 80MHz, 100MHz, 110MHz, 120MHz, 122.88MHz and 125MHz. The **Zmod SDR Controller** further exports to the user logic two distinct SDR channels synchronized in the ADC sampling clock domain (*DcoClkOut*).

# Overview

A diagram of a computer system

Description automatically generated

Figure . Zmod SDR Controller block diagram.

The structure of the IP is presented in [Figure 1](#_Overview). The main functionalities are divided as ADC input clock generation, data capture (data path), ADC configuration (two items related to configuration functionalities will be detailed separately: the configuration state machine and the SPI controller) and Clock Generator configuration (state machine and I2C controller).

## Clocking

The IP is divided in 4 clock domains as shown in Figure 1:

The system clock domain (*SysClk100*) clocks the ADC configuration module, the Clock Generator configuration module together with its I2C controller and the SPI controller. The frequency of this clock is expected to be 100MHz. All signals synchronous with *SysClk100* have the prefix “s”.

The ADC input clock (*ClockGenPriRefClk*) is used to clock the primitives responsible with passing the input clock to the Clock Generator which then feeds the ADC with a clock signal. All signals synchronous with *ClockGenPriRefClk* have the prefix “i”.

The DCO clock (*DcoClkIn*) is generated by the ADC and is used to clock the IDDR primitives that demultiplex the ADC incoming DDR data bus through a BUFIO primitive (*DcoBufioClk*). All signals synchronous with the de-skewed version of *DcoClkIn* have the prefix “do” for *DcoClkOut* or “db” for *DcoBufioClk*.

The IP does not constrain the clocks it requires as inputs, except for the DCO clock, therefore clocks need to be constrained in the top-level design either manually or by relying on the auto-derived constraints, if using clock modifying blocks. It is the user’s responsibility to correctly configure the input clocks of this IP.

## Reset

This IP has a single asynchronous reset input with negative polarity (aRst\_n) which resets the logic in all four clock domains. To assure that recovery/removal time of sequential logic is respected, the reset input is distributed to the different clock domains throughout the IP by ResetBridge modules. The ResetBridge modules are responsible with converting the asynchronous reset input in reset signals with synchronous de-assertion (RSD) for each clock domain.

The input reset (aRst\_n) must be asserted for at least 2\**Tslowest*, where *Tslowest* represents the period of the slowest clock input of the IP. After applying a reset, the *sRstBusy* output is asserted by the IP. The user/upper level IP has to wait for *sRstBusy* to be de-asserted in order to safely apply a new reset to the **Zmod SDR Controller**.

## ADC Input Clock Generation

The ADC ICs (AD96xx) on the supported Zmod SDR modules require a differential clock as input. This IP allows a set range of frequencies for this clock while also allowing custom frequency configurations thanks to the Clock Generator that is used to feed a differential clocking signal directly to the ADC. The minimum frequency is limited to 10 MHz, while for the maximum frequency the limit is imposed by the Clock Generator’s maximum output frequency [1], the FPGA’s clocking network limitations [2] and by the ADC capabilities. This IP does not generate these clock frequencies internally, it only instantiates the IO primitives required to pass it further into the FPGA.

The Clock Generator can be configured to use one of two possible differential input reference clocks, a primary reference clock that is meant to come from the FPGA and a secondary reference clock that is hardwired to an XTAL source.

## Data Path (DataPath.vhd)

The data path consists of two stages. First, each bit of the input parallel data bus is passed to an IDDR primitive used to demultiplex the DDR interleaved format exported by the ADC (Figure 2), obtaining two SDR data channels.




Figure . Input data channel demultiplexing

To meet timing requirements a MMCM is used for de-skew purposes. The MMCM is also used to detect the ADC’s DCO clock loss. The Data Path module is implemented as a distinct VHDL module and its parameters and ports are described below:

*Table 1.* Data Path module parameter description

|  |  |
| --- | --- |
| Parameter Name | Description |
| *kSamplingPeriod* | The sampling clock period expressed in ns. The maximum value is limited to 100, while it is the user’s responsibility to determine the minimum value based on the targeted Zmod’s capabilities and the targeted FPGA’s clocking distribution network capabilities. |
| *kADC\_Width* | ADC resolution (number of bits). This parameter ranges from 10 to 16. |

*Table 2.* Data Path port description

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Signal Name | Interface | Signal Type | Init State | Description |
| *RefClk* | - | I | N/A | Reference clock. |
| *arRst* | - | I | N/A | Active high reset (can be asynchronously de-asserted but synchronously asserted in the RefClk domain). |
| *DcoClkIn* | - | I | N/A | Connected directly to the Zmod’s AD96xx DCO output clock. |
| *DcoClkOut* | - | O | N/A | The Zmod’s AD96xx DCO output clock forwarded to the IP's top-level module (the de-skew block output). |
| *doEnableAcquisition* | - | I | N/A | When logic '1', this signal enables data acquisition from the ADC. This signal should be kept in logic '0' until the downstream IP (e.g. DMA controller) is ready to receive the ADC data. Once this signal has been set to logic ‘1’, it should be kept in this state and never de-asserted. |
| *adoRst* | - | I | N/A | Reset signal asynchronously de-asserted and synchronously asserted (in the DcoClkOut domain). |
| *rDcoMMCM\_LockState* | - | O | N/A | MMCM Locked output signal synchronized on RefClk. |
| *diADC\_Data[kADC\_Width-1 : 0]* | - | I | N/A | *kADC\_Width* bit wide DDR parallel data bus exported by ADC containing Channel1 and Channel 2 interleaved samples. |
| *doChannelA[kADC\_Width-1 : 0]* | - | O | N/A | The demultiplexed ADC’s Channel A data output synchronized in the DcoClkOut domain. |
| *doChannelB[kADC\_Width-1 : 0]* | - | O | N/A | The demultiplexed ADC’s Channel B data output synchronized in the DcoClkOut domain. |
| *doDataOutValid* | - | O | N/A | Channel A & B data valid indicator. |

## ADC Configuration (ConfigADC.vhd)

The ADC Configuration block sends a predefined list of SPI commands to the Zmod SDR, performing the ADC initialization, and manages the SPI Indirect Access Port (IAP). The ports and parameters of the ADC configuration block, which is implemented as a distinct VHDL module are listed below:

*Table 5.* ADC Configuration parameter description

|  |  |
| --- | --- |
| Parameter Name | Description |
| *kZmodID* | Parameter identifying the targeted Zmod. See Table 13 for more details. |
| *kDataWidth* | The number of data bits for the data phase of the transaction: only 8 data bits currently supported, parameter provided for future development. |
| *kCommandWidth* | The number of bits of the command phase of the SPI transaction. |

*Table 6.* ADC Configuration port description

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Signal Name | Interface | Signal Type | Init State | Description |
| *SysClk100* | - | I | N/A | 100MHz input clock signal. |
| *asRst\_n* | - | I | N/A | Active low reset (can be asynchronously asserted but synchronously de-asserted). |
| *sADC\_Sclk* | SPI | O | N/A | Output SPI clock. Signal managed by the SPI controller. More details in section 4.9. |
| *sADC\_SDIO* | SPI | IO | N/A | 2 Wire SPI interface SDIO signal. Signal managed by the SPI controller. More details in section 4.9. |
| *sADC\_CS* | SPI | O | N/A | 2 Wire SPI interface CS signal. Signal managed by the SPI controller. More details in section 4.9. |
| *sInitDoneADC* | - | O | N/A | Flag indicating when the Zmod’s ADC initialization is complete. |
| *sConfigError* | - | O | N/A | This flag is asserted if the ADC initialization fails. An IP reset is required to clear this flag. |
| *sConfigADCEnable* | - | I | N/A | ADC initialization enable signal. Configuration of the ADC over SPI should be done after sConfigADCEnable is asserted which only happens after the CDCE clock generator is configured and the PLL inside the CDCE is locked, otherwise the ADC configuration state machine should be kept in reset. |
| *sCmdTxAxisTdata[31:0]* | SPI IAP | I | N/A | IAP command TX interface (AXI Stream) data port. |
| *sCmdTxAxisTvalid* | SPI IAP | I | N/A | IAP command TX interface (AXI Stream) valid signal. |
| *sCmdTxAxisTready* | SPI IAP | O | N/A | IAP command TX interface (AXI Stream) ready signal. |
| *sCmdRxAxisTdata[31:0]* | SPI IAP | O | N/A | IAP command RX interface (AXI Stream) data port. |
| *sCmdRxAxisTvalid* | SPI IAP | O | N/A | IAP command RX interface (AXI Stream) valid signal. |
| *sCmdRxAxisTready* | SPI IAP | I | N/A | IAP command RX interface (AXI Stream) ready signal. |

Once the initialization is complete, the state machine of the ADC configuration block enters the idle state where it monitors if there is any valid data on the upper level SPI command interface named the SPI Indirect Access port (IAP). After executing the requested SPI transfers, the state machine passes the received SPI data (for read commands) and returns to the idle state. The SPI IAP is optional, and it can be enabled by setting the *kExtCmdInterfaceEn* to “true”. It is designed to interface with two AXI StreamFIFOs, one that stores commands to be transmitted (command queue TX FIFO) and one to store the received data (command RX FIFO). Thus, the IAP consists of two AXI Stream interfaces: the IAP command TX interface and the IAP RX command interface. Each element of the command queue should be represented on 32 bits, having the following format:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 31 24 | 23 | 22 21 | 20 8 | 7 0 |
| - | Read/Write | Width | Address | Data |

|  |  |  |
| --- | --- | --- |
| **Bits** | **Field Name** | **Description** |
| 23 | Read/Write | Write this bit to 1 for a read command and to 0 for a write command |
| 22-21 | Width | Only 1 byte SPI transfers are supported. This field should be always 0h. |
| 20-8 | Address | ADC SPI register address |
| 7-0 | Data | Data byte to be sent to the AD9648. Ignored for read operations |

The ADC Configuration state machine, when in the idle state, monitors the valid signal of the IAP command TX interface (*sCmdTxAxisTvalid*) and, if asserted and if the SPI controller can process a new command (not busy), the ready signal of the IAP command TX interface is asserted for one SysClk100 clock cycle. Write commands only consist of a single transaction on the IAP command TX interface. For read commands, after passing the register read request to the SPI controller and the request successfully completes, the ADC Configuration state machine asserts the valid signal of the IAP command RX interface (*sCmdRxAxisTvalid*) and places the register read data on the data port of the interface (*sCmdRxAxisTdata*). The ADC Configuration state machine waits for the upper layer IP to assert the ready signal on the IAP command interface (*sCmdRxAxisTready*) before it transitions to the idle state.

The initialization configuration command sequence is listed below. After configuring each register, the register data is read back and checked against the expected value in order to determine any SPI transaction error.

1. **SPI Port config register**: Soft Reset (Address: 00h; Data: 3C).
2. **Chip ID Register**: Check ID (Read, Address: 01h; Data: -).
3. **Device Index Register**: Select CHA (Address: 05h; Data: 01h).
4. **Power modes Register**: Digital reset (Address: 08h; Data: 03h).
5. **Output mode register**: Output port logic type -> CMOS 1.8V, output interleave enable, disable port (port A), output invert disable, 2’s complement (Address: 14h; Data: 31h).
6. **Device Index Register**: Select CHB (Address: 05h; Data: 01h).
7. **Power modes Register**: Digital reset (Address: 08h; Data: 03h).
8. **Output mode register**: Output port logic type -> CMOS 1.8V, output interleave enable, enable port (port B), output invert disable, 2’s complement (Address: 14h; Data: 21h).
9. **Device Index Register**: Select none (Address: 05h; Data: 00h).
10. **Clock Phase Control register**: Invert DCO (Address: 16h; Data: 80h).
11. **Clock Divide register**: Divide input clock by ADC\_ClkDiv (Address: 0Bh; Data: ADC\_ClkDiv).
12. **Overrange Control register**: Disable overrange output (Address: 2Ah; Data: 00h).
13. **Output Adjust register**: DCO and DATA 2X drive strength (Address: 15h; Data: 00h).
14. **Output delay register**: 1.12ns delay added to DCO (Address: 17h; Data: 81h).
15. **Sync control register**: SYNC enable, continuous SYNC (Address: 3Ah; Data: 02h).
16. **Device Index Register:** Select CHA (Address: 05h; Data: 01h).
17. **Power modes:** Normal operation (Address: 08h; Data: 00h).
18. **Device Index Register:** Select CHB (Address: 05h; Data: 02h).
19. **Power modes:** Normal operation (Address: 08h; Data: 00h).
20. **Device Index Register**: Select none (Address: 05h; Data: 00h).

## SPI Controller (ADI\_SPI.vhd)

The SPI controller is designed to carry out basic register access over the Analog Devices 2 wire SPI interface. The controller’s parameters and ports are listed below:

*Table 7.* SPI controller parameter description

|  |  |
| --- | --- |
| Parameter Name | Description |
| *kSysClkDiv* | The *sSPI\_Clk* signal is obtained by dividing SysClk100 to 2kSysClkDiv. |
| *kDataWidth* | The number of data bits for the data phase of the transaction: only 8 data bits currently supported, parameter provided for future development. |
| *kCommandWidth* | The number of bits of the command phase of the SPI transaction. |

*Table 8.* SPI controller port description

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Signal Name | Interface | Signal Type | Init State | Description |
| *SysClk100* | - | I | N/A | 100MHz input clock signal. |
| *asRst\_n* | - | I | N/A | Active low reset (can be asynchronously asserted but synchronously de-asserted). |
| *sSPI\_Clk* | SPI | O | N/A | Output SPI clock [4] divided from *SysClk100*. Connected directly to the corresponding Zmod port. |
| *sSDIO* | SPI | IO | N/A | 2 Wire SPI interface SDIO signal [4]. Connected directly to the corresponding Zmod port. |
| *sCS* | SPI | O | N/A | 2 Wire SPI interface CS signal [4]. Connected directly to the corresponding Zmod port. |
| *sApStart* | - | I | N/A | A pulse on this input initiates the transfers. When asserted, the inputs of the upper layer interface are also registered. |
| *sRdData[kDataWidth-1 : 0]* | - | O | N/A | SPI register read received data |
| *sWrData[kDataWidth-1 : 0]* | - | I | N/A | SPI register write data. |
| *sAddr[kCommandWidth - 4:0]* | - | I | N/A | SPI instruction phase address. |
| *sWidth[1:0]* | - | I | N/A | SPI instruction phase word length. The only value currently supported is 0 (1 data byte transferred). |
| *sRdWr* | - | I | N/A | Encodes the requested transaction type:  ‘1’ - read transaction.  ‘0’ – write transaction. |
| *sDone* | - | O | N/A | Indicates that the operation requested has completed and that the data placed on the *sRdData* port is valid. |
| *sBusy* | - | O | N/A | Indicates when a new command can be processed. It is de-asserted only when the internal state machine of the SPI Controller is in the idle state and it is asserted at any other time. *sApStart* is ignored while this signal is asserted. |

An SPI transaction is triggered by generating a pulse on the *sApStart* input. When the pulse is detected, the inputs of the upper layer interface are also registered. The *sRdWr* signal encodes the type of the transaction (read/write). The SPI controller further constructs the command word and the data word based on the module’s inputs and formats them on the SPI bus as requested by the Analog Devices’ specifications [4]. For read operations, the received data is outputted on the *sRdData* port and can be read by the upper layer module when the *sDone* signal pulses high. When the SPI controller returns to the idle state and is ready to process new commands, the *sBusy* output signal is de-asserted. The *sApStart* signal is ignored while *sBusy* is asserted. The width of the command word is configurable through the *kCommandWidth* generic. The frequency of the SPI output clock is obtained by dividing the controller’s input clock frequency by a factor of 2*kSysClkDiv* (*kSysClkDiv* is also a generic). Only single byte data transfers are currently supported. More details about the SPI interface of the supported ADCs can be found in [4].

## Clock Generator Configuration (ConfigClockGen.vhd)

The Clock Generator Configuration block sends a predefined list of I2C commands to the Clock Generator that feeds the ADC a differential clocking signal source. From the IP GUI the user can select from a set of frequency configurations. The possibility of adding custom frequency configurations is open to the user, however, it requires advanced knowledge of the IP, the clock generator and the proprietary software that must be used to generate said custom frequency configurations.

The REFSEL signal is used to select between the two reference clock inputs of the Clock Generator, a value of ‘0’ selects the secondary reference input while a value of ‘1’ selects the primary one which comes from the FPGA and is a tri-level output signal. This reference clock selection can also be done irrespective of the value of the signal by writing 0x02 for SECREF or 0x03 for PRIREF to the REFSEL\_SW register bit field of R2.

The set values of output frequencies provided all use the XTAL input as reference clock and that is not dependent on the value of the REFSEL signal because the Clock Generator’s REFSEL\_SW register bit field is set to 0x02 and the REFSEL signal is kept in tristate.

The configuration of the Clock Generator registers can also be done via its internal 2 Page EEPROM and the pages can be written and rewritten over I2C. The signal that acts as page select is called HW\_SW\_CTRL and is also a tri-level output pin.

By default, the Clock Generator is configured to run in Fall-Back Mode (0x67 in 7-bit format or 0xCE in 8-bit format), a mode in which the I2C serial interface is always enabled and the configurations written inside the EEPROM are ignored. This is done by forcing the REFSEL and HW\_SW\_CTRL output signals to be in High-Z state through the use of an OBUFT FPGA primitive. **This means that the user should not add any kind of pull-up or pull-down on those signals as it would disrupt their functionality.** The other modes involve its configuration being read from an internal factory programmed 2 Page EEPROM which can have frequency configurations unsupported by this IP.

*Table 9.* Clock Generator Configuration parameter description

|  |  |
| --- | --- |
| Parameter Name | Description |
| *kCDCE\_SimulationConfig* | Clock Generator I2C parameter for enabling a shortened configuration for simulation purposes. |
| *kCDCE\_SimulationCmdTotal* | Clock Generator I2C shortened configuration number of commands to send over I2C for simulation purposes. |
| *kCDCEI2C\_Addr* | Clock Generator 7-bit I2C address (0x67 (Fall-Back Mode), 0x68(Default Mode), 0x69). |
| *kRefSel* | Clock Generator input reference clock selection parameter ('0' selects SECREF(XTAL) and '1' selects PRIREF(FPGA)). Only matters when the Clock Generator is not in Fall-Back Mode. |
| *kHwSwCtrlSel* | Clock Generator EEPROM Page selection parameter ('0' selects Page 0 and '1' selects Page 1). Only matters when the Clock Generator is not in Fall-Back Mode. |
| *kFreqSel* | Parameter identifying the CDCE output frequency with SECREF(XTAL) as reference frequency:  -- 0 -> 122.88MHz  -- 1 -> 50MHz  -- 2 -> 80MHz  -- 3 -> 100MHz  -- 4 -> 110MHz  -- 5 -> 120MHz  -- 6 -> 125MHz |

*Table 10.* Clock Generator Configuration port description

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Signal Name | Interface | Signal Type | Init State | Description |
| *RefClk* | - | I | N/A | 100MHz input clock signal. |
| *arRst* | - | I | N/A | Active high reset (can be synchronously asserted but asynchronously de-asserted). |
| *rInitConfigDoneClockGen* | - | O | N/A | Clock Generator configuration done successfully signal. |
| *aCG\_PLL\_Lock* | - | I | N/A | Clock Generator PLL lock signal sent via the GPIO1 or GPIO4 port. |
| *rPLL\_LockClockGen* | - | O | N/A | Clock Generator PLL lock signal sent via the GPIO1 or GPIO4 port and synchronized in the RefClk domain. |
| *rConfigADCEnable* | - | O | N/A | rConfigADCEnable is used to hold the ConfigADC module in reset until the Clock Generator is configured and locked. |
| *REFSEL* | - | O | Z | Clock Generator reference selection signal (low selects SECREF (XTAL) and high selects PRIREF (FPGA)). When High-Z selection is determined by register value. |
| *HW\_SW\_CTRL* | - | O | Z | Clock Generator EEPROM Page selection signal (low selects Page 0 and high selects Page 1). When High-Z selection is determined by register value. |
| *rPDNout\_n* | - | O | L | Clock Generator power down signal. Resets the internal circuitry and is used in the initial power-up sequence. |
| *s\_scl\_i* | I2C | I | Z | I2C Serial Clock Input from 3-state buffer. |
| *s\_scl\_o* | I2C | O | L | I2C Serial Clock Output to 3-state buffer. |
| *s\_scl\_t* | I2C | T | N/A | I2C Serial Clock Output Enable to 3-state buffer. |
| *s\_sda\_i* | I2C | I | Z | I2C Serial Data Input from 3-state buffer. |
| *s\_sda\_o* | I2C | O | L | I2C Serial Data Output to 3-state buffer. |
| *s\_sda\_t* | I2C | T | N/A | I2C Serial Data Output Enable to 3-state buffer. |

# IP Top-Level Parameter Description

*Table 11.* IP core parameter descriptions.

|  |  |
| --- | --- |
| Signal Name | Description |
| *kZmodID* | Parameter identifying the targeted Zmod. See Table 13 for more details. |
| *kADC\_Width* | ADC resolution (number of bits). It is automatically computed based on *kZmodID*. |
| *kExtCmdInterfaceEn* | Enables the upper layer IP SPI configuration interface. Set to “true” when the IP core is expected to be interfaced with the processing system through a high level IP. This will enable the processor to access the Zmod SDR SPI interface and to change the ADC settings if desired. Set to “false” when initial configuration described in Section 4.8 is sufficient. |
| *kCG\_SimulationConfig* | Clock Generator I2C shortened config for simulation purposes. |
| *kCG\_SimulationCmdTotal* | Clock Generator I2C shortened configuration number of commands to send over I2C for simulation purposes, range should have been 0 to kCDCE\_RegNrZeroBased := kCDCE\_RegNrZeroBased, however Vivado IP GUI does not accept expressions. |
| *kCGI2C\_Addr* | Clock Generator 7-bit I2C config address (0x67 (Fall-Back Mode), 0x68(Default Mode), 0x69). |
| *kRefSel* | Clock Generator input reference clock selection parameter ('0' selects SECREF(XTAL) and '1' selects PRIREF(FPGA)). Only relevant when the Clock Generator is not in Fall-Back Mode. |
| *kHwSwCtrlSel* | Clock Generator EEPROM Page selection parameter ('0' selects Page 0 and '1' selects Page 1). Only relevant when the Clock Generator is not in Fall-Back Mode. |
| *kCDCEFreqSel* | Parameter identifying the CDCE output frequency with SECREF(XTAL) as reference frequency, range should have been 0 to CDCE\_I2C\_Cmds'length, however Vivado IP GUI does not accept expressions:  -- 0 -> 122.88MHz  -- 1 -> 50MHz  -- 2 -> 80MHz  -- 3 -> 100MHz  -- 4 -> 110MHz  -- 5 -> 120MHz  -- 6 -> 125MHz |

# IP Top-Level Port Description

A screenshot of a computer program

Description automatically generated

Figure : Zmod SDR Controller IP

*Table 12.* IP core port description

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Signal Name | Interface | Signal Type | Init State | Description |
| *SysClk100* | - | I | N/A | 100MHz input clock signal. |
| *DcoClkIn* | - | I | N/A | Sampling clock. The frequency range supported is between 10MHz and the maximum frequency supported by the Zmod/target FPGA clock distribution network. Clock generated by the ADC synchronous with diZmodSDR\_Data [4]. |
| *ClockGenPriRefClk* | - | I | N/A | Clock Generator primary input reference clock signal. By default, the Clock Generator uses its secondary input reference clock. This input clock signal is completely optional. |
| *sInitDoneClockGen* | - | O | L | Clock Generator config done successful signal. |
| *sPLL\_LockClockGen* | - | O | L | Clock Generator PLL lock signal sent via the GPIO1 or GPIO4 port and synchronized in the SysClock100 domain. |
| *aRst\_n* | - | I | N/A | Asynchronous reset of negative polarity which resets the logic in all four clock domains. Must be asserted for at least 2\**Tslowest*- see section 4.2 for details. |
| *sRstBusy* | - | O | N/A | Reset busy flag. While this signal is asserted it is not recommended to apply a new reset to the IP. The user/upper level IP must wait for this signal to de-assert in order to apply a new reset. |
| *sInitDoneADC* | - | O | N/A | Flag indicating when the Zmod’s ADC initialization is complete. |
| *sConfigError* | - | O | N/A | This flag is asserted if the ADC initialization fails. An IP reset is required to clear this flag. |
| *sEnableAcquisition* | - | I | N/A | When logic '1', this signal enables data acquisition from the ADC. This signal should be kept in logic '0' until the downstream IP (e.g. DMA controller) is ready to receive the ADC data.  Once this signal has been set to logic ‘1’, it should be kept in this state and never de-asserted. |
| *doDataAxisTdata[31:0]* | Data interface | O | N/A | (Master) AXI Stream Data interface TDATA port. Channel1 and Channel2 data are concatenated as follows:  Channel1 -> doDataAxisTdata[31:16].  Channel2 -> doDataAxisTdata[15:0]. |
| *doDataAxisTvalid* | Data interface | O | N/A | (Master) AXI Stream Data interface TVALID signal. |
| *doDataAxisTready* | Data interface | I | N/A | (Master) AXI Stream Data interface TREADY signal. |
| *sCmdTxAxisTdata[31:0]* | SPI IAP | I | N/A | IAP command TX interface (Slave AXI Stream) data port. For more information see section 4.8. |
| *sCmdTxAxisTvalid* | SPI IAP | I | N/A | IAP command TX interface (Slave AXI Stream) valid signal. For more information see section 4.8. |
| *sCmdTxAxisTready* | SPI IAP | O | N/A | IAP command TX interface (Slave AXI Stream) ready signal. For more information see section 4.8. |
| *sCmdRxAxisTdata[31:0]* | SPI IAP | O | N/A | IAP command RX interface (Master AXI Stream) data port. For more information see section 4.8. |
| *sCmdRxAxisTvalid* | SPI IAP | O | N/A | IAP command RX interface (Master AXI Stream) valid signal. For more information see section 4.8. |
| *sCmdRxAxisTready* | SPI IAP | I | N/A | IAP command RX interface (Master AXI Stream) ready signal. For more information see section 4.8. |
| *CG\_InputClk\_p* | Zmod | O | N/A | Clock Generator positive differential primary clock input. For more details see [1]. |
| *CG\_InputClk\_n* | Zmod | O | N/A | Clock Generator negative differential primary clock input. For more details see [1]. |
| *aCG\_PLL\_Lock* | Zmod | I | N/A | Clock Generator PLL lock signal sent via the GPIO1 or GPIO4 port. |
| *aREFSEL* | Zmod | O | N/A | Clock Generator reference selection signal ('0' selects SECREF(XTAL) and '1' selects PRIREF(FPGA)). |
| *aHW\_SW\_CTRL* | Zmod | O | N/A | Clock Generator EEPROM Page selection signal. |
| *sPDNout\_n* | Zmod | O | L | Clock Generator power down signal, passthrough output. |
| *ZmodDcoClkOut* | - | O | N/A | De-skewed version of DcoClkIn through MMCM and BUFG primitives. |
| *sZmodDcoPLL\_Lock* | - | O | L | Lock signal of the MMCM used for de-skewing purposes. Signals that ZmodDcoClkOut is stable. |
| *diZmodSDR\_Data[kADC\_Width-1 : 0]* | Zmod | I | N/A | *kADC\_Width* bit wide DDR parallel data bus exported by ADC containing Channel1 and Channel 2 interleaved samples [4]. |
| *sZmodADC\_SDIO* | Zmod | IO | N/A | SPI SDIO signal [4]. |
| *sZmodADC\_CS* | Zmod | O | N/A | SPI CS signal [4]. |
| *sZmodADC\_Sclk* | Zmod | O | N/A | SPI output clock [4]. |
| *s\_scl\_i* | CDCE IIC | I | Z | I2C Serial Clock Input from 3-state buffer. |
| *s\_scl\_o* | CDCE IIC | O | L | I2C Serial Clock Output to 3-state buffer. |
| *s\_scl\_t* | CDCE IIC | T | N/A | I2C Serial Clock Output Enable to 3-state buffer. |
| *s\_sda\_i* | CDCE IIC | I | Z | I2C Serial Data Input from 3-state buffer. |
| *s\_sda\_o* | CDCE IIC | O | L | I2C Serial Data Output to 3-state buffer. |
| *s\_sda\_t* | CDCE IIC | T | N/A | I2C Serial Data Output Enable to 3-state buffer. |

# IP Core customization

The customization parameters allow:

Selecting the Zmod SDR targeted through the *kZmodID* parameter. The *kZmodID* parameter also configures the *kADC\_Width* generic. Table 13 details how kZmodID should be configured.

Table : kZmodID configuration

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Zmod | ADC | kZmodID | kADC\_Width | kSamplingPeriod (max) |
| Zmod SDR 1450 - 122 | AD9648 | 6 | 14 | 8000 (125 MSPS) |

Enabling/disabling the external SPI IAP interface through the *kExtCmdInterfaceEn*parameter. The SPI IAP interface needs to be enabled (*kExtCmdInterfaceEn*= true) to modify the ADC’s configuration registers after initialization.

Selecting the ADC Sampling frequency from a set of supported frequencies through the *kCDCEFreqSel* parameter.

Table : ADC Sampling Clock Frequency Selection

|  |  |  |
| --- | --- | --- |
| Sampling Frequency | kCDCEFreqSel | kSamplingPeriod |
| 122.88 MHz | 0 | 8138 ps |
| 50 MHz | 1 | 20000 ps |
| 80 MHz | 2 | 12500 ps |
| 100 MHz | 3 | 10000 ps |
| 110 MHz | 4 | 9090 ps |
| 120 MHz | 5 | 8333 ps |
| 125 MHz | 6 | 8000 ps |

Changing CDCE6214-Q1 I2C address (*kCGI2C\_Addr*) and thus potentially changing the Clock Generator operating mode, the primary mode is called Fall-Back Mode [1] where the I2C interface is always enabled, the other modes involve its configuration being read from an internal factory programmed 2 Page EEPROM which can have frequency configurations unsupported by this IP.

Changing CDCE6214-Q1 clock reference selection between SECREF (XTAL) and PRIREF (generated inside the FPGA).

Selecting CDCE6124-Q1 internal EEPROM Page (Page 0 has a factory configuration that disables the I2C serial interface).

# References

The following documents provide additional information on the subjects discussed:

1. Texas Instruments, CDCE6214-Q1 Datasheet, SNAS786B, Rev B.
2. Xilinx Inc., *UG472: 7 Series FPGAs Clocking Resources*, v1.6, October 2, 2012.
3. Xilinx Inc., *UG471: 7 Series FPGAs SelectIO Resources*, v1.4, May 13, 2014.
4. Analog Devices, AD9648 Datasheet, Rev C.