| Paho MQTT C Client Library

Loading...
Searching...
No Matches
Data Structures | Macros | Typedefs | Enumerations | Functions
MQTTProperties.h File Reference
`#include "MQTTExportDeclarations.h"`
`#include <stdint.h>`

Go to the source code of this file.

## Data Structures
struct | MQTTLenString
struct | MQTTProperty
struct | MQTTProperties

## Macros
#define | MQTT_INVALID_PROPERTY_ID -2
#define | MQTTProperties_initializer {0, 0, 0, NULL}

## Typedefs
typedef struct MQTTProperties | MQTTProperties

## Enumerations
enum | MQTTPropertyCodes { MQTTPROPERTY_CODE_PAYLOAD_FORMAT_INDICATOR = 1 , MQTTPROPERTY_CODE_MESSAGE_EXPIRY_INTERVAL = 2 , MQTTPROPERTY_CODE_CONTENT_TYPE = 3 , MQTTPROPERTY_CODE_RESPONSE_TOPIC = 8 , MQTTPROPERTY_CODE_CORRELATION_DATA = 9 , MQTTPROPERTY_CODE_SUBSCRIPTION_IDENTIFIER = 11 , MQTTPROPERTY_CODE_SESSION_EXPIRY_INTERVAL = 17 , MQTTPROPERTY_CODE_ASSIGNED_CLIENT_IDENTIFIER = 18 , MQTTPROPERTY_CODE_ASSIGNED_CLIENT_IDENTIFER = 18 , MQTTPROPERTY_CODE_SERVER_KEEP_ALIVE = 19 , MQTTPROPERTY_CODE_AUTHENTICATION_METHOD = 21 , MQTTPROPERTY_CODE_AUTHENTICATION_DATA = 22 , MQTTPROPERTY_CODE_REQUEST_PROBLEM_INFORMATION = 23 , MQTTPROPERTY_CODE_WILL_DELAY_INTERVAL = 24 , MQTTPROPERTY_CODE_REQUEST_RESPONSE_INFORMATION = 25 , MQTTPROPERTY_CODE_RESPONSE_INFORMATION = 26 , MQTTPROPERTY_CODE_SERVER_REFERENCE = 28 , MQTTPROPERTY_CODE_REASON_STRING = 31 , MQTTPROPERTY_CODE_RECEIVE_MAXIMUM = 33 , MQTTPROPERTY_CODE_TOPIC_ALIAS_MAXIMUM = 34 , MQTTPROPERTY_CODE_TOPIC_ALIAS = 35 , MQTTPROPERTY_CODE_MAXIMUM_QOS = 36 , MQTTPROPERTY_CODE_RETAIN_AVAILABLE = 37 , MQTTPROPERTY_CODE_USER_PROPERTY = 38 , MQTTPROPERTY_CODE_MAXIMUM_PACKET_SIZE = 39 , MQTTPROPERTY_CODE_WILDCARD_SUBSCRIPTION_AVAILABLE = 40 , MQTTPROPERTY_CODE_SUBSCRIPTION_IDENTIFIERS_AVAILABLE = 41 , MQTTPROPERTY_CODE_SHARED_SUBSCRIPTION_AVAILABLE = 42 }
enum | MQTTPropertyTypes { MQTTPROPERTY_TYPE_BYTE , MQTTPROPERTY_TYPE_TWO_BYTE_INTEGER , MQTTPROPERTY_TYPE_FOUR_BYTE_INTEGER , MQTTPROPERTY_TYPE_VARIABLE_BYTE_INTEGER , MQTTPROPERTY_TYPE_BINARY_DATA , MQTTPROPERTY_TYPE_UTF_8_ENCODED_STRING , MQTTPROPERTY_TYPE_UTF_8_STRING_PAIR }

## Functions
const char * | MQTTPropertyName (enum MQTTPropertyCodes value)
int | MQTTProperty_getType (enum MQTTPropertyCodes value)
int | MQTTProperties_len (const MQTTProperties *props)
int | MQTTProperties_add (MQTTProperties *props, const MQTTProperty *prop)
int | MQTTProperties_write (char **pptr, const MQTTProperties *properties)
int | MQTTProperties_read (MQTTProperties *properties, char **pptr, char *enddata)
void | MQTTProperties_free (MQTTProperties *properties)
MQTTProperties | MQTTProperties_copy (const MQTTProperties *props)
int | MQTTProperties_hasProperty (const MQTTProperties *props, enum MQTTPropertyCodes propid)
int | MQTTProperties_propertyCount (const MQTTProperties *props, enum MQTTPropertyCodes propid)
int64_t | MQTTProperties_getNumericValue (const MQTTProperties *props, enum MQTTPropertyCodes propid)
int64_t | MQTTProperties_getNumericValueAt (const MQTTProperties *props, enum MQTTPropertyCodes propid, int index)
MQTTProperty * | MQTTProperties_getProperty (const MQTTProperties *props, enum MQTTPropertyCodes propid)
MQTTProperty * | MQTTProperties_getPropertyAt (const MQTTProperties *props, enum MQTTPropertyCodes propid, int index)

## Macro Definition Documentation

## ◆ MQTT_INVALID_PROPERTY_ID

#define MQTT_INVALID_PROPERTY_ID -2

## ◆ MQTTProperties_initializer

#define MQTTProperties_initializer {0, 0, 0, NULL}

## Typedef Documentation

## ◆ MQTTProperties

typedef struct MQTTProperties MQTTProperties

MQTT version 5 property list

## Enumeration Type Documentation

## ◆ MQTTPropertyCodes

enum MQTTPropertyCodes

The one byte MQTT V5 property indicator

Enumerator
MQTTPROPERTY_CODE_PAYLOAD_FORMAT_INDICATOR | The value is 1
MQTTPROPERTY_CODE_MESSAGE_EXPIRY_INTERVAL | The value is 2
MQTTPROPERTY_CODE_CONTENT_TYPE | The value is 3
MQTTPROPERTY_CODE_RESPONSE_TOPIC | The value is 8
MQTTPROPERTY_CODE_CORRELATION_DATA | The value is 9
MQTTPROPERTY_CODE_SUBSCRIPTION_IDENTIFIER | The value is 11
MQTTPROPERTY_CODE_SESSION_EXPIRY_INTERVAL | The value is 17
MQTTPROPERTY_CODE_ASSIGNED_CLIENT_IDENTIFIER | The value is 18
MQTTPROPERTY_CODE_ASSIGNED_CLIENT_IDENTIFER | The value is 18 (obsolete, misspelled)
MQTTPROPERTY_CODE_SERVER_KEEP_ALIVE | The value is 19
MQTTPROPERTY_CODE_AUTHENTICATION_METHOD | The value is 21
MQTTPROPERTY_CODE_AUTHENTICATION_DATA | The value is 22
MQTTPROPERTY_CODE_REQUEST_PROBLEM_INFORMATION | The value is 23
MQTTPROPERTY_CODE_WILL_DELAY_INTERVAL | The value is 24
MQTTPROPERTY_CODE_REQUEST_RESPONSE_INFORMATION | The value is 25
MQTTPROPERTY_CODE_RESPONSE_INFORMATION | The value is 26
MQTTPROPERTY_CODE_SERVER_REFERENCE | The value is 28
MQTTPROPERTY_CODE_REASON_STRING | The value is 31
MQTTPROPERTY_CODE_RECEIVE_MAXIMUM | The value is 33
MQTTPROPERTY_CODE_TOPIC_ALIAS_MAXIMUM | The value is 34
MQTTPROPERTY_CODE_TOPIC_ALIAS | The value is 35
MQTTPROPERTY_CODE_MAXIMUM_QOS | The value is 36
MQTTPROPERTY_CODE_RETAIN_AVAILABLE | The value is 37
MQTTPROPERTY_CODE_USER_PROPERTY | The value is 38
MQTTPROPERTY_CODE_MAXIMUM_PACKET_SIZE | The value is 39
MQTTPROPERTY_CODE_WILDCARD_SUBSCRIPTION_AVAILABLE | The value is 40
MQTTPROPERTY_CODE_SUBSCRIPTION_IDENTIFIERS_AVAILABLE | The value is 41
MQTTPROPERTY_CODE_SHARED_SUBSCRIPTION_AVAILABLE | The value is 241

## ◆ MQTTPropertyTypes

enum MQTTPropertyTypes

The one byte MQTT V5 property type

Enumerator
MQTTPROPERTY_TYPE_BYTE |
MQTTPROPERTY_TYPE_TWO_BYTE_INTEGER |
MQTTPROPERTY_TYPE_FOUR_BYTE_INTEGER |
MQTTPROPERTY_TYPE_VARIABLE_BYTE_INTEGER |
MQTTPROPERTY_TYPE_BINARY_DATA |
MQTTPROPERTY_TYPE_UTF_8_ENCODED_STRING |
MQTTPROPERTY_TYPE_UTF_8_STRING_PAIR |

## Function Documentation

## ◆ MQTTPropertyName()

const char * MQTTPropertyName | ( | enum MQTTPropertyCodes | value | ) |
| extern

Returns a printable string description of an MQTT V5 property code.

Parameters

  value | an MQTT V5 property code.

Returns
  the printable string description of the input property code. NULL if the code was not found.

## ◆ MQTTProperty_getType()

int MQTTProperty_getType | ( | enum MQTTPropertyCodes | value | ) |
| extern

Returns the MQTT V5 type code of an MQTT V5 property.

Parameters

  value | an MQTT V5 property code.

Returns
  the MQTT V5 type code of the input property. -1 if the code was not found.

## ◆ MQTTProperties_len()

int MQTTProperties_len | ( | const MQTTProperties * | props | ) |

Returns the length of the properties structure when serialized ready for network transmission.

Parameters

  props | an MQTT V5 property structure.

Returns
  the length in bytes of the properties when serialized.

## ◆ MQTTProperties_add()

int MQTTProperties_add | ( | MQTTProperties * | props,
|  | const MQTTProperty * | prop )
| extern

Add a property pointer to the property array. Memory is allocated in this function, so MQTTClient_create or MQTTAsync_create must be called first to initialize the internal heap tracking. Alternatively MQTTAsync_global_init() can be called first or build with the HIGH_PERFORMANCE option which disables the heap tracking.

Parameters

  props | The property list to add the property to.
  prop | The property to add to the list.

Returns
  0 on success, -1 on failure.

## ◆ MQTTProperties_write()

int MQTTProperties_write | ( | char ** | pptr,
|  | const MQTTProperties * | properties )

Serialize the given property list to a character buffer, e.g. for writing to the network.

Parameters

  pptr | pointer to the buffer - move the pointer as we add data
  properties | pointer to the property list, can be NULL

Returns
  whether the write succeeded or not: number of bytes written, or < 0 on failure.

## ◆ MQTTProperties_read()

int MQTTProperties_read | ( | MQTTProperties * | properties,
|  | char ** | pptr,
|  | char * | enddata )

Reads a property list from a character buffer into an array.

Parameters

  properties | pointer to the property list to be filled. Should be initalized but empty.
  pptr | pointer to the character buffer.
  enddata | pointer to the end of the character buffer so we don't read beyond.

Returns
  1 if the properties were read successfully.

## ◆ MQTTProperties_free()

void MQTTProperties_free | ( | MQTTProperties * | properties | ) |
| extern

Free all memory allocated to the property list, including any to individual properties.

Parameters

  properties | pointer to the property list.

## ◆ MQTTProperties_copy()

MQTTProperties MQTTProperties_copy | ( | const MQTTProperties * | props | ) |
| extern

Copy the contents of a property list, allocating additional memory if needed.

Parameters

  props | pointer to the property list.

Returns
  the duplicated property list.

## ◆ MQTTProperties_hasProperty()

int MQTTProperties_hasProperty | ( | const MQTTProperties * | props,
|  | enum MQTTPropertyCodes | propid )
| extern

Checks if property list contains a specific property.

Parameters

  props | pointer to the property list.
  propid | the property id to check for.

Returns
  1 if found, 0 if not.

## ◆ MQTTProperties_propertyCount()

int MQTTProperties_propertyCount | ( | const MQTTProperties * | props,
|  | enum MQTTPropertyCodes | propid )
| extern

Returns the number of instances of a property id. Most properties can exist only once. User properties and subscription ids can exist more than once.

Parameters

  props | pointer to the property list.
  propid | the property id to check for.

Returns
  the number of times found. Can be 0.

## ◆ MQTTProperties_getNumericValue()

int64_t MQTTProperties_getNumericValue | ( | const MQTTProperties * | props,
|  | enum MQTTPropertyCodes | propid )
| extern

Returns the integer value of a specific property. The property given must be a numeric type.

Parameters

  props | pointer to the property list.
  propid | the property id to check for.

Returns
  the integer value of the property. -9999999 on failure.

## ◆ MQTTProperties_getNumericValueAt()

int64_t MQTTProperties_getNumericValueAt | ( | const MQTTProperties * | props,
|  | enum MQTTPropertyCodes | propid,
|  | int | index )
| extern

Returns the integer value of a specific property when it's not the only instance. The property given must be a numeric type.

Parameters

  props | pointer to the property list.
  propid | the property id to check for.
  index | the instance number, starting at 0.

Returns
  the integer value of the property. -9999999 on failure.

## ◆ MQTTProperties_getProperty()

MQTTProperty * MQTTProperties_getProperty | ( | const MQTTProperties * | props,
|  | enum MQTTPropertyCodes | propid )
| extern

Returns a pointer to the property structure for a specific property.

Parameters

  props | pointer to the property list.
  propid | the property id to check for.

Returns
  the pointer to the property structure if found. NULL if not found.

## ◆ MQTTProperties_getPropertyAt()

MQTTProperty * MQTTProperties_getPropertyAt | ( | const MQTTProperties * | props,
|  | enum MQTTPropertyCodes | propid,
|  | int | index )
| extern

Returns a pointer to the property structure for a specific property when it's not the only instance.

Parameters

  props | pointer to the property list.
  propid | the property id to check for.
  index | the instance number, starting at 0.

Returns
  the pointer to the property structure if found. NULL if not found.