Device Status Codes:
====================

 0 = "Initializing"
 1 = "Autotuning"
 2 = "Selftest"
 3 = "Running"
 4 = "Paused"
 5 = "Exhausted"
 6 = "Cracked"
 7 = "Aborted"
 8 = "Quit"
 9 = "Bypass"
10 = "Aborted (Checkpoint)"
11 = "Aborted (Runtime)"
12 = "Running (Checkpoint Quit requested)"
13 = "Error"
14 = "Aborted (Finish)"
15 = "Running (Quit after attack requested)"
16 = "Autodetect"
