drillTime: 240
liquidBoostIntensity: 1.7327
hardnessDrillMultiplier: 30
consumes: {
  remove: [
    liquid
  ]
  liquid: {
    liquid: cryofluid
    amount: 0.4
    optional: true
    booster: true
  }
  liquids: [
    oil/0.15
  ]
}
drillMultipliers: {
  copper: 1.0312
  lead: 1.0312
  coal: 1.0412
  titanium: 1.0315
  beryllium: 1.0315
  tungsten: 0.8125
}
requirements: [
  graphite/250
  silicon/100
  thorium/100
  plastanium/50
  phase-fabric/50
]