type: ArmoredConduit
category: liquid
requirements: [
  01a-05-item-aluminium/1
  01a-10-item-bethine/1
]
health: 500
armor: 5
junctionReplacement: 06f-02-seaduct-junction
rotBridgeReplacement: 06f-04-m-clevoritebridge
solid: false
research: 06f-01-b-aqua-conduit
researchCostMultiplier: 1
leaks: false
underBullets: true
liquidCapacity: 50
liquidPressure: 1.5